{"text_format":"3","workbook":"xlsx","n_sheets":6,"sheets":["设备","累积量","模拟量","数字量","数字量控制","保护定值"],"not_rendered":{"defined_names":3},"read":"whole","date_system":"1900"}

{"sheet":"设备","index":0,"n_rows":147,"n_cols":4,"rows_kept":147}
["TAG_NAME","DESCRIPTION","DEV_ID","DEV_MODEL"]
["设备名称","设备描述","设备ID","设备模板"]
["Station","220kV站",0,"通用前置"]
["BusIM","220kVI母测控",1,"通用前置"]
["BusIIM","220kVII母测控",2,"通用前置"]
["TieM","220kV母联测控",3,"通用前置"]
["TF1HVM","220kV#1主变高压侧测控",4,"通用前置"]
["TF1LVM-C308","存308#1主变低压侧测控",5,"通用前置"]
["TF1M","220kV#1主变本体侧测控",6,"通用前置"]
["TF2HVM","220kV#2主变高压侧测控",7,"通用前置"]
["TF2LV-C408","存408#2主变低压侧测控",8,"通用前置"]
["TF2M","220kV#2主变本体侧测控",9,"通用前置"]
["TF3HVM","220kV#3主变高压侧测控",10,"通用前置"]
["TF3LVM-C508","存508#3主变低压侧测控",11,"通用前置"]
["TF3M","220kV#3主变本体侧测控",12,"通用前置"]
["TF4HVM","220kV#4主变高压侧测控",13,"通用前置"]
["TF4LVM-C608","存608#4主变低压侧测控",14,"通用前置"]
["TF4M","220kV#4主变本体侧测控",15,"通用前置"]
["LZCM","220kV庄存线测控",16,"通用前置"]
["LCCM","220kV存储线测控",17,"通用前置"]
["LBYM","220kV备用线测控",18,"通用前置"]
["PT03bM","互03b母线测控",19,"通用前置"]
["PT04bM","互04b母线测控",20,"通用前置"]
["PT05bM","互05b母线测控",21,"通用前置"]
["PT06bM","互06b母线测控",22,"通用前置"]
["LC301","存301馈线",23,"通用前置"]
["LC302","存302馈线",24,"通用前置"]
["LC303","存303馈线",25,"通用前置"]
["LC304","存304馈线",26,"通用前置"]
["LC305","存305馈线",27,"通用前置"]
["LC306","存306馈线",28,"通用前置"]
["LC307","存307馈线",29,"通用前置"]
["BusC314","存314分段",30,"通用前置"]
["LC401","存401馈线",31,"通用前置"]
["LC402","存402馈线",32,"通用前置"]
["LC403","存403馈线",33,"通用前置"]
["LC404","存404馈线",34,"通用前置"]
["LC405","存405馈线",35,"通用前置"]
["LC406","存406馈线",36,"通用前置"]
["LC407","存407馈线",37,"通用前置"]
["BusC415","存415分段",38,"通用前置"]
["LC501","存501馈线",39,"通用前置"]
["LC502","存502馈线",40,"通用前置"]
["LC503","存503馈线",41,"通用前置"]
["LC504","存504馈线",42,"通用前置"]
["LC505","存505馈线",43,"通用前置"]
["LC506","存506馈线",44,"通用前置"]
["LC507","存507馈线",45,"通用前置"]
["BusC516","存516分段",46,"通用前置"]
["LC601","存601馈线",47,"通用前置"]
["LC602","存602馈线",48,"通用前置"]
["LC603","存603馈线",49,"通用前置"]
["LC604","存604馈线",50,"通用前置"]
["LC605","存605馈线",51,"通用前置"]
["LC606","存606馈线",52,"通用前置"]
["LC607","存607馈线",53,"通用前置"]
["BusC613","存613分段",54,"通用前置"]
["CAP1C309","#1电容存309",55,"通用前置"]
["GTF1C310","#1接地变存310",56,"通用前置"]
["STF1C311","#1站用变存311",57,"通用前置"]
["CAP3C419","#3电容存419",58,"通用前置"]
["GTF2C410","#2接地变存410",59,"通用前置"]
["CAP3C509","#3电容存509",60,"通用前置"]
["GTF3C510","#3接地变存510",61,"通用前置"]
["CAP4C609","#4电容存609",62,"通用前置"]
["GTF4C610","#4接地变存610",63,"通用前置"]
["STF4C611","#4所用变存611",64,"通用前置"]
["BZTC314","存314分段备自投",65,"通用前置"]
["BZTC415","存415分段备自投",66,"通用前置"]
["BZTC516","存516分段备自投",67,"通用前置"]
["BZTC613","存613分段备自投",68,"通用前置"]
["ComMea1","公用测控1",69,"通用前置"]
["ComMea2","公用测控2",70,"通用前置"]
["BusRey1","220kV母线第一套保护CSC-150A",71,"通用前置"]
["BusRey2","220kV母线第二套保护PCS-915A",72,"通用前置"]
["TieRey1","220kV母联第一套保护CSC-122A",73,"通用前置"]
["TieRey2","220kV母联第二套保护PCS-923A",74,"通用前置"]
["TF1Rey1","220kV#1主变第一套保护CSC-326T2",75,"通用前置"]
["TF1Rey2","220kV#1主变第二套保护PCS-978T2",76,"通用前置"]
["TF1Rey3","220kV#1主变非电量保护CSC336C2B",77,"通用前置"]
["TF2Rey1","220kV#2主变第一套保护CSC-326T2",78,"通用前置"]
["TF2Rey2","220kV#2主变第二套保护PCS-978T2",79,"通用前置"]
["TF2Rey3","220kV#2主变非电量保护CSC336C2B",80,"通用前置"]
["TF3Rey1","220kV#3主变第一套保护CSC-326T2",81,"通用前置"]
["TF3Rey2","220kV#3主变第二套保护PCS-978T2",82,"通用前置"]
["TF3Rey3","220kV#3主变非电量保护CSC336C2B",83,"通用前置"]
["TF4Rey1","220kV#4主变第一套保护CSC-326T2",84,"通用前置"]
["TF4Rey2","220kV#4主变第二套保护PCS-978T2",85,"通用前置"]
["TF4Rey3","220kV#4主变非电量保护CSC336C2B",86,"通用前置"]
["LZCRey1","220kV庄存线第一套保护WXH-803A",87,"通用前置"]
["LZCRey2","220kV庄存线第二套保护PCS-931SA",88,"通用前置"]
["LCCRey1","220kV存储线第一套保护CSC-103A",89,"通用前置"]
["LCCRey2","220kV存储线第二套保护PCS-931SA",90,"通用前置"]
["SC901","存901站用",91,"通用前置"]
["SC902","存902站用",92,"通用前置"]
["ZC222YB","存222仪表",101,"通用前置"]
["CC229YB","存229仪表",102,"通用前置"]
["TF12211LYB","存2211主仪表",103,"通用前置"]
["TF12212SYB","存2212副仪表",104,"通用前置"]
["TF22241LYB","存2241主仪表",105,"通用前置"]
["TF22242SYB","存2242副仪表",106,"通用前置"]
["TF32261LYB","存2261主仪表",107,"通用前置"]
["TF32262SYB","存2262副仪表",108,"通用前置"]
["TF42301LYB","存2301主仪表",109,"通用前置"]
["TF42302SYB","存2302副仪表",110,"通用前置"]
["LC308YB","存308仪表",111,"通用前置"]
["LC408YB","存408仪表",112,"通用前置"]
["LC508YB","存508仪表",113,"通用前置"]
["LC608YB","存608仪表",114,"通用前置"]
["LC301YB","存301仪表",115,"通用前置"]
["LC302YB","存302仪表",116,"通用前置"]
["LC303YB","存303仪表",117,"通用前置"]
["LC304YB","存304仪表",118,"通用前置"]
["LC305YB","存305仪表",119,"通用前置"]
["LC306YB","存306仪表",120,"通用前置"]
["LC307YB","存307仪表",121,"通用前置"]
["CAP1C309YB","存309仪表",122,"通用前置"]
["GTF1C310YB","存310仪表",123,"通用前置"]
["STF1C311YB","存311仪表",124,"通用前置"]
["LC401YB","存401仪表",125,"通用前置"]
["LC402YB","存402仪表",126,"通用前置"]
["LC403YB","存403仪表",127,"通用前置"]
["LC404YB","存404仪表",128,"通用前置"]
["LC405YB","存405仪表",129,"通用前置"]
["LC406YB","存406仪表",130,"通用前置"]
["LC407YB","存407仪表",131,"通用前置"]
["CAP3C419YB","存419仪表",132,"通用前置"]
["GTF3C410YB","存410仪表",133,"通用前置"]
["LC501YB","存501仪表",134,"通用前置"]
["LC502YB","存502仪表",135,"通用前置"]
["LC503YB","存503仪表",136,"通用前置"]
["LC504YB","存504仪表",137,"通用前置"]
["LC505YB","存505仪表",138,"通用前置"]
["LC506YB","存506仪表",139,"通用前置"]
["LC507YB","存507仪表",140,"通用前置"]
["CAP3C509YB","存509仪表",141,"通用前置"]
["GTF3C510YB","存510仪表",142,"通用前置"]
["LC601YB","存601仪表",143,"通用前置"]
["LC602YB","存602仪表",144,"通用前置"]
["LC603YB","存603仪表",145,"通用前置"]
["LC604YB","存604仪表",146,"通用前置"]
["LC605YB","存605仪表",147,"通用前置"]
["LC606YB","存606仪表",148,"通用前置"]
["LC607YB","存607仪表",149,"通用前置"]
["CAP4C609YB","存609仪表",150,"通用前置"]
["GTF4C610YB","存610仪表",151,"通用前置"]
["STF4C611YB","存611仪表",152,"通用前置"]

{"sheet":"累积量","index":1,"n_rows":210,"n_cols":6,"rows_kept":210}
["DEV_ID","TAG_NAME","DESCRIPTION","REMOTE_NO","RATIO","REVISE"]
["设备ID","标签名","点描述","远动号","变比系数","修正值"]
[101,"EPd","正向有功电度",0,1]
[101,"EQd","正向无功电度",1,1]
[101,"EQr","反向无功电度",2,1]
[101,"EPr","反向有功电度",3,1]
[102,"EPd","正向有功电度",4,1]
[102,"EQd","正向无功电度",5,1]
[102,"EQr","反向无功电度",6,1]
[102,"EPr","反向有功电度",7,1]
[103,"EPd","正向有功电度",8,1]
[103,"EQd","正向无功电度",9,1]
[103,"EQr","反向无功电度",10,1]
[103,"EPr","反向有功电度",11,1]
[104,"EPd","正向有功电度",12,1]
[104,"EQd","正向无功电度",13,1]
[104,"EQr","反向无功电度",14,1]
[104,"EPr","反向有功电度",15,1]
[105,"EPd","正向有功电度",16,1]
[105,"EQd","正向无功电度",17,1]
[105,"EQr","反向无功电度",18,1]
[105,"EPr","反向有功电度",19,1]
[106,"EPd","正向有功电度",20,1]
[106,"EQd","正向无功电度",21,1]
[106,"EQr","反向无功电度",22,1]
[106,"EPr","反向有功电度",23,1]
[107,"EPd","正向有功电度",24,1]
[107,"EQd","正向无功电度",25,1]
[107,"EQr","反向无功电度",26,1]
[107,"EPr","反向有功电度",27,1]
[108,"EPd","正向有功电度",28,1]
[108,"EQd","正向无功电度",29,1]
[108,"EQr","反向无功电度",30,1]
[108,"EPr","反向有功电度",31,1]
[109,"EPd","正向有功电度",32,1]
[109,"EQd","正向无功电度",33,1]
[109,"EQr","反向无功电度",34,1]
[109,"EPr","反向有功电度",35,1]
[110,"EPd","正向有功电度",36,1]
[110,"EQd","正向无功电度",37,1]
[110,"EQr","反向无功电度",38,1]
[110,"EPr","反向有功电度",39,1]
[111,"EPd","正向有功电度",40,1]
[111,"EQd","正向无功电度",41,1]
[111,"EQr","反向无功电度",42,1]
[111,"EPr","反向有功电度",43,1]
[112,"EPd","正向有功电度",44,1]
[112,"EQd","正向无功电度",45,1]
[112,"EQr","反向无功电度",46,1]
[112,"EPr","反向有功电度",47,1]
[113,"EPd","正向有功电度",48,1]
[113,"EQd","正向无功电度",49,1]
[113,"EQr","反向无功电度",50,1]
[113,"EPr","反向有功电度",51,1]
[114,"EPd","正向有功电度",52,1]
[114,"EQd","正向无功电度",53,1]
[114,"EQr","反向无功电度",54,1]
[114,"EPr","反向有功电度",55,1]
[115,"EPd","正向有功电度",56,1]
[115,"EQd","正向无功电度",57,1]
[115,"EQr","反向无功电度",58,1]
[115,"EPr","反向有功电度",59,1]
[116,"EPd","正向有功电度",60,1]
[116,"EQd","正向无功电度",61,1]
[116,"EQr","反向无功电度",62,1]
[116,"EPr","反向有功电度",63,1]
[117,"EPd","正向有功电度",64,1]
[117,"EQd","正向无功电度",65,1]
[117,"EQr","反向无功电度",66,1]
[117,"EPr","反向有功电度",67,1]
[118,"EPd","正向有功电度",68,1]
[118,"EQd","正向无功电度",69,1]
[118,"EQr","反向无功电度",70,1]
[118,"EPr","反向有功电度",71,1]
[119,"EPd","正向有功电度",72,1]
[119,"EQd","正向无功电度",73,1]
[119,"EQr","反向无功电度",74,1]
[119,"EPr","反向有功电度",75,1]
[120,"EPd","正向有功电度",76,1]
[120,"EQd","正向无功电度",77,1]
[120,"EQr","反向无功电度",78,1]
[120,"EPr","反向有功电度",79,1]
[121,"EPd","正向有功电度",80,1]
[121,"EQd","正向无功电度",81,1]
[121,"EQr","反向无功电度",82,1]
[121,"EPr","反向有功电度",83,1]
[122,"EPd","正向有功电度",84,1]
[122,"EQd","正向无功电度",85,1]
[122,"EQr","反向无功电度",86,1]
[122,"EPr","反向有功电度",87,1]
[123,"EPd","正向有功电度",88,1]
[123,"EQd","正向无功电度",89,1]
[123,"EQr","反向无功电度",90,1]
[123,"EPr","反向有功电度",91,1]
[124,"EPd","正向有功电度",92,1]
[124,"EQd","正向无功电度",93,1]
[124,"EQr","反向无功电度",94,1]
[124,"EPr","反向有功电度",95,1]
[125,"EPd","正向有功电度",96,1]
[125,"EQd","正向无功电度",97,1]
[125,"EQr","反向无功电度",98,1]
[125,"EPr","反向有功电度",99,1]
[126,"EPd","正向有功电度",100,1]
[126,"EQd","正向无功电度",101,1]
[126,"EQr","反向无功电度",102,1]
[126,"EPr","反向有功电度",103,1]
[127,"EPd","正向有功电度",104,1]
[127,"EQd","正向无功电度",105,1]
[127,"EQr","反向无功电度",106,1]
[127,"EPr","反向有功电度",107,1]
[128,"EPd","正向有功电度",108,1]
[128,"EQd","正向无功电度",109,1]
[128,"EQr","反向无功电度",110,1]
[128,"EPr","反向有功电度",111,1]
[129,"EPd","正向有功电度",112,1]
[129,"EQd","正向无功电度",113,1]
[129,"EQr","反向无功电度",114,1]
[129,"EPr","反向有功电度",115,1]
[130,"EPd","正向有功电度",116,1]
[130,"EQd","正向无功电度",117,1]
[130,"EQr","反向无功电度",118,1]
[130,"EPr","反向有功电度",119,1]
[131,"EPd","正向有功电度",120,1]
[131,"EQd","正向无功电度",121,1]
[131,"EQr","反向无功电度",122,1]
[131,"EPr","反向有功电度",123,1]
[132,"EPd","正向有功电度",124,1]
[132,"EQd","正向无功电度",125,1]
[132,"EQr","反向无功电度",126,1]
[132,"EPr","反向有功电度",127,1]
[133,"EPd","正向有功电度",128,1]
[133,"EQd","正向无功电度",129,1]
[133,"EQr","反向无功电度",130,1]
[133,"EPr","反向有功电度",131,1]
[134,"EPd","正向有功电度",132,1]
[134,"EQd","正向无功电度",133,1]
[134,"EQr","反向无功电度",134,1]
[134,"EPr","反向有功电度",135,1]
[135,"EPd","正向有功电度",136,1]
[135,"EQd","正向无功电度",137,1]
[135,"EQr","反向无功电度",138,1]
[135,"EPr","反向有功电度",139,1]
[136,"EPd","正向有功电度",140,1]
[136,"EQd","正向无功电度",141,1]
[136,"EQr","反向无功电度",142,1]
[136,"EPr","反向有功电度",143,1]
[137,"EPd","正向有功电度",144,1]
[137,"EQd","正向无功电度",145,1]
[137,"EQr","反向无功电度",146,1]
[137,"EPr","反向有功电度",147,1]
[138,"EPd","正向有功电度",148,1]
[138,"EQd","正向无功电度",149,1]
[138,"EQr","反向无功电度",150,1]
[138,"EPr","反向有功电度",151,1]
[139,"EPd","正向有功电度",152,1]
[139,"EQd","正向无功电度",153,1]
[139,"EQr","反向无功电度",154,1]
[139,"EPr","反向有功电度",155,1]
[140,"EPd","正向有功电度",156,1]
[140,"EQd","正向无功电度",157,1]
[140,"EQr","反向无功电度",158,1]
[140,"EPr","反向有功电度",159,1]
[141,"EPd","正向有功电度",160,1]
[141,"EQd","正向无功电度",161,1]
[141,"EQr","反向无功电度",162,1]
[141,"EPr","反向有功电度",163,1]
[142,"EPd","正向有功电度",164,1]
[142,"EQd","正向无功电度",165,1]
[142,"EQr","反向无功电度",166,1]
[142,"EPr","反向有功电度",167,1]
[143,"EPd","正向有功电度",168,1]
[143,"EQd","正向无功电度",169,1]
[143,"EQr","反向无功电度",170,1]
[143,"EPr","反向有功电度",171,1]
[144,"EPd","正向有功电度",172,1]
[144,"EQd","正向无功电度",173,1]
[144,"EQr","反向无功电度",174,1]
[144,"EPr","反向有功电度",175,1]
[145,"EPd","正向有功电度",176,1]
[145,"EQd","正向无功电度",177,1]
[145,"EQr","反向无功电度",178,1]
[145,"EPr","反向有功电度",179,1]
[146,"EPd","正向有功电度",180,1]
[146,"EQd","正向无功电度",181,1]
[146,"EQr","反向无功电度",182,1]
[146,"EPr","反向有功电度",183,1]
[147,"EPd","正向有功电度",184,1]
[147,"EQd","正向无功电度",185,1]
[147,"EQr","反向无功电度",186,1]
[147,"EPr","反向有功电度",187,1]
[148,"EPd","正向有功电度",188,1]
[148,"EQd","正向无功电度",189,1]
[148,"EQr","反向无功电度",190,1]
[148,"EPr","反向有功电度",191,1]
[149,"EPd","正向有功电度",192,1]
[149,"EQd","正向无功电度",193,1]
[149,"EQr","反向无功电度",194,1]
[149,"EPr","反向有功电度",195,1]
[150,"EPd","正向有功电度",196,1]
[150,"EQd","正向无功电度",197,1]
[150,"EQr","反向无功电度",198,1]
[150,"EPr","反向有功电度",199,1]
[151,"EPd","正向有功电度",200,1]
[151,"EQd","正向无功电度",201,1]
[151,"EQr","反向无功电度",202,1]
[151,"EPr","反向有功电度",203,1]
[152,"EPd","正向有功电度",204,1]
[152,"EQd","正向无功电度",205,1]
[152,"EQr","反向无功电度",206,1]
[152,"EPr","反向有功电度",207,1]

{"sheet":"模拟量","index":2,"n_rows":362,"n_cols":6,"rows_kept":362}
["DEV_ID","TAG_NAME","DESCRIPTION","REMOTE_NO","RATIO","REVISE"]
["设备ID","标签名","点描述","远动号","变比系数","修正值"]
[1,"UAB","AB相电压","0","1"]
[1,"VA","A相电压","1","1"]
[1,"VB","B相电压","2","1"]
[1,"VC","C相电压","3","1"]
[1,"VO","采集零序电压","4","1"]
[1,"F","频率","5","1"]
[2,"UAB","AB相电压","6","1"]
[2,"VA","A相电压","7","1"]
[2,"VB","B相电压","8","1"]
[2,"VC","C相电压","9","1"]
[2,"VO","采集零序电压","10","1"]
[2,"F","频率","11","1"]
[3,"P","有功功率","12","1"]
[3,"Q","无功功率","13","1"]
[3,"IA","A相电流","14","1"]
[3,"IB","B相电流","15","1"]
[3,"IC","C相电流","16","1"]
[4,"P","有功功率","17","1"]
[4,"Q","无功功率","18","1"]
[4,"PF","功率因数","19","1"]
[4,"IA","A相电流","20","1"]
[4,"IB","B相电流","21","1"]
[4,"IC","C相电流","22","1"]
[5,"P","有功功率","23","1"]
[5,"Q","无功功率","24","1"]
[5,"PF","功率因数","25","1"]
[5,"IA","A相电流","26","1"]
[5,"IB","B相电流","27","1"]
[5,"IC","C相电流","28","1"]
[6,"Tap","档位1","29","1"]
[6,"TP1","油面温度1","30","1"]
[6,"TP2","油面温度2","31","1"]
[6,"TP3","绕组温度","32","1"]
[7,"P","有功功率","33","1"]
[7,"Q","无功功率","34","1"]
[7,"PF","功率因数","35","1"]
[7,"IA","A相电流","36","1"]
[7,"IB","B相电流","37","1"]
[7,"IC","C相电流","38","1"]
[8,"P","有功功率","39","1"]
[8,"Q","无功功率","40","1"]
[8,"PF","功率因数","41","1"]
[8,"IA","A相电流","42","1"]
[8,"IB","B相电流","43","1"]
[8,"IC","C相电流","44","1"]
[9,"Tap","档位","45","1"]
[9,"TP1","油面温度1","46","1"]
[9,"TP2","油面温度2","47","1"]
[9,"TP3","绕组温度","48","1"]
[10,"P","有功功率","49","1"]
[10,"Q","无功功率","50","1"]
[10,"PF","功率因数","51","1"]
[10,"IA","A相电流","52","1"]
[10,"IB","B相电流","53","1"]
[10,"IC","C相电流","54","1"]
[11,"P","有功功率","55","1"]
[11,"Q","无功功率","56","1"]
[11,"PF","功率因数","57","1"]
[11,"IA","A相电流","58","1"]
[11,"IB","B相电流","59","1"]
[11,"IC","C相电流","60","1"]
[12,"Tap","档位","61","1"]
[12,"TP1","油面温度1","62","1"]
[12,"TP2","油面温度2","63","1"]
[12,"TP3","绕组温度","64","1"]
[13,"P","有功功率","65","1"]
[13,"Q","无功功率","66","1"]
[13,"PF","功率因数","67","1"]
[13,"IA","A相电流","68","1"]
[13,"IB","B相电流","69","1"]
[13,"IC","C相电流","70","1"]
[14,"P","有功功率","71","1"]
[14,"Q","无功功率","72","1"]
[14,"PF","功率因数","73","1"]
[14,"IA","A相电流","74","1"]
[14,"IB","B相电流","75","1"]
[14,"IC","C相电流","76","1"]
[15,"Tap","档位","77","1"]
[15,"TP1","油面温度1","78","1"]
[15,"TP2","油面温度2","79","1"]
[15,"TP3","绕组温度","80","1"]
[16,"P","有功功率","81","1"]
[16,"Q","无功功率","82","1"]
[16,"IA","A相电流","83","1"]
[16,"IB","B相电流","84","1"]
[16,"IC","C相电流","85","1"]
[17,"P","有功功率","86","1"]
[17,"Q","无功功率","87","1"]
[17,"IA","A相电流","88","1"]
[17,"IB","B相电流","89","1"]
[17,"IC","C相电流","90","1"]
[18,"P","有功功率","91","1"]
[18,"Q","无功功率","92","1"]
[18,"IA","A相电流","93","1"]
[18,"IB","B相电流","94","1"]
[18,"IC","C相电流","95","1"]
[19,"UAB","AB相电压","96","1"]
[19,"VA","A相电压","97","1"]
[19,"VB","B相电压","98","1"]
[19,"VC","C相电压","99","1"]
[19,"VO","采集零序电压","100","1"]
[19,"F","频率","101","1"]
[20,"UAB","AB相电压","102","1"]
[20,"VA","A相电压","103","1"]
[20,"VB","B相电压","104","1"]
[20,"VC","C相电压","105","1"]
[20,"VO","采集零序电压","106","1"]
[20,"F","频率","107","1"]
[21,"UAB","AB相电压","108","1"]
[21,"VA","A相电压","109","1"]
[21,"VB","B相电压","110","1"]
[21,"VC","C相电压","111","1"]
[21,"VO","采集零序电压","112","1"]
[21,"F","频率","113","1"]
[22,"UAB","AB相电压","114","1"]
[22,"VA","A相电压","115","1"]
[22,"VB","B相电压","116","1"]
[22,"VC","C相电压","117","1"]
[22,"VO","采集零序电压","118","1"]
[22,"F","频率","119","1"]
[23,"P","有功功率","120","1"]
[23,"Q","无功功率","121","1"]
[23,"PF","功率因数","122","1"]
[23,"IA","A相电流","123","1"]
[23,"IB","B相电流","124","1"]
[23,"IC","C相电流","125","1"]
[24,"P","有功功率","126","1"]
[24,"Q","无功功率","127","1"]
[24,"PF","功率因数","128","1"]
[24,"IA","A相电流","129","1"]
[24,"IB","B相电流","130","1"]
[24,"IC","C相电流","131","1"]
[25,"P","有功功率","132","1"]
[25,"Q","无功功率","133","1"]
[25,"PF","功率因数","134","1"]
[25,"IA","A相电流","135","1"]
[25,"IB","B相电流","136","1"]
[25,"IC","C相电流","137","1"]
[26,"P","有功功率","138","1"]
[26,"Q","无功功率","139","1"]
[26,"PF","功率因数","140","1"]
[26,"IA","A相电流","141","1"]
[26,"IB","B相电流","142","1"]
[26,"IC","C相电流","143","1"]
[27,"P","有功功率","144","1"]
[27,"Q","无功功率","145","1"]
[27,"PF","功率因数","146","1"]
[27,"IA","A相电流","147","1"]
[27,"IB","B相电流","148","1"]
[27,"IC","C相电流","149","1"]
[28,"P","有功功率","150","1"]
[28,"Q","无功功率","151","1"]
[28,"PF","功率因数","152","1"]
[28,"IA","A相电流","153","1"]
[28,"IB","B相电流","154","1"]
[28,"IC","C相电流","155","1"]
[29,"P","有功功率","156","1"]
[29,"Q","无功功率","157","1"]
[29,"PF","功率因数","158","1"]
[29,"IA","A相电流","159","1"]
[29,"IB","B相电流","160","1"]
[29,"IC","C相电流","161","1"]
[30,"IA","A相电流","162","1"]
[30,"IB","B相电流","163","1"]
[30,"IC","C相电流","164","1"]
[31,"P","有功功率","165","1"]
[31,"Q","无功功率","166","1"]
[31,"PF","功率因数","167","1"]
[31,"IA","A相电流","168","1"]
[31,"IB","B相电流","169","1"]
[31,"IC","C相电流","170","1"]
[32,"P","有功功率","171","1"]
[32,"Q","无功功率","172","1"]
[32,"PF","功率因数","173","1"]
[32,"IA","A相电流","174","1"]
[32,"IB","B相电流","175","1"]
[32,"IC","C相电流","176","1"]
[33,"P","有功功率","177","1"]
[33,"Q","无功功率","178","1"]
[33,"PF","功率因数","179","1"]
[33,"IA","A相电流","180","1"]
[33,"IB","B相电流","181","1"]
[33,"IC","C相电流","182","1"]
[34,"P","有功功率","183","1"]
[34,"Q","无功功率","184","1"]
[34,"PF","功率因数","185","1"]
[34,"IA","A相电流","186","1"]
[34,"IB","B相电流","187","1"]
[34,"IC","C相电流","188","1"]
[35,"P","有功功率","189","1"]
[35,"Q","无功功率","190","1"]
[35,"PF","功率因数","191","1"]
[35,"IA","A相电流","192","1"]
[35,"IB","B相电流","193","1"]
[35,"IC","C相电流","194","1"]
[36,"P","有功功率","195","1"]
[36,"Q","无功功率","196","1"]
[36,"PF","功率因数","197","1"]
[36,"IA","A相电流","198","1"]
[36,"IB","B相电流","199","1"]
[36,"IC","C相电流","200","1"]
[37,"P","有功功率","201","1"]
[37,"Q","无功功率","202","1"]
[37,"PF","功率因数","203","1"]
[37,"IA","A相电流","204","1"]
[37,"IB","B相电流","205","1"]
[37,"IC","C相电流","206","1"]
[38,"IA","A相电流","207","1"]
[38,"IB","B相电流","208","1"]
[38,"IC","C相电流","209","1"]
[39,"P","有功功率","210","1"]
[39,"Q","无功功率","211","1"]
[39,"PF","功率因数","212","1"]
[39,"IA","A相电流","213","1"]
[39,"IB","B相电流","214","1"]
[39,"IC","C相电流","215","1"]
[40,"P","有功功率","216","1"]
[40,"Q","无功功率","217","1"]
[40,"PF","功率因数","218","1"]
[40,"IA","A相电流","219","1"]
[40,"IB","B相电流","220","1"]
[40,"IC","C相电流","221","1"]
[41,"P","有功功率","222","1"]
[41,"Q","无功功率","223","1"]
[41,"PF","功率因数","224","1"]
[41,"IA","A相电流","225","1"]
[41,"IB","B相电流","226","1"]
[41,"IC","C相电流","227","1"]
[42,"P","有功功率","228","1"]
[42,"Q","无功功率","229","1"]
[42,"PF","功率因数","230","1"]
[42,"IA","A相电流","231","1"]
[42,"IB","B相电流","232","1"]
[42,"IC","C相电流","233","1"]
[43,"P","有功功率","234","1"]
[43,"Q","无功功率","235","1"]
[43,"PF","功率因数","236","1"]
[43,"IA","A相电流","237","1"]
[43,"IB","B相电流","238","1"]
[43,"IC","C相电流","239","1"]
[44,"P","有功功率","240","1"]
[44,"Q","无功功率","241","1"]
[44,"PF","功率因数","242","1"]
[44,"IA","A相电流","243","1"]
[44,"IB","B相电流","244","1"]
[44,"IC","C相电流","245","1"]
[45,"P","有功功率","246","1"]
[45,"Q","无功功率","247","1"]
[45,"PF","功率因数","248","1"]
[45,"IA","A相电流","249","1"]
[45,"IB","B相电流","250","1"]
[45,"IC","C相电流","251","1"]
[46,"IA","A相电流","252","1"]
[46,"IB","B相电流","253","1"]
[46,"IC","C相电流","254","1"]
[47,"P","有功功率","255","1"]
[47,"Q","无功功率","256","1"]
[47,"PF","功率因数","257","1"]
[47,"IA","A相电流","258","1"]
[47,"IB","B相电流","259","1"]
[47,"IC","C相电流","260","1"]
[48,"P","有功功率","261","1"]
[48,"Q","无功功率","262","1"]
[48,"PF","功率因数","263","1"]
[48,"IA","A相电流","264","1"]
[48,"IB","B相电流","265","1"]
[48,"IC","C相电流","266","1"]
[49,"P","有功功率","267","1"]
[49,"Q","无功功率","268","1"]
[49,"PF","功率因数","269","1"]
[49,"IA","A相电流","270","1"]
[49,"IB","B相电流","271","1"]
[49,"IC","C相电流","272","1"]
[50,"P","有功功率","273","1"]
[50,"Q","无功功率","274","1"]
[50,"PF","功率因数","275","1"]
[50,"IA","A相电流","276","1"]
[50,"IB","B相电流","277","1"]
[50,"IC","C相电流","278","1"]
[51,"P","有功功率","279","1"]
[51,"Q","无功功率","280","1"]
[51,"PF","功率因数","281","1"]
[51,"IA","A相电流","282","1"]
[51,"IB","B相电流","283","1"]
[51,"IC","C相电流","284","1"]
[52,"P","有功功率","285","1"]
[52,"Q","无功功率","286","1"]
[52,"PF","功率因数","287","1"]
[52,"IA","A相电流","288","1"]
[52,"IB","B相电流","289","1"]
[52,"IC","C相电流","290","1"]
[53,"P","有功功率","291","1"]
[53,"Q","无功功率","292","1"]
[53,"PF","功率因数","293","1"]
[53,"IA","A相电流","294","1"]
[53,"IB","B相电流","295","1"]
[53,"IC","C相电流","296","1"]
[54,"IA","A相电流","297","1"]
[54,"IB","B相电流","298","1"]
[54,"IC","C相电流","299","1"]
[55,"IA","A相电流","300","1"]
[55,"IB","B相电流","301","1"]
[55,"IC","C相电流","302","1"]
[55,"P","有功功率","303","1"]
[55,"Q","无功功率","304","1"]
[55,"PF","功率因数","305","1"]
[56,"IA","A相电流","306","1"]
[56,"IB","B相电流","307","1"]
[56,"IC","C相电流","308","1"]
[56,"P","有功功率","309","1"]
[56,"Q","无功功率","310","1"]
[56,"PF","功率因数","311","1"]
[57,"IA","A相电流","312","1"]
[57,"IB","B相电流","313","1"]
[57,"IC","C相电流","314","1"]
[57,"P","有功功率","315","1"]
[57,"Q","无功功率","316","1"]
[57,"PF","功率因数","317","1"]
[58,"IA","A相电流","318","1"]
[58,"IB","B相电流","319","1"]
[58,"IC","C相电流","320","1"]
[58,"P","有功功率","321","1"]
[58,"Q","无功功率","322","1"]
[58,"PF","功率因数","323","1"]
[59,"IA","A相电流","324","1"]
[59,"IB","B相电流","325","1"]
[59,"IC","C相电流","326","1"]
[59,"P","有功功率","327","1"]
[59,"Q","无功功率","328","1"]
[59,"PF","功率因数","329","1"]
[60,"IA","A相电流","330","1"]
[60,"IB","B相电流","331","1"]
[60,"IC","C相电流","332","1"]
[60,"P","有功功率","333","1"]
[60,"Q","无功功率","334","1"]
[60,"PF","功率因数","335","1"]
[61,"IA","A相电流","336","1"]
[61,"IB","B相电流","337","1"]
[61,"IC","C相电流","338","1"]
[61,"P","有功功率","339","1"]
[61,"Q","无功功率","340","1"]
[61,"PF","功率因数","341","1"]
[62,"IA","A相电流","342","1"]
[62,"IB","B相电流","343","1"]
[62,"IC","C相电流","344","1"]
[62,"P","有功功率","345","1"]
[62,"Q","无功功率","346","1"]
[62,"PF","功率因数","347","1"]
[63,"IA","A相电流","348","1"]
[63,"IB","B相电流","349","1"]
[63,"IC","C相电流","350","1"]
[63,"P","有功功率","351","1"]
[63,"Q","无功功率","352","1"]
[63,"PF","功率因数","353","1"]
[64,"IA","A相电流","354","1"]
[64,"IB","B相电流","355","1"]
[64,"IC","C相电流","356","1"]
[64,"P","有功功率","357","1"]
[64,"Q","无功功率","358","1"]
[64,"PF","功率因数","359","1"]

{"sheet":"数字量","index":3,"n_rows":5843,"n_cols":4,"rows_kept":5843}
["DEV_ID","TAG_NAME","DESCRIPTION","REMOTE_NO"]
["设备ID","标签名","点描述","远动号"]
[0,"TotEvt","全站事故总",0]
[16,"PosOn","存222断路器三相合位",1]
[16,"SPos2","存2221隔刀合位",2]
[16,"SPos3","存2222隔刀合位",3]
[16,"SPos","存2226隔刀合位",4]
[16,"ESPos","存2225地刀合位",5]
[16,"ESPos2","存2228地刀合位",6]
[16,"ESPos3","存2229地刀合位",7]
[17,"PosOn","存229断路器三相合位",8]
[17,"SPos2","存2291隔刀合位",9]
[17,"SPos3","存2292隔刀合位",10]
[17,"SPos","存2296隔刀合位",11]
[17,"ESPos","存2295地刀合位",12]
[17,"ESPos2","存2298地刀合位",13]
[17,"ESPos3","存2299地刀合位",14]
[17,"by1","备用",15]
[17,"by2","备用",16]
[17,"by3","备用",17]
[17,"by4","备用",18]
[17,"by5","备用",19]
[17,"by6","备用",20]
[17,"by7","备用",21]
[3,"PosOn","存227断路器三相合位",22]
[3,"SPos2","存2271隔刀合位",23]
[3,"SPos3","存2272隔刀合位",24]
[3,"ESPos2","存2275地刀合位",25]
[3,"ESPos3","存2274地刀合位",26]
[1,"SPos","互01隔刀合位",27]
[1,"ESPos2","互015地刀合位",28]
[1,"ESPos","互014地刀合位",29]
[2,"SPos","互02隔刀合位",30]
[2,"ESPos2","互025地刀合位",31]
[2,"ESPos","互024地刀合位",32]
[4,"PosOn","存221断路器三相合位",33]
[4,"SPos2","存2211隔刀合位",34]
[4,"SPos3","存2212隔刀合位",35]
[4,"SPos","存2216隔刀合位",36]
[4,"ESPos","存2215地刀合位",37]
[4,"ESPos2","存2218地刀合位",38]
[4,"ESPos3","存2219地刀合位",39]
[6,"ESPos","2217中性点地刀合位",40]
[5,"PosOn","存308断路器合位",41]
[5,"RkdIn","存308手车工作位置",42]
[7,"PosOn","存224断路器三相合位",43]
[7,"SPos2","存2241隔刀合位",44]
[7,"SPos3","存2242隔刀合位",45]
[7,"SPos","存2246隔刀合位",46]
[7,"ESPos","存2245地刀合位",47]
[7,"ESPos2","存2248地刀合位",48]
[7,"ESPos3","存2249地刀合位",49]
[9,"ESPos","2247中性点地刀合位",50]
[8,"PosOn","存408断路器合位",51]
[8,"RkdIn","存408手车工作位置",52]
[10,"PosOn","存226断路器三相合位",53]
[10,"SPos2","存2261隔刀合位",54]
[10,"SPos3","存2262隔刀合位",55]
[10,"SPos","存2266隔刀合位",56]
[10,"ESPos","存2265地刀合位",57]
[10,"ESPos2","存2268地刀合位",58]
[10,"ESPos3","存2269地刀合位",59]
[12,"ESPos","2267中性点地刀合位",60]
[11,"PosOn","存508断路器合位",61]
[11,"RkdIn","存508手车工作位置",62]
[13,"PosOn","存230断路器三相合位",63]
[13,"SPos2","存2301隔刀合位",64]
[13,"SPos3","存2302隔刀合位",65]
[13,"SPos","存2306隔刀合位",66]
[13,"ESPos","存2305地刀合位",67]
[13,"ESPos2","存2308地刀合位",68]
[13,"ESPos3","存2309地刀合位",69]
[15,"ESPos","2307中性点地刀合位",70]
[14,"PosOn","存608断路器合位",71]
[14,"RkdIn","存608手车工作位置",72]
[55,"PosOn","存309断路器合位",73]
[55,"RkdIn","存309手车工作位置",74]
[55,"ESPos","存3099地刀合位",75]
[55,"by1","备用",76]
[55,"by2","备用",77]
[58,"PosOn","存419断路器合位",78]
[58,"RkdIn","存419手车工作位置",79]
[58,"ESPos","存4199地刀合位",80]
[58,"by1","备用",81]
[58,"by2","备用",82]
[60,"PosOn","存509断路器合位",83]
[60,"RkdIn","存509手车工作位置",84]
[60,"ESPos","存509地刀合位",85]
[60,"by1","备用",86]
[60,"by2","备用",87]
[62,"PosOn","存609断路器合位",88]
[62,"RkdIn","存609手车工作位置",89]
[62,"ESPos","存609地刀合位",90]
[62,"by1","备用",91]
[62,"by2","备用",92]
[56,"PosOn","存310断路器合位",93]
[56,"RkdIn","存310手车工作位置",94]
[56,"ESPos","存3109地刀合位",95]
[56,"SPos","接地电阻柜隔离开关合位",96]
[59,"PosOn","存410断路器合位",97]
[59,"RkdIn","存410手车工作位置",98]
[59,"ESPos","存4109地刀合位",99]
[59,"SPos","接地电阻柜隔离开关合位",100]
[61,"PosOn","存510断路器合位",101]
[61,"RkdIn","存510手车工作位置",102]
[61,"ESPos","存5109地刀合位",103]
[61,"SPos","接地电阻柜隔离开关合位",104]
[63,"PosOn","存610断路器合位",105]
[63,"RkdIn","存610手车工作位置",106]
[63,"ESPos","存6109地刀合位",107]
[63,"SPos","接地电阻柜隔离开关合位",108]
[57,"PosOn","存311断路器合位",109]
[57,"RkdIn","存311手车工作位置",110]
[57,"ESPos","存3119地刀合位",111]
[64,"PosOn","存611断路器合位",112]
[64,"RkdIn","存611手车工作位置",113]
[64,"ESPos","存6119地刀合位",114]
[92,"PosOn","存902断路器合位",115]
[92,"RkdIn","存902手车工作位置",116]
[92,"ESPos","存9029地刀合位",117]
[91,"RkdIn","存901站用进线手车工作位置",118]
[91,"ESPos","存901站用进线地刀合位",119]
[65,"PosOn","存314断路器合位",120]
[65,"RkdIn","存314手车工作位置",121]
[66,"PosOn","存415断路器合位",122]
[66,"RkdIn","存415手车工作位置",123]
[67,"PosOn","存516断路器合位",124]
[67,"RkdIn","存516手车工作位置",125]
[68,"PosOn","存613断路器合位",126]
[68,"RkdIn","存613手车工作位置",127]
[19,"RkdIn","互03b手车工作位置",128]
[19,"sRkdIn","存3141隔离手车工作位置",129]
[20,"RkdIn","互04b手车工作位置",130]
[20,"sRkdIn","存4151隔离手车工作位置",131]
[21,"RkdIn","互05b手车工作位置",132]
[21,"sRkdIn","存5161隔离手车工作位置",133]
[22,"RkdIn","互06b手车工作位置",134]
[22,"sRkdIn","存6131隔离手车工作位置",135]
[23,"PosOn","存301断路器合位",136]
[23,"RkdIn","存301手车工作位置",137]
[23,"ESPos","存3019地刀合位",138]
[24,"PosOn","存302断路器合位",139]
[24,"RkdIn","存302手车工作位置",140]
[24,"ESPos","存3029地刀合位",141]
[25,"PosOn","存303断路器合位",142]
[25,"RkdIn","存303手车工作位置",143]
[25,"ESPos","存3039地刀合位",144]
[26,"PosOn","存304断路器合位",145]
[26,"RkdIn","存304手车工作位置",146]
[26,"ESPos","存3049地刀合位",147]
[27,"PosOn","存305断路器合位",148]
[27,"RkdIn","存305手车工作位置",149]
[27,"ESPos","存3059地刀合位",150]
[28,"PosOn","存306断路器合位",151]
[28,"RkdIn","存306手车工作位置",152]
[28,"ESPos","存3069地刀合位",153]
[29,"PosOn","存307断路器合位",154]
[29,"RkdIn","存307手车工作位置",155]
[29,"ESPos","存3079地刀合位",156]
[31,"PosOn","存401断路器合位",157]
[31,"RkdIn","存401手车工作位置",158]
[31,"ESPos","存4019地刀合位",159]
[32,"PosOn","存402断路器合位",160]
[32,"RkdIn","存402手车工作位置",161]
[32,"ESPos","存4029地刀合位",162]
[33,"PosOn","存403断路器合位",163]
[33,"RkdIn","存403手车工作位置",164]
[33,"ESPos","存4039地刀合位",165]
[34,"PosOn","存404断路器合位",166]
[34,"RkdIn","存404手车工作位置",167]
[34,"ESPos","存4049地刀合位",168]
[35,"PosOn","存405断路器合位",169]
[35,"RkdIn","存405手车工作位置",170]
[35,"ESPos","存4059地刀合位",171]
[36,"PosOn","存406断路器合位",172]
[36,"RkdIn","存406手车工作位置",173]
[36,"ESPos","存4069地刀合位",174]
[37,"PosOn","存407断路器合位",175]
[37,"RkdIn","存407手车工作位置",176]
[37,"ESPos","存4079地刀合位",177]
[39,"PosOn","存501断路器合位",178]
[39,"RkdIn","存501手车工作位置",179]
[39,"ESPos","存5019地刀合位",180]
[40,"PosOn","存502断路器合位",181]
[40,"RkdIn","存502手车工作位置",182]
[40,"ESPos","存5029地刀合位",183]
[41,"PosOn","存503断路器合位",184]
[41,"RkdIn","存503手车工作位置",185]
[41,"ESPos","存5039地刀合位",186]
[42,"PosOn","存504断路器合位",187]
[42,"RkdIn","存504手车工作位置",188]
[42,"ESPos","存504地刀合位",189]
[43,"PosOn","存505断路器合位",190]
[43,"RkdIn","存505手车工作位置",191]
[43,"ESPos","存505地刀合位",192]
[44,"PosOn","存506断路器合位",193]
[44,"RkdIn","存506手车工作位置",194]
[44,"ESPos","存506地刀合位",195]
[45,"PosOn","存507断路器合位",196]
[45,"RkdIn","存507手车工作位置",197]
[45,"ESPos","存507地刀合位",198]
[47,"PosOn","存601断路器合位",199]
[47,"RkdIn","存601手车工作位置",200]
[47,"ESPos","存601地刀合位",201]
[48,"PosOn","存602断路器合位",202]
[48,"RkdIn","存602手车工作位置",203]
[48,"ESPos","存602地刀合位",204]
[49,"PosOn","存603断路器合位",205]
[49,"RkdIn","存603手车工作位置",206]
[49,"ESPos","存603地刀合位",207]
[50,"PosOn","存604断路器合位",208]
[50,"RkdIn","存604手车工作位置",209]
[50,"ESPos","存604地刀合位",210]
[51,"PosOn","存605断路器合位",211]
[51,"RkdIn","存605手车工作位置",212]
[51,"ESPos","存605地刀合位",213]
[52,"PosOn","存606断路器合位",214]
[52,"RkdIn","存606手车工作位置",215]
[52,"ESPos","存606地刀合位",216]
[53,"PosOn","存607断路器合位",217]
[53,"RkdIn","存607手车工作位置",218]
[53,"ESPos","存607地刀合位",219]
[53,"by1","备用",220]
[53,"by2","备用",221]
[53,"by3","备用",222]
[53,"by4","备用",223]
[53,"by5","备用",224]
[53,"by6","备用",225]
[53,"by7","备用",226]
[53,"by8","备用",227]
[53,"by9","备用",228]
[53,"by10","备用",229]
[53,"by11","备用",230]
[53,"by12","备用",231]
[53,"by13","备用",232]
[53,"by14","备用",233]
[53,"by15","备用",234]
[53,"by16","备用",235]
[53,"by17","备用",236]
[53,"by18","备用",237]
[53,"by19","备用",238]
[53,"by20","备用",239]
[53,"by21","备用",240]
[53,"by22","备用",241]
[53,"by23","备用",242]
[53,"by24","备用",243]
[1,"Arm1","装置闭锁",244]
[1,"Arm2","装置异常告警",245]
[1,"Arm3","装置自检异常",246]
[1,"Arm4","通信传动报警",247]
[1,"Arm5","开出传动报警",248]
[1,"Arm6","对时异常",249]
[1,"Arm7","IEC61850通信传动报警",250]
[1,"Arm8","对时信号状态",251]
[1,"Arm9","对时服务状态",252]
[1,"Arm10","时间跳变侦测状态",253]
[1,"Arm11","母线1零序过压报警",254]
[1,"Arm12","母线1低电压报警",255]
[1,"Arm13","母线2零序过压报警",256]
[1,"Arm14","母线2低电压报警",257]
[1,"Arm15","母线3零序过压报警",258]
[1,"Arm16","母线3低电压报警",259]
[1,"Arm17","母线4零序过压报警",260]
[1,"Arm18","母线4低电压报警",261]
[1,"Arm19","双位置异常",262]
[1,"Arm20","事故总信号",263]
[1,"Arm21","三相档位不一致",264]
[1,"Arm22","滑档跳闸",265]
[1,"Arm23","出口使能软压板",266]
[1,"Arm24","外间隔退出软压板",267]
[1,"Arm25","投检修(B05X02)",268]
[1,"Arm26","解除闭锁(B05X03)",269]
[1,"Arm27","投远方(B05X04)",270]
[1,"Arm28","手合同期(B05X05)",271]
[1,"Arm29","手动分闸(B05X06)",272]
[1,"Arm30","保留1(B05X07)",273]
[1,"Arm31","保留2(B05X08)",274]
[1,"Arm32","保留3(B05X09)",275]
[1,"Arm33","保留4(B05X10)",276]
[1,"Arm34","保留5(B05X11)",277]
[1,"Arm35","保留6(B05X12)",278]
[1,"Arm36","保留7(B05X13)",279]
[1,"Arm37","保留8(B05X14)",280]
[1,"Arm38","保留9(B05X15)",281]
[1,"Arm39","互01隔刀分位",282]
[1,"Arm40","互015地刀分位",283]
[1,"Arm41","互014地刀分位",284]
[1,"Arm42","刀闸近控",285]
[1,"Arm43","联锁解除",286]
[1,"Arm44","SF6气舱漏气",287]
[1,"Arm45","SF6气舱密度达到最小",288]
[1,"Arm46","交流电源断电",289]
[1,"Arm47","马达电源断电",290]
[1,"Arm48","直流电源断电",291]
[1,"Arm49","计量电压空开跳闸",292]
[1,"Arm50","测量电压空开跳闸",293]
[1,"Arm51","保护电压空开跳闸",294]
[1,"Arm52","报警信号电源断电",295]
[1,"Arm53","公用测控1装置闭锁",296]
[1,"Arm54","公用测控1装置报警",297]
[1,"Arm55","公用测控1遥控信号",298]
[1,"Arm56","公用测控2装置闭锁",299]
[1,"Arm57","公用测控2装置报警",300]
[1,"Arm58","公用测控2遥控信号",301]
[1,"Arm59","KKJ",302]
[1,"Arm60","网络状态1",303]
[1,"Arm61","网络状态2",304]
[1,"Arm62","装置通讯状态",305]
[1,"Arm63","检修状态",306]
[1,"Arm64","参数变化",307]
[1,"Arm65","就地状态虚遥信",308]
[1,"Arm66","遥控解除闭锁",309]
[1,"Arm67","A网中断",310]
[1,"Arm68","B网中断",311]
[1,"Arm69","网络中断",312]
[2,"Arm1","装置闭锁",313]
[2,"Arm2","装置异常告警",314]
[2,"Arm3","装置自检异常",315]
[2,"Arm4","通信传动报警",316]
[2,"Arm5","开出传动报警",317]
[2,"Arm6","对时异常",318]
[2,"Arm7","对时信号状态",319]
[2,"Arm8","对时服务状态",320]
[2,"Arm9","时间跳变侦测状态",321]
[2,"Arm10","母线1零序过压报警",322]
[2,"Arm11","母线1低电压报警",323]
[2,"Arm12","母线2零序过压报警",324]
[2,"Arm13","母线2低电压报警",325]
[2,"Arm14","母线3零序过压报警",326]
[2,"Arm15","母线3低电压报警",327]
[2,"Arm16","母线4零序过压报警",328]
[2,"Arm17","母线4低电压报警",329]
[2,"Arm18","双位置异常",330]
[2,"Arm19","事故总信号",331]
[2,"Arm20","三相档位不一致",332]
[2,"Arm21","滑档跳闸",333]
[2,"Arm22","出口使能软压板",334]
[2,"Arm23","外间隔退出软压板",335]
[2,"Arm24","投检修(B05X02)",336]
[2,"Arm25","解除闭锁(B05X03)",337]
[2,"Arm26","投远方(B05X04)",338]
[2,"Arm27","手合同期(B05X05)",339]
[2,"Arm28","手动分闸(B05X06)",340]
[2,"Arm29","保留1(B05X07)",341]
[2,"Arm30","保留2(B05X08)",342]
[2,"Arm31","保留3(B05X09)",343]
[2,"Arm32","保留4(B05X10)",344]
[2,"Arm33","保留5(B05X11)",345]
[2,"Arm34","保留6(B05X12)",346]
[2,"Arm35","保留7(B05X13)",347]
[2,"Arm36","保留8(B05X14)",348]
[2,"Arm37","保留9(B05X15)",349]
[2,"Arm38","互02隔刀分位",350]
[2,"Arm39","互025地刀分位",351]
[2,"Arm40","互024地刀分位",352]
[2,"Arm41","刀闸近控",353]
[2,"Arm42","联锁解除",354]
[2,"Arm43","SF6气舱漏气",355]
[2,"Arm44","SF6气舱密度达到最小",356]
[2,"Arm45","交流电源断电",357]
[2,"Arm46","马达电源断电",358]
[2,"Arm47","直流电源断电",359]
[2,"Arm48","计量电压空开跳闸",360]
[2,"Arm49","测量电压空开跳闸",361]
[2,"Arm50","保护电压空开跳闸",362]
[2,"Arm51","报警信号电源断电",363]
[2,"Arm52","KKJ",364]
[2,"Arm53","网络状态1",365]
[2,"Arm54","网络状态2",366]
[2,"Arm55","装置通讯状态",367]
[2,"Arm56","检修状态",368]
[2,"Arm57","参数变化",369]
[2,"Arm58","就地状态虚遥信",370]
[2,"Arm59","遥控解除闭锁",371]
[2,"Arm60","A网中断",372]
[2,"Arm61","B网中断",373]
[2,"Arm62","网络中断",374]
[3,"Arm1","装置闭锁",375]
[3,"Arm2","装置异常告警",376]
[3,"Arm3","装置自检异常",377]
[3,"Arm4","通信传动报警",378]
[3,"Arm5","开出传动报警",379]
[3,"Arm6","对时异常",380]
[3,"Arm7","对时信号状态",381]
[3,"Arm8","对时服务状态",382]
[3,"Arm9","时间跳变侦测状态",383]
[3,"Arm10","零序过压报警",384]
[3,"Arm11","PT断线报警",385]
[3,"Arm12","低电压报警",386]
[3,"Arm13","CT异常报警",387]
[3,"Arm14","双位置异常",388]
[3,"Arm15","事故总信号",389]
[3,"Arm16","三相档位不一致",390]
[3,"Arm17","滑档跳闸",391]
[3,"Arm18","出口使能软压板",392]
[3,"Arm19","外间隔退出软压板",393]
[3,"Arm20","检无压软压板",394]
[3,"Arm21","检同期软压板",395]
[3,"Arm22","检合环软压板",396]
[3,"Arm23","投检修(B05X02)",397]
[3,"Arm24","解除闭锁(B05X03)",398]
[3,"Arm25","投远方(B05X04)",399]
[3,"Arm26","手合同期(B05X05)",400]
[3,"Arm27","手动分闸(B05X06)",401]
[3,"Arm28","保留1(B05X07)",402]
[3,"Arm29","保留2(B05X08)",403]
[3,"Arm30","保留3(B05X09)",404]
[3,"Arm31","保留4(B05X10)",405]
[3,"Arm32","保留5(B05X11)",406]
[3,"Arm33","存227断路器C相合位",407]
[3,"Arm34","保留7(B05X13)",408]
[3,"Arm35","保留8(B05X14)",409]
[3,"Arm36","保留9(B05X15)",410]
[3,"PosOff","存227断路器三相分位",411]
[3,"Arm38","存227断路器A相分位",412]
[3,"Arm39","存227断路器A相合位",413]
[3,"Arm40","存227断路器B相分位",414]
[3,"Arm41","存227断路器B相合位",415]
[3,"Arm42","存227断路器C相分位",416]
[3,"Arm43","存227断路器C相合位",417]
[3,"Arm44","存2271隔刀分位",418]
[3,"Arm45","存2272隔刀分位",419]
[3,"Arm46","存2275地刀分位",420]
[3,"Arm47","存2274地刀分位",421]
[3,"Arm48","开入31",422]
[3,"Arm49","开入32",423]
[3,"Arm50","开入33",424]
[3,"Arm51","开入34",425]
[3,"Arm52","刀闸近控",426]
[3,"Arm53","断路器近控",427]
[3,"Arm54","联锁解除",428]
[3,"Arm55","断路器SF6闭锁",429]
[3,"Arm56","三相不一致",430]
[3,"Arm57","马达保护",431]
[3,"Arm58","断路器SF6泄露",432]
[3,"Arm59","弹簧储能超时",433]
[3,"Arm60","弹簧未储能",434]
[3,"Arm61","SF6气舱漏气",435]
[3,"Arm62","SF6气舱密度达到最小",436]
[3,"Arm63","交流电源断电",437]
[3,"Arm64","马达电源断电",438]
[3,"Arm65","直流电源断电",439]
[3,"Arm66","报警信号电源断电",440]
[3,"Arm67","开入50",441]
[3,"Arm68","开入51",442]
[3,"Arm69","开入52",443]
[3,"Arm70","开入53",444]
[3,"Arm71","开入54",445]
[3,"Arm72","第一套保护动作",446]
[3,"Arm73","第一套保护运行异常",447]
[3,"Arm74","第一套保护装置故障失电告警",448]
[3,"Arm75","第一组控制回路断线",449]
[3,"Arm76","第二组控制回路断线",450]
[3,"Arm77","第二组控制电源消失",451]
[3,"Arm78","第一组出口跳闸",452]
[3,"Arm79","第二组出口跳闸",453]
[3,"Arm80","第二套保护装置闭锁",454]
[3,"Arm81","第二套保护装置异常",455]
[3,"Arm82","第二套保护动作",456]
[3,"Arm83","KKJ",457]
[3,"Arm84","网络状态1",458]
[3,"Arm85","网络状态2",459]
[3,"Arm86","装置通讯状态",460]
[3,"Arm87","检修状态",461]
[3,"Arm88","参数变化",462]
[3,"Arm89","就地状态虚遥信",463]
[3,"Arm90","遥控解除闭锁",464]
[3,"Arm91","A网中断",465]
[3,"Arm92","B网中断",466]
[3,"Arm93","网络中断",467]
[4,"Arm1","装置闭锁",468]
[4,"Arm2","装置异常告警",469]
[4,"Arm3","装置自检异常",470]
[4,"Arm4","通信传动报警",471]
[4,"Arm5","开出传动报警",472]
[4,"Arm6","对时异常",473]
[4,"Arm7","对时信号状态",474]
[4,"Arm8","对时服务状态",475]
[4,"Arm9","时间跳变侦测状态",476]
[4,"Arm10","零序过压报警",477]
[4,"Arm11","PT断线报警",478]
[4,"Arm12","低电压报警",479]
[4,"Arm13","CT异常报警",480]
[4,"Arm14","双位置异常",481]
[4,"Arm15","事故总信号",482]
[4,"Arm16","三相档位不一致",483]
[4,"Arm17","滑档跳闸",484]
[4,"Arm18","出口使能软压板",485]
[4,"Arm19","外间隔退出软压板",486]
[4,"Arm20","检无压软压板",487]
[4,"Arm21","检同期软压板",488]
[4,"Arm22","检合环软压板",489]
[4,"Arm23","投检修(B05X02)",490]
[4,"Arm24","解除闭锁(B05X03)",491]
[4,"Arm25","投远方(B05X04)",492]
[4,"Arm26","手合同期(B05X05)",493]
[4,"Arm27","手动分闸(B05X06)",494]
[4,"Arm28","保留1(B05X07)",495]
[4,"Arm29","保留2(B05X08)",496]
[4,"Arm30","保留3(B05X09)",497]
[4,"Arm31","保留4(B05X10)",498]
[4,"Arm32","保留5(B05X11)",499]
[4,"Arm33","保留6(B05X12)",500]
[4,"Arm34","保留7(B05X13)",501]
[4,"Arm35","保留8(B05X14)",502]
[4,"Arm36","保留9(B05X15)",503]
[4,"PosOff","存221断路器三相分位",504]
[4,"Arm38","存221断路器A相分位",505]
[4,"Arm39","存221断路器A相合位",506]
[4,"Arm40","存221断路器B相分位",507]
[4,"Arm41","存221断路器B相合位",508]
[4,"Arm42","存221断路器C相分位",509]
[4,"Arm43","存221断路器C相合位",510]
[4,"Arm44","存2211隔刀分位",511]
[4,"Arm45","存2212隔刀分位",512]
[4,"Arm46","存2216隔刀分位",513]
[4,"Arm47","存2215地刀分位",514]
[4,"Arm48","存2218地刀分位",515]
[4,"Arm49","存2219地刀分位",516]
[4,"Arm50","刀闸近控",517]
[4,"Arm51","断路器近控",518]
[4,"Arm52","联锁解除",519]
[4,"Arm53","断路器SF6闭锁",520]
[4,"Arm54","三相不一致",521]
[4,"Arm55","马达保护",522]
[4,"Arm56","断路器SF6泄露",523]
[4,"Arm57","弹簧储能超时",524]
[4,"Arm58","弹簧未储能",525]
[4,"Arm59","SF6气舱漏气",526]
[4,"Arm60","SF6气舱密度达到最小",527]
[4,"Arm61","交流电源断电",528]
[4,"Arm62","马达电源断电",529]
[4,"Arm63","直流电源断电",530]
[4,"Arm64","电压互感器空开跳闸",531]
[4,"Arm65","交流配电回路总空开跳闸",532]
[4,"Arm66","带电显示装置故障",533]
[4,"Arm67","带电显示装置线上无压",534]
[4,"Arm68","报警信号电源断电",535]
[4,"Arm69","直流配电回路总空开跳闸",536]
[4,"Arm70","开入55",537]
[4,"Arm71","开入56",538]
[4,"Arm72","开入57",539]
[4,"Arm73","第一套保护动作",540]
[4,"Arm74","第一套保护过负荷报警",541]
[4,"Arm75","第一套保护运行异常",542]
[4,"Arm76","第一套保护装置故障失电告警",543]
[4,"Arm77","第一套高压侧切换继电器同时动作",544]
[4,"Arm78","第一套高压侧切换继电器回路断线线或直流消失",545]
[4,"Arm79","第二套保护装置闭锁",546]
[4,"Arm80","第二套保护装置报警",547]
[4,"Arm81","第二套保护过负荷告警",548]
[4,"Arm82","第二套保护动作",549]
[4,"Arm83","第二套高压侧切换继电器同时消失",550]
[4,"Arm84","第二套高压侧切换继电器同时动作",551]
[4,"Arm85","第一组控制回路断线",552]
[4,"Arm86","第二组控制回路断线",553]
[4,"Arm87","第一组控制电源消失",554]
[4,"Arm88","第二组控制电源消失",555]
[4,"Arm89","第一组出口跳闸",556]
[4,"Arm90","第二组出口跳闸",557]
[4,"Arm91","KKJ",558]
[4,"Arm92","网络状态1",559]
[4,"Arm93","网络状态2",560]
[4,"Arm94","装置通讯状态",561]
[4,"Arm95","检修状态",562]
[4,"Arm96","参数变化",563]
[4,"Arm97","就地状态虚遥信",564]
[4,"Arm98","遥控解除闭锁",565]
[4,"Arm99","A网中断",566]
[4,"Arm100","B网中断",567]
[4,"Arm101","网络中断",568]
[7,"Arm1","装置闭锁",569]
[7,"Arm2","装置异常告警",570]
[7,"Arm3","装置自检异常",571]
[7,"Arm4","通信传动报警",572]
[7,"Arm5","开出传动报警",573]
[7,"Arm6","对时异常",574]
[7,"Arm7","对时信号状态",575]
[7,"Arm8","对时服务状态",576]
[7,"Arm9","时间跳变侦测状态",577]
[7,"Arm10","零序过压报警",578]
[7,"Arm11","PT断线报警",579]
[7,"Arm12","低电压报警",580]
[7,"Arm13","CT异常报警",581]
[7,"Arm14","双位置异常",582]
[7,"Arm15","事故总信号",583]
[7,"Arm16","三相档位不一致",584]
[7,"Arm17","滑档跳闸",585]
[7,"Arm18","出口使能软压板",586]
[7,"Arm19","外间隔退出软压板",587]
[7,"Arm20","检无压软压板",588]
[7,"Arm21","检同期软压板",589]
[7,"Arm22","检合环软压板",590]
[7,"Arm23","投检修(B05X02)",591]
[7,"Arm24","解除闭锁(B05X03)",592]
[7,"Arm25","投远方(B05X04)",593]
[7,"Arm26","手合同期(B05X05)",594]
[7,"Arm27","手动分闸(B05X06)",595]
[7,"Arm28","保留1(B05X07)",596]
[7,"Arm29","保留2(B05X08)",597]
[7,"Arm30","保留3(B05X09)",598]
[7,"Arm31","保留4(B05X10)",599]
[7,"Arm32","保留5(B05X11)",600]
[7,"Arm33","保留6(B05X12)",601]
[7,"Arm34","保留7(B05X13)",602]
[7,"Arm35","保留8(B05X14)",603]
[7,"Arm36","保留9(B05X15)",604]
[7,"PosOff","存224断路器三相分位",605]
[7,"Arm38","存224断路器A相分位",606]
[7,"Arm39","存224断路器A相合位",607]
[7,"Arm40","存224断路器B相分位",608]
[7,"Arm41","存224断路器B相合位",609]
[7,"Arm42","存224断路器C相分位",610]
[7,"Arm43","存224断路器C相合位",611]
[7,"Arm44","存2241隔刀分位",612]
[7,"Arm45","存2242隔刀分位",613]
[7,"Arm46","存2246隔刀分位",614]
[7,"Arm47","存2245地刀分位",615]
[7,"Arm48","存2248地刀分位",616]
[7,"Arm49","存2249地刀分位",617]
[7,"Arm50","刀闸近控",618]
[7,"Arm51","断路器近控",619]
[7,"Arm52","联锁解除",620]
[7,"Arm53","断路器SF6闭锁",621]
[7,"Arm54","三相不一致",622]
[7,"Arm55","马达保护",623]
[7,"Arm56","断路器SF6泄露",624]
[7,"Arm57","弹簧储能超时",625]
[7,"Arm58","弹簧未储能",626]
[7,"Arm59","SF6气舱漏气",627]
[7,"Arm60","SF6气舱密度达到最小",628]
[7,"Arm61","交流电源断电",629]
[7,"Arm62","马达电源断电",630]
[7,"Arm63","直流电源断电",631]
[7,"Arm64","电压互感器空开跳闸",632]
[7,"Arm65","交流配电回路总空开跳闸",633]
[7,"Arm66","带电显示装置故障",634]
[7,"Arm67","带电显示装置线上无压",635]
[7,"Arm68","报警信号电源断电",636]
[7,"Arm69","直流配电回路总空开跳闸",637]
[7,"Arm70","开入55",638]
[7,"Arm71","开入56",639]
[7,"Arm72","开入57",640]
[7,"Arm73","第一套保护动作",641]
[7,"Arm74","第一套保护过负荷报警",642]
[7,"Arm75","第一套保护运行异常",643]
[7,"Arm76","第一套保护装置故障失电告警",644]
[7,"Arm77","第一套高压侧切换继电器同时动作",645]
[7,"Arm78","第一套高压侧切换继电器回路断线线或直流消失",646]
[7,"Arm79","第二套保护装置闭锁",647]
[7,"Arm80","第二套保护装置报警",648]
[7,"Arm81","第二套保护过负荷告警",649]
[7,"Arm82","第二套保护动作",650]
[7,"Arm83","第二套高压侧切换继电器同时消失",651]
[7,"Arm84","第二套高压侧切换继电器同时动作",652]
[7,"Arm85","第一组控制回路断线",653]
[7,"Arm86","第二组控制回路断线",654]
[7,"Arm87","第一组控制电源消失",655]
[7,"Arm88","第二组控制电源消失",656]
[7,"Arm89","第一组出口跳闸",657]
[7,"Arm90","第二组出口跳闸",658]
[7,"Arm91","KKJ",659]
[7,"Arm92","网络状态1",660]
[7,"Arm93","网络状态2",661]
[7,"Arm94","装置通讯状态",662]
[7,"Arm95","检修状态",663]
[7,"Arm96","参数变化",664]
[7,"Arm97","就地状态虚遥信",665]
[7,"Arm98","遥控解除闭锁",666]
[7,"Arm99","A网中断",667]
[7,"Arm100","B网中断",668]
[7,"Arm101","网络中断",669]
[10,"Arm1","装置闭锁",670]
[10,"Arm2","装置异常告警",671]
[10,"Arm3","装置自检异常",672]
[10,"Arm4","通信传动报警",673]
[10,"Arm5","开出传动报警",674]
[10,"Arm6","对时异常",675]
[10,"Arm7","对时信号状态",676]
[10,"Arm8","对时服务状态",677]
[10,"Arm9","时间跳变侦测状态",678]
[10,"Arm10","零序过压报警",679]
[10,"Arm11","PT断线报警",680]
[10,"Arm12","低电压报警",681]
[10,"Arm13","CT异常报警",682]
[10,"Arm14","双位置异常",683]
[10,"Arm15","事故总信号",684]
[10,"Arm16","三相档位不一致",685]
[10,"Arm17","滑档跳闸",686]
[10,"Arm18","出口使能软压板",687]
[10,"Arm19","外间隔退出软压板",688]
[10,"Arm20","检无压软压板",689]
[10,"Arm21","检同期软压板",690]
[10,"Arm22","检合环软压板",691]
[10,"Arm23","投检修(B05X02)",692]
[10,"Arm24","解除闭锁(B05X03)",693]
[10,"Arm25","投远方(B05X04)",694]
[10,"Arm26","手合同期(B05X05)",695]
[10,"Arm27","手动分闸(B05X06)",696]
[10,"Arm28","保留1(B05X07)",697]
[10,"Arm29","保留2(B05X08)",698]
[10,"Arm30","保留3(B05X09)",699]
[10,"Arm31","保留4(B05X10)",700]
[10,"Arm32","保留5(B05X11)",701]
[10,"Arm33","保留6(B05X12)",702]
[10,"Arm34","保留7(B05X13)",703]
[10,"Arm35","保留8(B05X14)",704]
[10,"Arm36","保留9(B05X15)",705]
[10,"PosOff","存226断路器三相分位",706]
[10,"Arm38","存226断路器A相分位",707]
[10,"Arm39","存226断路器A相合位",708]
[10,"Arm40","存226断路器B相分位",709]
[10,"Arm41","存226断路器B相合位",710]
[10,"Arm42","存226断路器C相分位",711]
[10,"Arm43","存226断路器C相合位",712]
[10,"Arm44","存2261隔刀分位",713]
[10,"Arm45","存2262隔刀分位",714]
[10,"Arm46","存2266隔刀分位",715]
[10,"Arm47","存2265地刀分位",716]
[10,"Arm48","存2268地刀分位",717]
[10,"Arm49","存2269地刀分位",718]
[10,"Arm50","刀闸近控",719]
[10,"Arm51","断路器近控",720]
[10,"Arm52","联锁解除",721]
[10,"Arm53","断路器SF6闭锁",722]
[10,"Arm54","三相不一致",723]
[10,"Arm55","马达保护",724]
[10,"Arm56","断路器SF6泄露",725]
[10,"Arm57","弹簧储能超时",726]
[10,"Arm58","弹簧未储能",727]
[10,"Arm59","SF6气舱漏气",728]
[10,"Arm60","SF6气舱密度达到最小",729]
[10,"Arm61","交流电源断电",730]
[10,"Arm62","马达电源断电",731]
[10,"Arm63","直流电源断电",732]
[10,"Arm64","电压互感器空开跳闸",733]
[10,"Arm65","交流配电回路总空开跳闸",734]
[10,"Arm66","带电显示装置故障",735]
[10,"Arm67","带电显示装置线上无压",736]
[10,"Arm68","报警信号电源断电",737]
[10,"Arm69","直流配电回路总空开跳闸",738]
[10,"Arm70","开入55",739]
[10,"Arm71","开入56",740]
[10,"Arm72","开入57",741]
[10,"Arm73","第一套保护动作",742]
[10,"Arm74","第一套保护过负荷报警",743]
[10,"Arm75","第一套保护运行异常",744]
[10,"Arm76","第一套保护装置故障失电告警",745]
[10,"Arm77","第一套高压侧切换继电器同时动作",746]
[10,"Arm78","第一套高压侧切换继电器回路断线线或直流消失",747]
[10,"Arm79","第二套保护装置闭锁",748]
[10,"Arm80","第二套保护装置报警",749]
[10,"Arm81","第二套保护过负荷告警",750]
[10,"Arm82","第二套保护动作",751]
[10,"Arm83","第二套高压侧切换继电器同时消失",752]
[10,"Arm84","第二套高压侧切换继电器同时动作",753]
[10,"Arm85","第一组控制回路断线",754]
[10,"Arm86","第二组控制回路断线",755]
[10,"Arm87","第一组控制电源消失",756]
[10,"Arm88","第二组控制电源消失",757]
[10,"Arm89","第一组出口跳闸",758]
[10,"Arm90","第二组出口跳闸",759]
[10,"Arm91","KKJ",760]
[10,"Arm92","网络状态1",761]
[10,"Arm93","网络状态2",762]
[10,"Arm94","装置通讯状态",763]
[10,"Arm95","检修状态",764]
[10,"Arm96","参数变化",765]
[10,"Arm97","就地状态虚遥信",766]
[10,"Arm98","遥控解除闭锁",767]
[10,"Arm99","A网中断",768]
[10,"Arm100","B网中断",769]
[10,"Arm101","网络中断",770]
[13,"Arm1","装置闭锁",771]
[13,"Arm2","装置异常告警",772]
[13,"Arm3","装置自检异常",773]
[13,"Arm4","通信传动报警",774]
[13,"Arm5","开出传动报警",775]
[13,"Arm6","对时异常",776]
[13,"Arm7","对时信号状态",777]
[13,"Arm8","对时服务状态",778]
[13,"Arm9","时间跳变侦测状态",779]
[13,"Arm10","零序过压报警",780]
[13,"Arm11","PT断线报警",781]
[13,"Arm12","低电压报警",782]
[13,"Arm13","CT异常报警",783]
[13,"Arm14","双位置异常",784]
[13,"Arm15","事故总信号",785]
[13,"Arm16","三相档位不一致",786]
[13,"Arm17","滑档跳闸",787]
[13,"Arm18","出口使能软压板",788]
[13,"Arm19","外间隔退出软压板",789]
[13,"Arm20","检无压软压板",790]
[13,"Arm21","检同期软压板",791]
[13,"Arm22","检合环软压板",792]
[13,"Arm23","投检修(B05X02)",793]
[13,"Arm24","解除闭锁(B05X03)",794]
[13,"Arm25","投远方(B05X04)",795]
[13,"Arm26","手合同期(B05X05)",796]
[13,"Arm27","手动分闸(B05X06)",797]
[13,"Arm28","保留1(B05X07)",798]
[13,"Arm29","保留2(B05X08)",799]
[13,"Arm30","保留3(B05X09)",800]
[13,"Arm31","保留4(B05X10)",801]
[13,"Arm32","保留5(B05X11)",802]
[13,"Arm33","保留6(B05X12)",803]
[13,"Arm34","保留7(B05X13)",804]
[13,"Arm35","保留8(B05X14)",805]
[13,"Arm36","保留9(B05X15)",806]
[13,"PosOff","存230断路器三相分位",807]
[13,"Arm38","存230断路器A相分位",808]
[13,"Arm39","存230断路器A相合位",809]
[13,"Arm40","存230断路器B相分位",810]
[13,"Arm41","存230断路器B相合位",811]
[13,"Arm42","存230断路器C相分位",812]
[13,"Arm43","存230断路器C相合位",813]
[13,"Arm44","存2301隔刀分位",814]
[13,"Arm45","存2302隔刀分位",815]
[13,"Arm46","存2306隔刀分位",816]
[13,"Arm47","存2305地刀分位",817]
[13,"Arm48","存2308地刀分位",818]
[13,"Arm49","存2309地刀分位",819]
[13,"Arm50","刀闸近控",820]
[13,"Arm51","断路器近控",821]
[13,"Arm52","联锁解除",822]
[13,"Arm53","断路器SF6闭锁",823]
[13,"Arm54","三相不一致",824]
[13,"Arm55","马达保护",825]
[13,"Arm56","断路器SF6泄露",826]
[13,"Arm57","弹簧储能超时",827]
[13,"Arm58","弹簧未储能",828]
[13,"Arm59","SF6气舱漏气",829]
[13,"Arm60","SF6气舱密度达到最小",830]
[13,"Arm61","交流电源断电",831]
[13,"Arm62","马达电源断电",832]
[13,"Arm63","直流电源断电",833]
[13,"Arm64","电压互感器空开跳闸",834]
[13,"Arm65","交流配电回路总空开跳闸",835]
[13,"Arm66","带电显示装置故障",836]
[13,"Arm67","带电显示装置线上无压",837]
[13,"Arm68","报警信号电源断电",838]
[13,"Arm69","直流配电回路总空开跳闸",839]
[13,"Arm70","开入55",840]
[13,"Arm71","开入56",841]
[13,"Arm72","开入57",842]
[13,"Arm73","第一套保护动作",843]
[13,"Arm74","第一套保护过负荷报警",844]
[13,"Arm75","第一套保护运行异常",845]
[13,"Arm76","第一套保护装置故障失电告警",846]
[13,"Arm77","第一套高压侧切换继电器同时动作",847]
[13,"Arm78","第一套高压侧切换继电器回路断线线或直流消失",848]
[13,"Arm79","第二套保护装置闭锁",849]
[13,"Arm80","第二套保护装置报警",850]
[13,"Arm81","第二套保护过负荷告警",851]
[13,"Arm82","第二套保护动作",852]
[13,"Arm83","第二套高压侧切换继电器同时消失",853]
[13,"Arm84","第二套高压侧切换继电器同时动作",854]
[13,"Arm85","第一组控制回路断线",855]
[13,"Arm86","第二组控制回路断线",856]
[13,"Arm87","第一组控制电源消失",857]
[13,"Arm88","第二组控制电源消失",858]
[13,"Arm89","第一组出口跳闸",859]
[13,"Arm90","第二组出口跳闸",860]
[13,"Arm91","KKJ",861]
[13,"Arm92","网络状态1",862]
[13,"Arm93","网络状态2",863]
[13,"Arm94","装置通讯状态",864]
[13,"Arm95","检修状态",865]
[13,"Arm96","参数变化",866]
[13,"Arm97","就地状态虚遥信",867]
[13,"Arm98","遥控解除闭锁",868]
[13,"Arm99","A网中断",869]
[13,"Arm100","B网中断",870]
[13,"Arm101","网络中断",871]
[6,"Arm1","装置闭锁",872]
[6,"Arm2","装置异常告警",873]
[6,"Arm3","装置自检异常",874]
[6,"Arm4","通信传动报警",875]
[6,"Arm5","开出传动报警",876]
[6,"Arm6","对时异常",877]
[6,"Arm7","对时信号状态",878]
[6,"Arm8","对时服务状态",879]
[6,"Arm9","时间跳变侦测状态",880]
[6,"Arm10","电压控制器开关运行中",881]
[6,"Arm11","档位控制器调压信号",882]
[6,"Arm12","零序过压报警",883]
[6,"Arm13","PT断线报警",884]
[6,"Arm14","低电压报警",885]
[6,"Arm15","CT异常报警",886]
[6,"Arm16","双位置异常",887]
[6,"Arm17","事故总信号",888]
[6,"Arm18","三相档位不一致",889]
[6,"Arm19","滑档跳闸",890]
[6,"Arm20","出口使能软压板",891]
[6,"Arm21","外间隔退出软压板",892]
[6,"Arm22","检无压软压板",893]
[6,"Arm23","检同期软压板",894]
[6,"Arm24","检合环软压板",895]
[6,"Arm25","投检修(B05X02)",896]
[6,"Arm26","解除闭锁(B05X03)",897]
[6,"Arm27","投远方(B05X04)",898]
[6,"Arm28","手合同期(B05X05)",899]
[6,"Arm29","手动分闸(B05X06)",900]
[6,"Arm30","保留1(B05X07)",901]
[6,"Arm31","保留2(B05X08)",902]
[6,"Arm32","保留3(B05X09)",903]
[6,"Arm33","保留4(B05X10)",904]
[6,"Arm34","保留5(B05X11)",905]
[6,"Arm35","保留6(B05X12)",906]
[6,"Arm36","保留7(B05X13)",907]
[6,"Arm37","保留8(B05X14)",908]
[6,"Arm38","保留9(B05X15)",909]
[6,"Arm39","BCD1",910]
[6,"Arm40","BCD2",911]
[6,"Arm41","BCD4",912]
[6,"Arm42","BCD8",913]
[6,"Arm43","BCD10",914]
[6,"Arm44","电源断开报警",915]
[6,"Arm45","过流闭锁开关继电器动作",916]
[6,"Arm46","调压开关电机电源跳闸",917]
[6,"Arm47","调压开关就地控制",918]
[6,"Arm48","调压开关控制照明电源跳闸",919]
[6,"Arm49","分接开关未完成切换",920]
[6,"Arm50","2217中性点地刀分位",921]
[6,"Arm51","2217中性点地刀电源故障报警",922]
[6,"Arm52","2217中性点地刀就地操作",923]
[6,"Arm53","本体重瓦斯跳闸",924]
[6,"Arm54","调压重瓦斯跳闸",925]
[6,"Arm55","本体压力释放跳闸",926]
[6,"Arm56","调压压力释放",927]
[6,"Arm57","压力突变",928]
[6,"Arm58","油温高跳闸",929]
[6,"Arm59","绕组超温跳闸",930]
[6,"Arm60","本体轻瓦斯",931]
[6,"Arm61","调压轻瓦斯",932]
[6,"Arm62","本体油位异常",933]
[6,"Arm63","调压油位异常",934]
[6,"Arm64","油温高报警",935]
[6,"Arm65","绕组高报警",936]
[6,"Arm66","本体压力释放报警",937]
[6,"Arm67","装置异常告警_(重复1)",938]
[6,"Arm68","直流消失",939]
[6,"Arm69","KKJ",940]
[6,"Arm70","网络状态1",941]
[6,"Arm71","网络状态2",942]
[6,"Arm72","装置通讯状态",943]
[6,"Arm73","检修状态",944]
[6,"Arm74","参数变化",945]
[6,"Arm75","就地状态虚遥信",946]
[6,"Arm76","遥控解除闭锁",947]
[6,"Arm77","A网中断",948]
[6,"Arm78","B网中断",949]
[6,"Arm79","网络中断",950]
[9,"Arm1","装置闭锁",951]
[9,"Arm2","装置异常告警",952]
[9,"Arm3","装置自检异常",953]
[9,"Arm4","通信传动报警",954]
[9,"Arm5","开出传动报警",955]
[9,"Arm6","对时异常",956]
[9,"Arm7","对时信号状态",957]
[9,"Arm8","对时服务状态",958]
[9,"Arm9","时间跳变侦测状态",959]
[9,"Arm10","零序过压报警",960]
[9,"Arm11","PT断线报警",961]
[9,"Arm12","低电压报警",962]
[9,"Arm13","CT异常报警",963]
[9,"Arm14","双位置异常",964]
[9,"Arm15","事故总信号",965]
[9,"Arm16","三相档位不一致",966]
[9,"Arm17","滑档跳闸",967]
[9,"Arm18","出口使能软压板",968]
[9,"Arm19","外间隔退出软压板",969]
[9,"Arm20","检无压软压板",970]
[9,"Arm21","检同期软压板",971]
[9,"Arm22","检合环软压板",972]
[9,"Arm23","投检修(B05X02)",973]
[9,"Arm24","解除闭锁(B05X03)",974]
[9,"Arm25","投远方(B05X04)",975]
[9,"Arm26","手合同期(B05X05)",976]
[9,"Arm27","手动分闸(B05X06)",977]
[9,"Arm28","保留1(B05X07)",978]
[9,"Arm29","保留2(B05X08)",979]
[9,"Arm30","保留3(B05X09)",980]
[9,"Arm31","保留4(B05X10)",981]
[9,"Arm32","保留5(B05X11)",982]
[9,"Arm33","保留6(B05X12)",983]
[9,"Arm34","保留7(B05X13)",984]
[9,"Arm35","保留8(B05X14)",985]
[9,"Arm36","保留9(B05X15)",986]
[9,"Arm37","BCD1",987]
[9,"Arm38","BCD2",988]
[9,"Arm39","BCD4",989]
[9,"Arm40","BCD8",990]
[9,"Arm41","BCD10",991]
[9,"Arm42","电源断开报警",992]
[9,"Arm43","过流闭锁开关继电器动作",993]
[9,"Arm44","调压开关电机电源跳闸",994]
[9,"Arm45","调压开关就地控制",995]
[9,"Arm46","调压开关控制照明电源跳闸",996]
[9,"Arm47","分接开关未完成切换",997]
[9,"Arm48","2247中性点地刀分位",998]
[9,"Arm49","2247中性点地刀电源故障报警",999]
[9,"Arm50","2247中性点地刀就地操作",1000]
[9,"Arm51","本体重瓦斯跳闸",1001]
[9,"Arm52","调压重瓦斯跳闸",1002]
[9,"Arm53","本体压力释放跳闸",1003]
[9,"Arm54","调压压力释放",1004]
[9,"Arm55","压力突变",1005]
[9,"Arm56","油温高跳闸",1006]
[9,"Arm57","绕组超温跳闸",1007]
[9,"Arm58","本体轻瓦斯",1008]
[9,"Arm59","调压轻瓦斯",1009]
[9,"Arm60","本体油位异常",1010]
[9,"Arm61","调压油位异常",1011]
[9,"Arm62","油温高报警",1012]
[9,"Arm63","绕组高报警",1013]
[9,"Arm64","本体压力释放报警",1014]
[9,"Arm65","装置异常告警_(重复1)",1015]
[9,"Arm66","直流消失",1016]
[9,"Arm67","电压控制器开关运行中",1017]
[9,"Arm68","档位控制器调压信号",1018]
[9,"Arm69","KKJ",1019]
[9,"Arm70","网络状态1",1020]
[9,"Arm71","网络状态2",1021]
[9,"Arm72","装置通讯状态",1022]
[9,"Arm73","检修状态",1023]
[9,"Arm74","参数变化",1024]
[9,"Arm75","就地状态虚遥信",1025]
[9,"Arm76","遥控解除闭锁",1026]
[9,"Arm77","A网中断",1027]
[9,"Arm78","B网中断",1028]
[9,"Arm79","网络中断",1029]
[12,"Arm1","装置闭锁",1030]
[12,"Arm2","装置异常告警",1031]
[12,"Arm3","装置自检异常",1032]
[12,"Arm4","通信传动报警",1033]
[12,"Arm5","开出传动报警",1034]
[12,"Arm6","对时异常",1035]
[12,"Arm7","对时信号状态",1036]
[12,"Arm8","对时服务状态",1037]
[12,"Arm9","时间跳变侦测状态",1038]
[12,"Arm10","零序过压报警",1039]
[12,"Arm11","PT断线报警",1040]
[12,"Arm12","低电压报警",1041]
[12,"Arm13","CT异常报警",1042]
[12,"Arm14","双位置异常",1043]
[12,"Arm15","事故总信号",1044]
[12,"Arm16","三相档位不一致",1045]
[12,"Arm17","滑档跳闸",1046]
[12,"Arm18","出口使能软压板",1047]
[12,"Arm19","外间隔退出软压板",1048]
[12,"Arm20","检无压软压板",1049]
[12,"Arm21","检同期软压板",1050]
[12,"Arm22","检合环软压板",1051]
[12,"Arm23","投检修(B05X02)",1052]
[12,"Arm24","解除闭锁(B05X03)",1053]
[12,"Arm25","投远方(B05X04)",1054]
[12,"Arm26","手合同期(B05X05)",1055]
[12,"Arm27","手动分闸(B05X06)",1056]
[12,"Arm28","保留1(B05X07)",1057]
[12,"Arm29","保留2(B05X08)",1058]
[12,"Arm30","保留3(B05X09)",1059]
[12,"Arm31","保留4(B05X10)",1060]
[12,"Arm32","保留5(B05X11)",1061]
[12,"Arm33","保留6(B05X12)",1062]
[12,"Arm34","保留7(B05X13)",1063]
[12,"Arm35","保留8(B05X14)",1064]
[12,"Arm36","保留9(B05X15)",1065]
[12,"Arm37","BCD1",1066]
[12,"Arm38","BCD2",1067]
[12,"Arm39","BCD4",1068]
[12,"Arm40","BCD8",1069]
[12,"Arm41","BCD10",1070]
[12,"Arm42","电源断开报警",1071]
[12,"Arm43","过流闭锁开关继电器动作",1072]
[12,"Arm44","调压开关电机电源跳闸",1073]
[12,"Arm45","调压开关就地控制",1074]
[12,"Arm46","调压开关控制照明电源跳闸",1075]
[12,"Arm47","分接开关未完成切换",1076]
[12,"Arm48","2267中性点地刀分位",1077]
[12,"Arm49","2267中性点地刀电源故障报警",1078]
[12,"Arm50","2267中性点地刀就地操作",1079]
[12,"Arm51","本体重瓦斯跳闸",1080]
[12,"Arm52","调压重瓦斯跳闸",1081]
[12,"Arm53","本体压力释放跳闸",1082]
[12,"Arm54","调压压力释放",1083]
[12,"Arm55","压力突变",1084]
[12,"Arm56","油温高跳闸",1085]
[12,"Arm57","绕组超温跳闸",1086]
[12,"Arm58","本体轻瓦斯",1087]
[12,"Arm59","调压轻瓦斯",1088]
[12,"Arm60","本体油位异常",1089]
[12,"Arm61","调压油位异常",1090]
[12,"Arm62","油温高报警",1091]
[12,"Arm63","绕组高报警",1092]
[12,"Arm64","本体压力释放报警",1093]
[12,"Arm65","装置异常告警_(重复1)",1094]
[12,"Arm66","直流消失",1095]
[12,"Arm67","电压控制器开关运行中",1096]
[12,"Arm68","档位控制器调压信号",1097]
[12,"Arm69","KKJ",1098]
[12,"Arm70","网络状态1",1099]
[12,"Arm71","网络状态2",1100]
[12,"Arm72","装置通讯状态",1101]
[12,"Arm73","检修状态",1102]
[12,"Arm74","参数变化",1103]
[12,"Arm75","就地状态虚遥信",1104]
[12,"Arm76","遥控解除闭锁",1105]
[12,"Arm77","A网中断",1106]
[12,"Arm78","B网中断",1107]
[12,"Arm79","网络中断",1108]
[16,"Arm1","装置闭锁",1109]
[16,"Arm2","装置异常告警",1110]
[16,"Arm3","装置自检异常",1111]
[16,"Arm4","通信传动报警",1112]
[16,"Arm5","开出传动报警",1113]
[16,"Arm6","对时异常",1114]
[16,"Arm7","对时信号状态",1115]
[16,"Arm8","对时服务状态",1116]
[16,"Arm9","时间跳变侦测状态",1117]
[16,"Arm10","零序过压报警",1118]
[16,"Arm11","PT断线报警",1119]
[16,"Arm12","低电压报警",1120]
[16,"Arm13","CT异常报警",1121]
[16,"Arm14","双位置异常",1122]
[16,"Arm15","事故总信号",1123]
[16,"Arm16","三相档位不一致",1124]
[16,"Arm17","滑档跳闸",1125]
[16,"Arm18","出口使能软压板",1126]
[16,"Arm19","外间隔退出软压板",1127]
[16,"Arm20","检无压软压板",1128]
[16,"Arm21","检同期软压板",1129]
[16,"Arm22","检合环软压板",1130]
[16,"Arm23","投检修(B05X02)",1131]
[16,"Arm24","解除闭锁(B05X03)",1132]
[16,"Arm25","投远方(B05X04)",1133]
[16,"Arm26","手合同期(B05X05)",1134]
[16,"Arm27","手动分闸(B05X06)",1135]
[16,"Arm28","保留1(B05X07)",1136]
[16,"Arm29","保留2(B05X08)",1137]
[16,"Arm30","保留3(B05X09)",1138]
[16,"Arm31","保留4(B05X10)",1139]
[16,"Arm32","保留5(B05X11)",1140]
[16,"Arm33","保留6(B05X12)",1141]
[16,"Arm34","保留7(B05X13)",1142]
[16,"Arm35","保留8(B05X14)",1143]
[16,"Arm36","保留9(B05X15)",1144]
[16,"PosOff","存222断路器三相分位",1145]
[16,"Arm38","存222断路器A相分位",1146]
[16,"Arm39","存222断路器A相合位",1147]
[16,"Arm40","存222断路器B相分位",1148]
[16,"Arm41","存222断路器B相合位",1149]
[16,"Arm42","存222断路器C相分位",1150]
[16,"Arm43","存222断路器C相合位",1151]
[16,"Arm44","存2221隔刀分位",1152]
[16,"Arm45","存2222隔刀分位",1153]
[16,"Arm46","存2226隔刀分位",1154]
[16,"Arm47","存2225地刀分位",1155]
[16,"Arm48","存2228地刀分位",1156]
[16,"Arm49","存2229地刀分位",1157]
[16,"Arm50","刀闸近控",1158]
[16,"Arm51","断路器近控",1159]
[16,"Arm52","联锁解除",1160]
[16,"Arm53","断路器SF6闭锁",1161]
[16,"Arm54","三相不一致",1162]
[16,"Arm55","马达保护",1163]
[16,"Arm56","断路器SF6泄露",1164]
[16,"Arm57","弹簧储能超时",1165]
[16,"Arm58","弹簧未储能",1166]
[16,"Arm59","SF6气舱漏气",1167]
[16,"Arm60","SF6气舱密度达到最小",1168]
[16,"Arm61","交流电源断电",1169]
[16,"Arm62","马达电源断电",1170]
[16,"Arm63","直流电源断电",1171]
[16,"Arm64","电压互感器空开跳闸",1172]
[16,"Arm65","带电显示装置故障",1173]
[16,"Arm66","带电显示装置线上无压",1174]
[16,"Arm67","报警信号电源断电",1175]
[16,"Arm68","开入53",1176]
[16,"Arm69","开入54",1177]
[16,"Arm70","开入55",1178]
[16,"Arm71","第一套保护动作",1179]
[16,"Arm72","第一套保护重合闸",1180]
[16,"Arm73","第一套保护运行异常",1181]
[16,"Arm74","第一套保护电流过负荷报警",1182]
[16,"Arm75","第一套保护装置故障失电告警",1183]
[16,"Arm76","第一套保护装置通道一告警",1184]
[16,"Arm77","第一套保护装置通道二告警",1185]
[16,"Arm78","第一组控制回路断线",1186]
[16,"Arm79","第二组控制回路断线",1187]
[16,"Arm80","第一组控制电源消失",1188]
[16,"Arm81","第二组控制电源消失",1189]
[16,"Arm82","第一组出口跳闸",1190]
[16,"Arm83","第二组出口跳闸",1191]
[16,"Arm84","第一套保护重合闸_(重复1)",1192]
[16,"Arm85","压力低禁止重合闸",1193]
[16,"Arm86","第一套切换继电器同时动作",1194]
[16,"Arm87","第一套切换继电器回路断线线或直流消失",1195]
[16,"Arm88","第二套切换继电器同时动作",1196]
[16,"Arm89","第二套切换继电器失压",1197]
[16,"Arm90","第二套保护装置闭锁",1198]
[16,"Arm91","第二套保护装置异常",1199]
[16,"Arm92","第二套保护动作",1200]
[16,"Arm93","第二套保护重合闸",1201]
[16,"Arm94","第二套保护装置通道一告警",1202]
[16,"Arm95","第二套保护装置通道二告警",1203]
[16,"Arm96","第二套保护装置通道总告警",1204]
[16,"Arm97","电能质量在线监测装置失电",1205]
[16,"Arm98","KKJ",1206]
[16,"Arm99","网络状态1",1207]
[16,"Arm100","网络状态2",1208]
[16,"Arm101","装置通讯状态",1209]
[16,"Arm102","检修状态",1210]
[16,"Arm103","参数变化",1211]
[16,"Arm104","就地状态虚遥信",1212]
[16,"Arm105","遥控解除闭锁",1213]
[16,"Arm106","A网中断",1214]
[16,"Arm107","B网中断",1215]
[16,"Arm108","网络中断",1216]
[17,"Arm1","装置闭锁",1217]
[17,"Arm2","装置异常告警",1218]
[17,"Arm3","装置自检异常",1219]
[17,"Arm4","通信传动报警",1220]
[17,"Arm5","开出传动报警",1221]
[17,"Arm6","对时异常",1222]
[17,"Arm7","对时信号状态",1223]
[17,"Arm8","对时服务状态",1224]
[17,"Arm9","时间跳变侦测状态",1225]
[17,"Arm10","零序过压报警",1226]
[17,"Arm11","PT断线报警",1227]
[17,"Arm12","低电压报警",1228]
[17,"Arm13","CT异常报警",1229]
[17,"Arm14","双位置异常",1230]
[17,"Arm15","事故总信号",1231]
[17,"Arm16","三相档位不一致",1232]
[17,"Arm17","滑档跳闸",1233]
[17,"Arm18","出口使能软压板",1234]
[17,"Arm19","外间隔退出软压板",1235]
[17,"Arm20","检无压软压板",1236]
[17,"Arm21","检同期软压板",1237]
[17,"Arm22","检合环软压板",1238]
[17,"Arm23","投检修(B05X02)",1239]
[17,"Arm24","解除闭锁(B05X03)",1240]
[17,"Arm25","投远方(B05X04)",1241]
[17,"Arm26","手合同期(B05X05)",1242]
[17,"Arm27","手动分闸(B05X06)",1243]
[17,"Arm28","保留1(B05X07)",1244]
[17,"Arm29","保留2(B05X08)",1245]
[17,"Arm30","保留3(B05X09)",1246]
[17,"Arm31","保留4(B05X10)",1247]
[17,"Arm32","保留5(B05X11)",1248]
[17,"Arm33","保留6(B05X12)",1249]
[17,"Arm34","保留7(B05X13)",1250]
[17,"Arm35","保留8(B05X14)",1251]
[17,"Arm36","保留9(B05X15)",1252]
[17,"PosOff","存229断路器三相分位",1253]
[17,"Arm38","存229断路器A相分位",1254]
[17,"Arm39","存229断路器A相合位",1255]
[17,"Arm40","存229断路器B相分位",1256]
[17,"Arm41","存229断路器B相合位",1257]
[17,"Arm42","存229断路器C相分位",1258]
[17,"Arm43","存229断路器C相合位",1259]
[17,"Arm44","存2291隔刀分位",1260]
[17,"Arm45","存2292隔刀分位",1261]
[17,"Arm46","存2296隔刀分位",1262]
[17,"Arm47","存2295地刀分位",1263]
[17,"Arm48","存2298地刀分位",1264]
[17,"Arm49","存2299地刀分位",1265]
[17,"Arm50","刀闸近控",1266]
[17,"Arm51","断路器近控",1267]
[17,"Arm52","联锁解除",1268]
[17,"Arm53","断路器SF6闭锁",1269]
[17,"Arm54","三相不一致",1270]
[17,"Arm55","马达保护",1271]
[17,"Arm56","断路器SF6泄露",1272]
[17,"Arm57","弹簧储能超时",1273]
[17,"Arm58","弹簧未储能",1274]
[17,"Arm59","SF6气舱漏气",1275]
[17,"Arm60","SF6气舱密度达到最小",1276]
[17,"Arm61","交流电源断电",1277]
[17,"Arm62","马达电源断电",1278]
[17,"Arm63","直流电源断电",1279]
[17,"Arm64","电压互感器空开跳闸",1280]
[17,"Arm65","带电显示装置故障",1281]
[17,"Arm66","带电显示装置线上无压",1282]
[17,"Arm67","报警信号电源断电",1283]
[17,"Arm68","开入53",1284]
[17,"Arm69","开入54",1285]
[17,"Arm70","开入55",1286]
[17,"Arm71","第一套保护动作",1287]
[17,"Arm72","第一套保护重合闸",1288]
[17,"Arm73","第一套保护运行异常",1289]
[17,"Arm74","第一套保护电流过负荷报警",1290]
[17,"Arm75","第一套保护装置故障失电告警",1291]
[17,"Arm76","第一套保护装置通道一告警",1292]
[17,"Arm77","第一套保护装置通道二告警",1293]
[17,"Arm78","第一组控制回路断线",1294]
[17,"Arm79","第二组控制回路断线",1295]
[17,"Arm80","第一组控制电源消失",1296]
[17,"Arm81","第二组控制电源消失",1297]
[17,"Arm82","第一组出口跳闸",1298]
[17,"Arm83","第二组出口跳闸",1299]
[17,"Arm84","第一套保护重合闸_(重复1)",1300]
[17,"Arm85","压力低禁止重合闸",1301]
[17,"Arm86","第一套切换继电器同时动作",1302]
[17,"Arm87","第一套切换继电器回路断线线或直流消失",1303]
[17,"Arm88","第二套切换继电器同时动作",1304]
[17,"Arm89","第二套切换继电器失压",1305]
[17,"Arm90","第二套保护装置闭锁",1306]
[17,"Arm91","第二套保护装置异常",1307]
[17,"Arm92","第二套保护动作",1308]
[17,"Arm93","第二套保护重合闸",1309]
[17,"Arm94","第二套保护装置通道一告警",1310]
[17,"Arm95","第二套保护装置通道二告警",1311]
[17,"Arm96","第二套保护装置通道总告警",1312]
[17,"Arm97","电能质量在线监测装置失电",1313]
[17,"Arm98","KKJ",1314]
[17,"Arm99","网络状态1",1315]
[17,"Arm100","网络状态2",1316]
[17,"Arm101","装置通讯状态",1317]
[17,"Arm102","检修状态",1318]
[17,"Arm103","参数变化",1319]
[17,"Arm104","就地状态虚遥信",1320]
[17,"Arm105","遥控解除闭锁",1321]
[17,"Arm106","A网中断",1322]
[17,"Arm107","B网中断",1323]
[17,"Arm108","网络中断",1324]
[69,"Arm1","间隔1零序过压报警",1325]
[69,"Arm2","间隔1PT断线报警",1326]
[69,"Arm3","间隔1低电压报警",1327]
[69,"Arm4","间隔1CT异常报警",1328]
[69,"Arm5","间隔2零序过压报警",1329]
[69,"Arm6","间隔2PT断线报警",1330]
[69,"Arm7","间隔2低电压报警",1331]
[69,"Arm8","间隔2CT异常报警",1332]
[69,"Arm9","双位置异常",1333]
[69,"Arm10","事故总信号",1334]
[69,"Arm11","三相档位不一致",1335]
[69,"Arm12","滑档跳闸",1336]
[69,"Arm13","出口使能软压板",1337]
[69,"Arm14","间隔1检无压软压板",1338]
[69,"Arm15","间隔1检同期软压板",1339]
[69,"Arm16","间隔1检合环软压板",1340]
[69,"Arm17","间隔2检无压软压板",1341]
[69,"Arm18","间隔2检同期软压板",1342]
[69,"Arm19","间隔2检合环软压板",1343]
[69,"Arm20","外间隔退出软压板",1344]
[69,"Arm21","投检修(B05X02)",1345]
[69,"Arm22","解除闭锁(B05X03)",1346]
[69,"Arm23","投远方(B05X04)",1347]
[69,"Arm24","手合同期(B05X05)",1348]
[69,"Arm25","手动分闸(B05X06)",1349]
[69,"Arm26","手合同期2(B05X07)",1350]
[69,"Arm27","手动分闸2(B05X08)",1351]
[69,"Arm28","保留3(B05X09)",1352]
[69,"Arm29","保留4(B05X10)",1353]
[69,"Arm30","保留5(B05X11)",1354]
[69,"Arm31","保留6(B05X12)",1355]
[69,"Arm32","保留7(B05X13)",1356]
[69,"Arm33","保留8(B05X14)",1357]
[69,"Arm34","保留9(B05X15)",1358]
[69,"Arm35","网络安全隔离装置装置闭锁",1359]
[69,"Arm36","网络安全隔离装置装置告警",1360]
[69,"Arm37","Ⅰ区A套网关机装置闭锁",1361]
[69,"Arm38","Ⅰ区A套网关机装置告警",1362]
[69,"Arm39","Ⅰ区A套网关机电源1失电",1363]
[69,"Arm40","Ⅰ区A套网关机电源2失电",1364]
[69,"Arm41","Ⅰ区B套网关机装置闭锁",1365]
[69,"Arm42","Ⅰ区B套网关机装置告警",1366]
[69,"Arm43","Ⅰ区B套网关机电源1失电",1367]
[69,"Arm44","Ⅰ区B套网关机电源2失电",1368]
[69,"Arm45","Ⅰ区网关机禁止调度远控",1369]
[69,"Arm46","Ⅰ区A套网关机维护",1370]
[69,"Arm47","Ⅰ区B套网关机维护",1371]
[69,"Arm48","Ⅰ区网关机事故总",1372]
[69,"Arm49","Ⅰ区网关机预告总",1373]
[69,"Arm50","Ⅰ区规转装置闭锁",1374]
[69,"Arm51","Ⅰ区规转装置告警",1375]
[69,"Arm52","Ⅰ区A套交换机失电告警",1376]
[69,"Arm53","Ⅰ区B套交换机失电告警",1377]
[69,"Arm54","Ⅰ区柜A套防火墙电源1失电告警",1378]
[69,"Arm55","Ⅰ区柜A套防火墙电源2失电告警",1379]
[69,"Arm56","Ⅰ区柜A套防火墙装置闭锁",1380]
[69,"Arm57","Ⅰ区柜A套防火墙装置告警",1381]
[69,"Arm58","Ⅰ区柜B套防火墙电源1失电告警",1382]
[69,"Arm59","Ⅰ区柜B套防火墙电源2失电告警",1383]
[69,"Arm60","Ⅰ区柜B套防火墙装置闭锁",1384]
[69,"Arm61","Ⅰ区柜B套防火墙装置告警",1385]
[69,"Arm62","Ⅱ区A套网关机装置闭锁",1386]
[69,"Arm63","Ⅱ区A套网关机装置告警",1387]
[69,"Arm64","Ⅱ区A套网关机电源1失电",1388]
[69,"Arm65","Ⅱ区A套网关机电源2失电",1389]
[69,"Arm66","Ⅱ区B套网关机装置闭锁",1390]
[69,"Arm67","Ⅱ区B套网关机装置告警",1391]
[69,"Arm68","Ⅱ区B套网关机电源1失电",1392]
[69,"Arm69","Ⅱ区B套网关机电源2失电",1393]
[69,"Arm70","Ⅱ区A套网关机维护",1394]
[69,"Arm71","Ⅱ区B套网关机维护",1395]
[69,"Arm72","Ⅱ区网关机事故总",1396]
[69,"Arm73","Ⅱ区网关机预告总",1397]
[69,"Arm74","Ⅱ区规转装置闭锁",1398]
[69,"Arm75","Ⅱ区规转装置告警",1399]
[69,"Arm76","Ⅱ区A套交换机失电告警",1400]
[69,"Arm77","Ⅱ区B套交换机失电告警",1401]
[69,"Arm78","间隔层交换机1失电告警",1402]
[69,"Arm79","间隔层交换机2失电告警",1403]
[69,"Arm80","间隔层交换机3失电告警",1404]
[69,"Arm81","间隔层交换机4失电告警",1405]
[69,"Arm82","间隔层交换机5失电告警",1406]
[69,"Arm83","Ⅱ母电压隔离信号",1407]
[69,"Arm84","220kV母线测控1装置闭锁",1408]
[69,"Arm85","220kV母线测控1装置报警",1409]
[69,"Arm86","220kV母线测控1遥控信号",1410]
[69,"Arm87","220kV母线测控2装置报警",1411]
[69,"Arm88","220kV母线测控2装置闭锁",1412]
[69,"Arm89","220kV母线测控2遥控信号",1413]
[69,"Arm90","电压并列直流消失",1414]
[69,"Arm91","电压并列信号",1415]
[69,"Arm92","Ⅰ母电压隔离信号",1416]
[69,"Arm93","Ⅱ母电压隔离信号",1417]
[69,"Arm94","切换开关远控位置",1418]
[69,"Arm95","Ⅰ母保护1电压消失",1419]
[69,"Arm96","Ⅰ母计量电压消失",1420]
[69,"Arm97","Ⅰ母保护2电压消失",1421]
[69,"Arm98","Ⅱ母保护1电压消失",1422]
[69,"Arm99","Ⅱ母计量电压消失",1423]
[69,"Arm100","Ⅱ母保护2电压消失",1424]
[69,"Arm101","保信子站交换机失电告警",1425]
[69,"Arm102","保信子站装置闭锁",1426]
[69,"Arm103","保信子站装置告警",1427]
[69,"Arm104","对时柜1n装置失电异常报警",1428]
[69,"Arm105","对时柜1n装置异常报警",1429]
[69,"Arm106","对时柜1n装置失步报警",1430]
[69,"Arm107","对时柜2n装置失电异常报警",1431]
[69,"Arm108","对时柜2n装置异常报警",1432]
[69,"Arm109","对时柜2n装置失步报警",1433]
[69,"Arm110","220kV线路电度表柜PT失压",1434]
[69,"Arm111","220kV线路电度表柜切换继电器同时动作",1435]
[69,"Arm112","220kV线路电度表柜PT失压_(重复1)",1436]
[69,"Arm113","220kV线路电度表柜切换继电器同时动作_(重复1)",1437]
[69,"Arm114","220kV线路故录装置闭锁",1438]
[69,"Arm115","220kV线路故录装置异常",1439]
[69,"Arm116","220kV线路故录录波启动",1440]
[69,"Arm117","主变故录1装置闭锁",1441]
[69,"Arm118","主变故录1装置异常",1442]
[69,"Arm119","主变故录1录波启动",1443]
[69,"Arm120","主变故录2装置闭锁",1444]
[69,"Arm121","主变故录2装置异常",1445]
[69,"Arm122","主变故录2录波启动",1446]
[69,"Arm123","1#交流进线柜1QF断路器分闸位置",1447]
[69,"Arm124","1#交流进线柜1QF断路器故障位置",1448]
[69,"Arm125","2#交流进线柜2QF断路器分闸位置",1449]
[69,"Arm126","2#交流进线柜2QF断路器故障位置",1450]
[69,"Arm127","交流联络柜3QF断路器分闸位置",1451]
[69,"Arm128","交流联络柜3QF断路器故障位置",1452]
[69,"Arm129","交流联络柜4QF断路器分闸位置",1453]
[69,"Arm130","交流联络柜4QF断路器故障位置",1454]
[69,"Arm131","#1直流监控故障",1455]
[69,"Arm132","#1充电模块故障",1456]
[69,"Arm133","#1直流母线异常",1457]
[69,"Arm134","#1充电机交流进线异常",1458]
[69,"Arm135","#2直流监控故障",1459]
[69,"Arm136","#2充电模块故障",1460]
[69,"Arm137","#2直流母线异常",1461]
[69,"Arm138","#2充电机交流进线异常",1462]
[69,"Arm139","KKJ",1463]
[69,"Arm140","网络状态1",1464]
[69,"Arm141","网络状态2",1465]
[69,"Arm142","装置通讯状态",1466]
[69,"Arm143","检修状态",1467]
[69,"Arm144","参数变化",1468]
[69,"Arm145","就地状态虚遥信",1469]
[69,"Arm146","遥控解除闭锁",1470]
[69,"Arm147","A网中断",1471]
[69,"Arm148","B网中断",1472]
[69,"Arm149","网络中断",1473]
[70,"Arm1","装置闭锁",1474]
[70,"Arm2","装置异常告警",1475]
[70,"Arm3","装置自检异常",1476]
[70,"Arm4","通信传动报警",1477]
[70,"Arm5","开出传动报警",1478]
[70,"Arm6","对时异常",1479]
[70,"Arm7","对时信号状态",1480]
[70,"Arm8","对时服务状态",1481]
[70,"Arm9","时间跳变侦测状态",1482]
[70,"Arm10","间隔1零序过压报警",1483]
[70,"Arm11","间隔1PT断线报警",1484]
[70,"Arm12","间隔1低电压报警",1485]
[70,"Arm13","间隔1CT异常报警",1486]
[70,"Arm14","间隔2零序过压报警",1487]
[70,"Arm15","间隔2PT断线报警",1488]
[70,"Arm16","间隔2低电压报警",1489]
[70,"Arm17","间隔2CT异常报警",1490]
[70,"Arm18","双位置异常",1491]
[70,"Arm19","事故总信号",1492]
[70,"Arm20","三相档位不一致",1493]
[70,"Arm21","滑档跳闸",1494]
[70,"Arm22","出口使能软压板",1495]
[70,"Arm23","间隔1检无压软压板",1496]
[70,"Arm24","间隔1检同期软压板",1497]
[70,"Arm25","间隔1检合环软压板",1498]
[70,"Arm26","间隔2检无压软压板",1499]
[70,"Arm27","间隔2检同期软压板",1500]
[70,"Arm28","间隔2检合环软压板",1501]
[70,"Arm29","外间隔退出软压板",1502]
[70,"Arm30","投检修(B05X02)",1503]
[70,"Arm31","解除闭锁(B05X03)",1504]
[70,"Arm32","投远方(B05X04)",1505]
[70,"Arm33","手合同期(B05X05)",1506]
[70,"Arm34","手动分闸(B05X06)",1507]
[70,"Arm35","手合同期2(B05X07)",1508]
[70,"Arm36","手动分闸2(B05X08)",1509]
[70,"Arm37","保留3(B05X09)",1510]
[70,"Arm38","保留4(B05X10)",1511]
[70,"Arm39","保留5(B05X11)",1512]
[70,"Arm40","保留6(B05X12)",1513]
[70,"Arm41","保留7(B05X13)",1514]
[70,"Arm42","保留8(B05X14)",1515]
[70,"Arm43","保留9(B05X15)",1516]
[70,"Arm44","16装置闭锁",1517]
[70,"Arm45","16装置报警",1518]
[70,"Arm46","16遥控信号",1519]
[70,"Arm47","17装置闭锁",1520]
[70,"Arm48","17装置报警",1521]
[70,"Arm49","17遥控信号",1522]
[70,"Arm50","3装置闭锁",1523]
[70,"Arm51","3装置报警",1524]
[70,"Arm52","3遥控信号",1525]
[70,"Arm53","220kV1#主变高压侧测控装置闭锁",1526]
[70,"Arm54","220kV1#主变高压侧测控装置报警",1527]
[70,"Arm55","220kV1#主变高压侧测控遥控信号",1528]
[70,"Arm56","220kV1#主变低压侧测控装置闭锁",1529]
[70,"Arm57","220kV1#主变低压侧测控装置报警",1530]
[70,"Arm58","220kV1#主变低压侧测控遥控信号",1531]
[70,"Arm59","220kV1#主变本体侧测控装置闭锁",1532]
[70,"Arm60","220kV1#主变本体侧测控装置报警",1533]
[70,"Arm61","220kV1#主变本体侧测控遥控信号",1534]
[70,"Arm62","220kV2#主变高压侧测控装置闭锁",1535]
[70,"Arm63","220kV2#主变高压侧测控装置报警",1536]
[70,"Arm64","220kV2#主变高压侧测控遥控信号",1537]
[70,"Arm65","220kV2#主变低压侧测控装置闭锁",1538]
[70,"Arm66","220kV2#主变低压侧测控装置报警",1539]
[70,"Arm67","220kV2#主变低压侧测控遥控信号",1540]
[70,"Arm68","220kV2#主变本体侧测控装置闭锁",1541]
[70,"Arm69","220kV2#主变本体侧测控装置报警",1542]
[70,"Arm70","220kV2#主变本体侧测控遥控信号",1543]
[70,"Arm71","220kV3#主变高压侧测控装置闭锁",1544]
[70,"Arm72","220kV3#主变高压侧测控装置报警",1545]
[70,"Arm73","220kV3#主变高压侧测控遥控信号",1546]
[70,"Arm74","220kV3#主变低压侧测控装置闭锁",1547]
[70,"Arm75","220kV3#主变低压侧测控装置报警",1548]
[70,"Arm76","220kV3#主变低压侧测控遥控信号",1549]
[70,"Arm77","220kV3#主变本体侧测控装置闭锁",1550]
[70,"Arm78","220kV3#主变本体侧测控装置报警",1551]
[70,"Arm79","220kV3#主变本体侧测控遥控信号",1552]
[70,"Arm80","220kV4#主变高压侧测控装置闭锁",1553]
[70,"Arm81","220kV4#主变高压侧测控装置报警",1554]
[70,"Arm82","220kV4#主变高压侧测控遥控信号",1555]
[70,"Arm83","220kV4#主变低压侧测控装置闭锁",1556]
[70,"Arm84","220kV4#主变低压侧测控装置报警",1557]
[70,"Arm85","220kV4#主变低压侧测控遥控信号",1558]
[70,"Arm86","220kV4#主变本体侧测控装置闭锁",1559]
[70,"Arm87","220kV4#主变本体侧测控装置报警",1560]
[70,"Arm88","220kV4#主变本体侧测控遥控信号",1561]
[70,"Arm89","220kV母线保护一Ⅰ母差动动作",1562]
[70,"Arm90","220kV母线保护一Ⅱ母差动动作",1563]
[70,"Arm91","220kV母线保护一Ⅰ母失灵动作",1564]
[70,"Arm92","220kV母线保护一Ⅱ母失灵动作",1565]
[70,"Arm93","220kV母线保护一母联(分段)出口",1566]
[70,"Arm94","220kV母线保护一母线互联告警",1567]
[70,"Arm95","220kV母线保护一CT或PT断线告警",1568]
[70,"Arm96","220kV母线保护一刀闸位置告警",1569]
[70,"Arm97","220kV母线保护一运行异常告警",1570]
[70,"Arm98","220kV母线保护一装置故障告警",1571]
[70,"Arm99","220kV母线保护一直流消失",1572]
[70,"Arm100","220kV母线保护二装置闭锁",1573]
[70,"Arm101","220kV母线保护二装置异常",1574]
[70,"Arm102","220kV母线保护二交流断线报警",1575]
[70,"Arm103","221kV母线保护二刀闸位置报警",1576]
[70,"Arm104","222kV母线保护二母线互联报警",1577]
[70,"Arm105","220kV母线保护二母差跳Ⅰ母",1578]
[70,"Arm106","220kV母线保护二母差跳Ⅱ母",1579]
[70,"Arm107","220kV母线保护二失灵跳Ⅰ母",1580]
[70,"Arm108","220kV母线保护二失灵跳Ⅱ母",1581]
[70,"Arm109","220kV母线保护二失灵跳母联",1582]
[70,"Arm110","火灾报警动作",1583]
[70,"Arm111","火灾报警故障",1584]
[70,"Arm112","红外对射1报警信号",1585]
[70,"Arm113","红外对射2报警信号",1586]
[70,"Arm114","红外双鉴探测器报警信号",1587]
[70,"Arm115","KKJ",1588]
[70,"Arm116","网络状态1",1589]
[70,"Arm117","网络状态2",1590]
[70,"Arm118","装置通讯状态",1591]
[70,"Arm119","检修状态",1592]
[70,"Arm120","参数变化",1593]
[70,"Arm121","就地状态虚遥信",1594]
[70,"Arm122","遥控解除闭锁",1595]
[70,"Arm123","A网中断",1596]
[70,"Arm124","B网中断",1597]
[70,"Arm125","网络中断",1598]
[71,"Arm1","I类告警总",1599]
[71,"Arm2","设备参数错",1600]
[71,"Arm3","ROM和校验错",1601]
[71,"Arm4","定值错",1602]
[71,"Arm5","定值区指针错",1603]
[71,"Arm6","开出异常",1604]
[71,"Arm7","保护CPU插件异常",1605]
[71,"Arm8","软压板错",1606]
[71,"Arm9","系统配置错",1607]
[71,"Arm10","开出配置错",1608]
[71,"Arm11","压板模式未确认",1609]
[71,"Arm12","开出EEPROM出错",1610]
[71,"Arm13","前置CPU ROM 和错",1611]
[71,"Arm14","采样数据异常",1612]
[71,"Arm15","模拟量采集错",1613]
[71,"Arm16","从机中断",1614]
[71,"Arm17","采样异常告警",1615]
[71,"Arm18","CPU通讯中断",1616]
[71,"Arm19","设备参数不一致",1617]
[71,"Arm20","定值区号不一致",1618]
[71,"Arm21","定值不一致",1619]
[71,"Arm22","压板不一致",1620]
[71,"Arm23","压板模式不一致",1621]
[71,"Arm24","召唤配置无应答",1622]
[71,"Arm25","对时异常",1623]
[71,"Arm26","对时信号状态异常",1624]
[71,"Arm27","对时服务状态异常",1625]
[71,"Arm28","时间跳变侦测状态异常",1626]
[71,"Arm29","差动保护硬压板",1627]
[71,"Arm30","失灵保护硬压板",1628]
[71,"Arm31","母线互联硬压板",1629]
[71,"Arm32","远方操作硬压板",1630]
[71,"Arm33","保护检修状态硬压板",1631]
[71,"Arm34","差动保护总压板",1632]
[71,"Arm35","失灵保护总压板",1633]
[71,"Arm36","母线互联总压板",1634]
[71,"Arm37","运行",1635]
[71,"Arm38","异常",1636]
[71,"Arm39","检修",1637]
[71,"Arm40","差动保护闭锁",1638]
[71,"Arm41","母线互联",1639]
[71,"Arm42","刀闸告警",1640]
[71,"Arm43","保护跳闸",1641]
[71,"Arm44","Ⅰ母差动A相有效",1642]
[71,"Arm45","Ⅰ母差动B相有效",1643]
[71,"Arm46","Ⅰ母差动C相有效",1644]
[71,"Arm47","Ⅱ母差动A相有效",1645]
[71,"Arm48","Ⅱ母差动B相有效",1646]
[71,"Arm49","Ⅱ母差动C相有效",1647]
[71,"Arm50","母联失灵有效",1648]
[71,"Arm51","分段1失灵有效",1649]
[71,"Arm52","分段2失灵有效",1650]
[71,"Arm53","主变1失灵有效",1651]
[71,"Arm54","主变2失灵有效",1652]
[71,"Arm55","支路4_失灵有效",1653]
[71,"Arm56","支路5_失灵有效",1654]
[71,"Arm57","支路6_失灵有效",1655]
[71,"Arm58","支路7_失灵有效",1656]
[71,"Arm59","支路8_失灵有效",1657]
[71,"Arm60","支路9_失灵有效",1658]
[71,"Arm61","支路10_失灵有效",1659]
[71,"Arm62","支路11_失灵有效",1660]
[71,"Arm63","支路12_失灵有效",1661]
[71,"Arm64","支路13_失灵有效",1662]
[71,"Arm65","主变3失灵有效",1663]
[71,"Arm66","主变4失灵有效",1664]
[71,"Arm67","支路16_失灵有效",1665]
[71,"Arm68","支路17_失灵有效",1666]
[71,"Arm69","支路18_失灵有效",1667]
[71,"Arm70","支路19_失灵有效",1668]
[71,"Arm71","支路20_失灵有效",1669]
[71,"Arm72","支路21_失灵有效",1670]
[71,"Arm73","支路22_失灵有效",1671]
[71,"Arm74","闭锁差动保护",1672]
[71,"Arm75","闭锁后备保护",1673]
[71,"Arm76","闭锁失灵保护",1674]
[71,"Arm77","差动保护投入",1675]
[71,"Arm78","失灵保护投入",1676]
[71,"Arm79","录波完成",1677]
[71,"Arm80","录波启动",1678]
[71,"Arm81","差动保护软压板",1679]
[71,"Arm82","失灵保护软压板",1680]
[71,"Arm83","母线互联软压板",1681]
[71,"Arm84","母联分列软压板",1682]
[71,"Arm85","分段1分列软压板",1683]
[71,"Arm86","分段2分列软压板",1684]
[71,"Arm87","远方投退压板软压板",1685]
[71,"Arm88","远方切换定值区软压板",1686]
[71,"Arm89","远方修改定值软压板",1687]
[71,"Arm90","信号复归",1688]
[71,"Arm91","母联TWJ",1689]
[71,"Arm92","分段1TWJ",1690]
[71,"Arm93","分段2TWJ",1691]
[71,"Arm94","备用",1692]
[71,"Arm95","备用_(重复1)",1693]
[71,"Arm96","备用_(重复2)",1694]
[71,"Arm97","母联SHJ",1695]
[71,"Arm98","分段1SHJ",1696]
[71,"Arm99","分段2SHJ",1697]
[71,"Arm100","母联_三相启动失灵开入",1698]
[71,"Arm101","分段1_三相启动失灵开入",1699]
[71,"Arm102","分段2_三相启动失灵开入",1700]
[71,"Arm103","母联带路运行",1701]
[71,"Arm104","Ⅰ母带旁路",1702]
[71,"Arm105","Ⅱ母带旁路",1703]
[71,"Arm106","支路1_1G刀闸位置",1704]
[71,"Arm107","支路1_2G刀闸位置",1705]
[71,"Arm108","支路23_1G刀闸位置",1706]
[71,"Arm109","支路24_2G刀闸位置",1707]
[71,"Arm110","主变1_1G刀闸位置",1708]
[71,"Arm111","主变1_2G刀闸位置",1709]
[71,"Arm112","主变2_1G刀闸位置",1710]
[71,"Arm113","主变2_2G刀闸位置",1711]
[71,"Arm114","支路4_1G刀闸位置",1712]
[71,"Arm115","支路4_2G刀闸位置",1713]
[71,"Arm116","支路5_1G刀闸位置",1714]
[71,"Arm117","支路5_2G刀闸位置",1715]
[71,"Arm118","支路6_1G刀闸位置",1716]
[71,"Arm119","支路6_2G刀闸位置",1717]
[71,"Arm120","支路7_1G刀闸位置",1718]
[71,"Arm121","支路7_2G刀闸位置",1719]
[71,"Arm122","支路8_1G刀闸位置",1720]
[71,"Arm123","支路8_2G刀闸位置",1721]
[71,"Arm124","支路9_1G刀闸位置",1722]
[71,"Arm125","支路9_2G刀闸位置",1723]
[71,"Arm126","支路10_1G刀闸位置",1724]
[71,"Arm127","支路10_2G刀闸位置",1725]
[71,"Arm128","支路11_1G刀闸位置",1726]
[71,"Arm129","支路11_2G刀闸位置",1727]
[71,"Arm130","支路12_1G刀闸位置",1728]
[71,"Arm131","支路12_2G刀闸位置",1729]
[71,"Arm132","支路13_1G刀闸位置",1730]
[71,"Arm133","支路13_2G刀闸位置",1731]
[71,"Arm134","主变3_1G刀闸位置",1732]
[71,"Arm135","主变3_2G刀闸位置",1733]
[71,"Arm136","主变4_1G刀闸位置",1734]
[71,"Arm137","主变4_2G刀闸位置",1735]
[71,"Arm138","支路16_1G刀闸位置",1736]
[71,"Arm139","支路16_2G刀闸位置",1737]
[71,"Arm140","支路17_1G刀闸位置",1738]
[71,"Arm141","支路17_2G刀闸位置",1739]
[71,"Arm142","支路18_1G刀闸位置",1740]
[71,"Arm143","支路18_2G刀闸位置",1741]
[71,"Arm144","支路19_1G刀闸位置",1742]
[71,"Arm145","支路19_2G刀闸位置",1743]
[71,"Arm146","支路20_1G刀闸位置",1744]
[71,"Arm147","支路20_2G刀闸位置",1745]
[71,"Arm148","支路21_1G刀闸位置",1746]
[71,"Arm149","支路21_2G刀闸位置",1747]
[71,"Arm150","支路22_1G刀闸位置",1748]
[71,"Arm151","支路22_2G刀闸位置",1749]
[71,"Arm152","支路1_A相启动失灵开入",1750]
[71,"Arm153","支路1_B相启动失灵开入",1751]
[71,"Arm154","支路1_C相启动失灵开入",1752]
[71,"Arm155","支路1_三相启动失灵开入",1753]
[71,"Arm156","主变1_A相启动失灵开入",1754]
[71,"Arm157","主变1_B相启动失灵开入",1755]
[71,"Arm158","主变1_C相启动失灵开入",1756]
[71,"Arm159","主变1_三相启动失灵开入",1757]
[71,"Arm160","主变2_A相启动失灵开入",1758]
[71,"Arm161","主变2_B相启动失灵开入",1759]
[71,"Arm162","主变2_C相启动失灵开入",1760]
[71,"Arm163","主变2_三相启动失灵开入",1761]
[71,"Arm164","支路4_A相启动失灵开入",1762]
[71,"Arm165","支路4_B相启动失灵开入",1763]
[71,"Arm166","支路4_C相启动失灵开入",1764]
[71,"Arm167","支路4_三相启动失灵开入",1765]
[71,"Arm168","支路5_A相启动失灵开入",1766]
[71,"Arm169","支路5_B相启动失灵开入",1767]
[71,"Arm170","支路5_C相启动失灵开入",1768]
[71,"Arm171","支路5_三相启动失灵开入",1769]
[71,"Arm172","支路6_A相启动失灵开入",1770]
[71,"Arm173","支路6_B相启动失灵开入",1771]
[71,"Arm174","支路6_C相启动失灵开入",1772]
[71,"Arm175","支路6_三相启动失灵开入",1773]
[71,"Arm176","支路7_A相启动失灵开入",1774]
[71,"Arm177","支路7_B相启动失灵开入",1775]
[71,"Arm178","支路7_C相启动失灵开入",1776]
[71,"Arm179","支路7_三相启动失灵开入",1777]
[71,"Arm180","支路8_A相启动失灵开入",1778]
[71,"Arm181","支路8_B相启动失灵开入",1779]
[71,"Arm182","支路8_C相启动失灵开入",1780]
[71,"Arm183","支路8_三相启动失灵开入",1781]
[71,"Arm184","支路9_A相启动失灵开入",1782]
[71,"Arm185","支路9_B相启动失灵开入",1783]
[71,"Arm186","支路9_C相启动失灵开入",1784]
[71,"Arm187","支路9_三相启动失灵开入",1785]
[71,"Arm188","支路10_A相启动失灵开入",1786]
[71,"Arm189","支路10_B相启动失灵开入",1787]
[71,"Arm190","支路10_C相启动失灵开入",1788]
[71,"Arm191","支路10_三相启动失灵开入",1789]
[71,"Arm192","支路11_A相启动失灵开入",1790]
[71,"Arm193","支路11_B相启动失灵开入",1791]
[71,"Arm194","支路11_C相启动失灵开入",1792]
[71,"Arm195","支路11_三相启动失灵开入",1793]
[71,"Arm196","支路12_A相启动失灵开入",1794]
[71,"Arm197","支路12_B相启动失灵开入",1795]
[71,"Arm198","支路12_C相启动失灵开入",1796]
[71,"Arm199","支路12_三相启动失灵开入",1797]
[71,"Arm200","支路13_A相启动失灵开入",1798]
[71,"Arm201","支路13_B相启动失灵开入",1799]
[71,"Arm202","支路13_C相启动失灵开入",1800]
[71,"Arm203","支路13_三相启动失灵开入",1801]
[71,"Arm204","主变3_A相启动失灵开入",1802]
[71,"Arm205","主变3_B相启动失灵开入",1803]
[71,"Arm206","主变3_C相启动失灵开入",1804]
[71,"Arm207","主变3_三相启动失灵开入",1805]
[71,"Arm208","主变4_A相启动失灵开入",1806]
[71,"Arm209","主变4_B相启动失灵开入",1807]
[71,"Arm210","主变4_C相启动失灵开入",1808]
[71,"Arm211","主变4_三相启动失灵开入",1809]
[71,"Arm212","支路16_A相启动失灵开入",1810]
[71,"Arm213","支路16_B相启动失灵开入",1811]
[71,"Arm214","支路16_C相启动失灵开入",1812]
[71,"Arm215","支路16_三相启动失灵开入",1813]
[71,"Arm216","支路17_A相启动失灵开入",1814]
[71,"Arm217","支路17_B相启动失灵开入",1815]
[71,"Arm218","支路17_C相启动失灵开入",1816]
[71,"Arm219","支路17_三相启动失灵开入",1817]
[71,"Arm220","支路18_A相启动失灵开入",1818]
[71,"Arm221","支路18_B相启动失灵开入",1819]
[71,"Arm222","支路18_C相启动失灵开入",1820]
[71,"Arm223","支路18_三相启动失灵开入",1821]
[71,"Arm224","支路19_A相启动失灵开入",1822]
[71,"Arm225","支路19_B相启动失灵开入",1823]
[71,"Arm226","支路19_C相启动失灵开入",1824]
[71,"Arm227","支路19_三相启动失灵开入",1825]
[71,"Arm228","支路20_A相启动失灵开入",1826]
[71,"Arm229","支路20_B相启动失灵开入",1827]
[71,"Arm230","支路20_C相启动失灵开入",1828]
[71,"Arm231","支路20_三相启动失灵开入",1829]
[71,"Arm232","支路21_A相启动失灵开入",1830]
[71,"Arm233","支路21_B相启动失灵开入",1831]
[71,"Arm234","支路21_C相启动失灵开入",1832]
[71,"Arm235","支路21_三相启动失灵开入",1833]
[71,"Arm236","支路22_A相启动失灵开入",1834]
[71,"Arm237","支路22_B相启动失灵开入",1835]
[71,"Arm238","支路22_C相启动失灵开入",1836]
[71,"Arm239","支路22_三相启动失灵开入",1837]
[71,"Arm240","支路23_A相启动失灵开入",1838]
[71,"Arm241","支路23_B相启动失灵开入",1839]
[71,"Arm242","支路23_C相启动失灵开入",1840]
[71,"Arm243","支路23_三相启动失灵开入",1841]
[71,"Arm244","支路24_A相启动失灵开入",1842]
[71,"Arm245","支路24_B相启动失灵开入",1843]
[71,"Arm246","支路24_C相启动失灵开入",1844]
[71,"Arm247","支路24_三相启动失灵开入",1845]
[71,"Arm248","主变1解闭锁开入",1846]
[71,"Arm249","主变2解闭锁开入",1847]
[71,"Arm250","主变3解闭锁开入",1848]
[71,"Arm251","主变4解闭锁开入",1849]
[71,"Arm252","备用_(重复3)",1850]
[71,"Arm253","保护动作",1851]
[71,"Arm254","差动保护启动",1852]
[71,"Arm255","Ⅱ母差动动作",1853]
[71,"Arm256","Ⅰ母差动跳母联",1854]
[71,"Arm257","Ⅱ母差动跳母联",1855]
[71,"Arm258","Ⅰ母差动跳分段1",1856]
[71,"Arm259","Ⅱ母差动跳分段2",1857]
[71,"Arm260","Ⅱ母差动跟跳",1858]
[71,"Arm261","Ⅰ母差动动作",1859]
[71,"Arm262","Ⅰ母差动跟跳",1860]
[71,"Arm263","母联失灵启动",1861]
[71,"Arm264","分段1失灵启动",1862]
[71,"Arm265","分段2失灵启动",1863]
[71,"Arm266","分段1失灵保护动作",1864]
[71,"Arm267","分段2失灵保护动作",1865]
[71,"Arm268","母联失灵保护动作",1866]
[71,"Arm269","失灵保护启动",1867]
[71,"Arm270","失灵保护跳母联",1868]
[71,"Arm271","失灵保护跳分段1",1869]
[71,"Arm272","失灵保护跳分段2",1870]
[71,"Arm273","Ⅱ母失灵保护动作",1871]
[71,"Arm274","变压器1失灵联跳",1872]
[71,"Arm275","变压器2失灵联跳",1873]
[71,"Arm276","变压器3失灵联跳",1874]
[71,"Arm277","变压器4失灵联跳",1875]
[71,"Arm278","Ⅰ母失灵保护动作",1876]
[71,"Arm279","II类告警总",1877]
[71,"Arm280","开入配置错",1878]
[71,"Arm281","开入通讯中断",1879]
[71,"Arm282","开出通讯中断",1880]
[71,"Arm283","传动状态未复归",1881]
[71,"Arm284","开入异常",1882]
[71,"Arm285","开入输入不正常",1883]
[71,"Arm286","双位置输入不一致",1884]
[71,"Arm287","开入自检回路出错",1885]
[71,"Arm288","开入EEPROM出错",1886]
[71,"Arm289","SRAM自检异常",1887]
[71,"Arm290","FLASH自检异常",1888]
[71,"Arm291","模拟通道异常",1889]
[71,"Arm292","工作于调试定值区",1890]
[71,"Arm293","失灵启动开入异常",1891]
[71,"Arm294","分段1失灵启动异常",1892]
[71,"Arm295","分段2失灵启动异常",1893]
[71,"Arm296","母联失灵启动异常",1894]
[71,"Arm297","无刀闸位置引入",1895]
[71,"Arm298","支路刀闸位置异常",1896]
[71,"Arm299","母线互联运行",1897]
[71,"Arm300","CT断线告警",1898]
[71,"Arm301","支路CT断线",1899]
[71,"Arm302","母联/分段CT断线",1900]
[71,"Arm303","Ⅰ母PT断线",1901]
[71,"Arm304","Ⅱ母PT断线",1902]
[71,"Arm305","Ⅰ母差动电压开放",1903]
[71,"Arm306","Ⅱ母差动电压开放",1904]
[71,"Arm307","Ⅰ母失灵电压开放",1905]
[71,"Arm308","Ⅱ母失灵电压开放",1906]
[71,"Arm309","解除Ⅰ母电压闭锁",1907]
[71,"Arm310","解除Ⅱ母电压闭锁",1908]
[71,"Arm311","母联死区故障",1909]
[71,"Arm312","保护处于检修状态",1910]
[71,"Arm313","主变1解闭锁开入异常",1911]
[71,"Arm314","主变2解闭锁开入异常",1912]
[71,"Arm315","主变3解闭锁开入异常",1913]
[71,"Arm316","主变4解闭锁开入异常",1914]
[71,"Arm317","母联跳位异常",1915]
[71,"Arm318","分段1跳位异常",1916]
[71,"Arm319","分段2跳位异常",1917]
[71,"Arm320","母联手合开入异常",1918]
[71,"Arm321","分段1手合开入异常",1919]
[71,"Arm322","分段2手合开入异常",1920]
[71,"Arm323","网络状态1",1921]
[71,"Arm324","网络状态2",1922]
[71,"Arm325","装置通讯状态",1923]
[71,"Arm326","检修状态",1924]
[71,"Arm327","参数变化",1925]
[71,"Arm328","就地状态虚遥信",1926]
[71,"Arm329","遥控解除闭锁",1927]
[71,"Arm330","A网中断",1928]
[71,"Arm331","B网中断",1929]
[71,"Arm332","网络中断",1930]
[72,"Arm1","板卡配置错误",1931]
[72,"Arm2","定值项变化告警",1932]
[72,"Arm3","装置闭锁",1933]
[72,"Arm4","板卡运行异常",1934]
[72,"Arm5","12号板出口回路异常",1935]
[72,"Arm6","13号板出口回路异常",1936]
[72,"Arm7","14号板出口回路异常",1937]
[72,"Arm8","15号板出口回路异常",1938]
[72,"Arm9","30号板出口回路异常",1939]
[72,"Arm10","31号板出口回路异常",1940]
[72,"Arm11","32号板出口回路异常",1941]
[72,"Arm12","4号板板卡异常",1942]
[72,"Arm13","5号板板卡异常",1943]
[72,"Arm14","6号板板卡异常",1944]
[72,"Arm15","7号板板卡异常",1945]
[72,"Arm16","8号板板卡异常",1946]
[72,"Arm17","9号板板卡异常",1947]
[72,"Arm18","10号板板卡异常",1948]
[72,"Arm19","11号板板卡异常",1949]
[72,"Arm20","12号板板卡异常",1950]
[72,"Arm21","13号板板卡异常",1951]
[72,"Arm22","14号板板卡异常",1952]
[72,"Arm23","15号板板卡异常",1953]
[72,"Arm24","30号板板卡异常",1954]
[72,"Arm25","31号板板卡异常",1955]
[72,"Arm26","32号板板卡异常",1956]
[72,"Arm27","2号板定值校验出错",1957]
[72,"Arm28","3号板定值校验出错",1958]
[72,"Arm29","2号板DSP出错",1959]
[72,"Arm30","3号板DSP出错",1960]
[72,"Arm31","母联采样校验出错",1961]
[72,"Arm32","主变1采样校验出错",1962]
[72,"Arm33","主变2采样校验出错",1963]
[72,"Arm34","支路4采样校验出错",1964]
[72,"Arm35","支路5采样校验出错",1965]
[72,"Arm36","支路6采样校验出错",1966]
[72,"Arm37","支路7采样校验出错",1967]
[72,"Arm38","支路8采样校验出错",1968]
[72,"Arm39","支路9采样校验出错",1969]
[72,"Arm40","支路10采样校验出错",1970]
[72,"Arm41","支路11采样校验出错",1971]
[72,"Arm42","支路12采样校验出错",1972]
[72,"Arm43","支路13采样校验出错",1973]
[72,"Arm44","主变3采样校验出错",1974]
[72,"Arm45","主变4采样校验出错",1975]
[72,"Arm46","支路16采样校验出错",1976]
[72,"Arm47","支路17采样校验出错",1977]
[72,"Arm48","支路18采样校验出错",1978]
[72,"Arm49","支路19采样校验出错",1979]
[72,"Arm50","支路20采样校验出错",1980]
[72,"Arm51","支路21采样校验出错",1981]
[72,"Arm52","支路22采样校验出错",1982]
[72,"Arm53","分段1采样校验出错",1983]
[72,"Arm54","分段2采样校验出错",1984]
[72,"Arm55","CCD文件错误",1985]
[72,"Arm56","CID文件错误",1986]
[72,"Arm57","版本错误报警",1987]
[72,"Arm58","定值校验出错",1988]
[72,"Arm59","定值修改",1989]
[72,"Arm60","定值区切换",1990]
[72,"Arm61","装置报警",1991]
[72,"Arm62","通信传动报警",1992]
[72,"Arm63","定值超范围",1993]
[72,"Arm64","内存不足",1994]
[72,"Arm65","对时信号状态",1995]
[72,"Arm66","对时服务状态",1996]
[72,"Arm67","时间跳变侦测状态",1997]
[72,"Arm68","CPU总告警",1998]
[72,"Arm69","进程异常",1999]
[72,"Arm70","IEC103配置文件无效",2000]
[72,"Arm71","装置5V电源过压告警",2001]
[72,"Arm72","装置5V电源低压告警",2002]
[72,"Arm73","装置高温告警",2003]
[72,"Arm74","装置低温告警",2004]
[72,"Arm75","4号板开入电源异常",2005]
[72,"Arm76","5号板开入电源异常",2006]
[72,"Arm77","6号板开入电源异常",2007]
[72,"Arm78","7号板开入电源异常",2008]
[72,"Arm79","8号板开入电源异常",2009]
[72,"Arm80","9号板开入电源异常",2010]
[72,"Arm81","10号板开入电源异常",2011]
[72,"Arm82","11号板开入电源异常",2012]
[72,"Arm83","Ⅰ母电压采样校验出错",2013]
[72,"Arm84","Ⅱ母电压采样校验出错",2014]
[72,"Arm85","运行",2015]
[72,"Arm86","异常",2016]
[72,"Arm87","检修",2017]
[72,"Arm88","差动保护闭锁",2018]
[72,"Arm89","母线互联",2019]
[72,"Arm90","刀闸告警",2020]
[72,"Arm91","保护跳闸",2021]
[72,"Arm92","闭锁差动保护",2022]
[72,"Arm93","闭锁失灵保护",2023]
[72,"Arm94","闭锁后备保护",2024]
[72,"Arm95","Ⅰ母差动A相有效",2025]
[72,"Arm96","Ⅰ母差动B相有效",2026]
[72,"Arm97","Ⅰ母差动C相有效",2027]
[72,"Arm98","Ⅱ母差动A相有效",2028]
[72,"Arm99","Ⅱ母差动B相有效",2029]
[72,"Arm100","Ⅱ母差动C相有效",2030]
[72,"Arm101","大差后备有效",2031]
[72,"Arm102","母联失灵有效",2032]
[72,"Arm103","支路4_失灵有效",2033]
[72,"Arm104","支路5_失灵有效",2034]
[72,"Arm105","支路6_失灵有效",2035]
[72,"Arm106","支路7_失灵有效",2036]
[72,"Arm107","支路8_失灵有效",2037]
[72,"Arm108","支路9_失灵有效",2038]
[72,"Arm109","支路10_失灵有效",2039]
[72,"Arm110","支路11_失灵有效",2040]
[72,"Arm111","支路12_失灵有效",2041]
[72,"Arm112","支路13_失灵有效",2042]
[72,"Arm113","主变3失灵有效",2043]
[72,"Arm114","主变4失灵有效",2044]
[72,"Arm115","支路16_失灵有效",2045]
[72,"Arm116","支路17_失灵有效",2046]
[72,"Arm117","支路18_失灵有效",2047]
[72,"Arm118","支路19_失灵有效",2048]
[72,"Arm119","支路20_失灵有效",2049]
[72,"Arm120","支路21_失灵有效",2050]
[72,"Arm121","支路22_失灵有效",2051]
[72,"Arm122","母联代路_失灵有效",2052]
[72,"Arm123","主变1失灵有效",2053]
[72,"Arm124","主变2失灵有效",2054]
[72,"Arm125","分段1失灵有效",2055]
[72,"Arm126","分段2失灵有效",2056]
[72,"Arm127","差动保护投入",2057]
[72,"Arm128","失灵保护投入",2058]
[72,"Arm129","录波完成",2059]
[72,"Arm130","启动打印",2060]
[72,"Arm131","保护检修状态硬压板",2061]
[72,"Arm132","信号复归",2062]
[72,"Arm133","刀闸位置确认",2063]
[72,"Arm134","远方操作硬压板",2064]
[72,"Arm135","失灵启动公共-1",2065]
[72,"Arm136","失灵启动公共-2",2066]
[72,"Arm137","失灵启动公共-3",2067]
[72,"Arm138","失灵启动公共-4",2068]
[72,"Arm139","母联代路_A相启动失灵开入",2069]
[72,"Arm140","母联代路_B相启动失灵开入",2070]
[72,"Arm141","母联代路_C相启动失灵开入",2071]
[72,"Arm142","母联代路_三相启动失灵开入",2072]
[72,"Arm143","母联TWJ",2073]
[72,"Arm144","母联SHJ",2074]
[72,"Arm145","母联_三相启动失灵开入",2075]
[72,"Arm146","母联_三相启动失灵开入2",2076]
[72,"Arm147","母联代路_1G刀闸常开",2077]
[72,"Arm148","母联代路_2G刀闸常开",2078]
[72,"Arm149","母联代路硬压板",2079]
[72,"Arm150","母联代路负硬压板",2080]
[72,"Arm151","主变1_三相启动失灵开入",2081]
[72,"Arm152","主变1解闭锁开入",2082]
[72,"Arm153","主变2_三相启动失灵开入",2083]
[72,"Arm154","主变2解闭锁开入",2084]
[72,"Arm155","支路4_A相启动失灵开入",2085]
[72,"Arm156","支路4_B相启动失灵开入",2086]
[72,"Arm157","支路4_C相启动失灵开入",2087]
[72,"Arm158","支路4_三相启动失灵开入",2088]
[72,"Arm159","支路4_1G刀闸常开",2089]
[72,"Arm160","支路4_2G刀闸常开",2090]
[72,"Arm161","支路4_1G刀闸位置",2091]
[72,"Arm162","支路4_2G刀闸位置",2092]
[72,"Arm163","支路5_A相启动失灵开入",2093]
[72,"Arm164","支路5_B相启动失灵开入",2094]
[72,"Arm165","支路5_C相启动失灵开入",2095]
[72,"Arm166","支路5_三相启动失灵开入",2096]
[72,"Arm167","支路5_1G刀闸常开",2097]
[72,"Arm168","支路5_2G刀闸常开",2098]
[72,"Arm169","支路5_1G刀闸位置",2099]
[72,"Arm170","支路5_2G刀闸位置",2100]
[72,"Arm171","支路6_A相启动失灵开入",2101]
[72,"Arm172","支路6_B相启动失灵开入",2102]
[72,"Arm173","支路6_C相启动失灵开入",2103]
[72,"Arm174","支路6_三相启动失灵开入",2104]
[72,"Arm175","支路6_1G刀闸常开",2105]
[72,"Arm176","支路6_2G刀闸常开",2106]
[72,"Arm177","支路6_1G刀闸位置",2107]
[72,"Arm178","支路6_2G刀闸位置",2108]
[72,"Arm179","支路7_A相启动失灵开入",2109]
[72,"Arm180","支路7_B相启动失灵开入",2110]
[72,"Arm181","支路7_C相启动失灵开入",2111]
[72,"Arm182","支路7_三相启动失灵开入",2112]
[72,"Arm183","支路7_1G刀闸常开",2113]
[72,"Arm184","支路7_2G刀闸常开",2114]
[72,"Arm185","支路7_1G刀闸位置",2115]
[72,"Arm186","支路7_2G刀闸位置",2116]
[72,"Arm187","支路8_A相启动失灵开入",2117]
[72,"Arm188","支路8_B相启动失灵开入",2118]
[72,"Arm189","支路8_C相启动失灵开入",2119]
[72,"Arm190","支路8_三相启动失灵开入",2120]
[72,"Arm191","支路8_1G刀闸常开",2121]
[72,"Arm192","支路8_2G刀闸常开",2122]
[72,"Arm193","支路8_1G刀闸位置",2123]
[72,"Arm194","支路8_2G刀闸位置",2124]
[72,"Arm195","支路9_A相启动失灵开入",2125]
[72,"Arm196","支路9_B相启动失灵开入",2126]
[72,"Arm197","支路9_C相启动失灵开入",2127]
[72,"Arm198","支路9_三相启动失灵开入",2128]
[72,"Arm199","支路9_1G刀闸常开",2129]
[72,"Arm200","支路9_2G刀闸常开",2130]
[72,"Arm201","支路9_1G刀闸位置",2131]
[72,"Arm202","支路9_2G刀闸位置",2132]
[72,"Arm203","支路10_A相启动失灵开入",2133]
[72,"Arm204","支路10_B相启动失灵开入",2134]
[72,"Arm205","支路10_C相启动失灵开入",2135]
[72,"Arm206","支路10_三相启动失灵开入",2136]
[72,"Arm207","支路10_1G刀闸常开",2137]
[72,"Arm208","支路10_2G刀闸常开",2138]
[72,"Arm209","支路10_1G刀闸位置",2139]
[72,"Arm210","支路10_2G刀闸位置",2140]
[72,"Arm211","支路11_A相启动失灵开入",2141]
[72,"Arm212","支路11_B相启动失灵开入",2142]
[72,"Arm213","支路11_C相启动失灵开入",2143]
[72,"Arm214","支路11_三相启动失灵开入",2144]
[72,"Arm215","支路11_1G刀闸常开",2145]
[72,"Arm216","支路11_2G刀闸常开",2146]
[72,"Arm217","支路11_1G刀闸位置",2147]
[72,"Arm218","支路11_2G刀闸位置",2148]
[72,"Arm219","支路12_A相启动失灵开入",2149]
[72,"Arm220","支路12_B相启动失灵开入",2150]
[72,"Arm221","支路12_C相启动失灵开入",2151]
[72,"Arm222","支路12_三相启动失灵开入",2152]
[72,"Arm223","支路12_1G刀闸常开",2153]
[72,"Arm224","支路12_2G刀闸常开",2154]
[72,"Arm225","支路12_1G刀闸位置",2155]
[72,"Arm226","支路12_2G刀闸位置",2156]
[72,"Arm227","支路13_A相启动失灵开入",2157]
[72,"Arm228","支路13_B相启动失灵开入",2158]
[72,"Arm229","支路13_C相启动失灵开入",2159]
[72,"Arm230","支路13_三相启动失灵开入",2160]
[72,"Arm231","支路13_1G刀闸常开",2161]
[72,"Arm232","支路13_2G刀闸常开",2162]
[72,"Arm233","支路13_1G刀闸位置",2163]
[72,"Arm234","支路13_2G刀闸位置",2164]
[72,"Arm235","主变3_三相启动失灵开入",2165]
[72,"Arm236","主变3解闭锁开入",2166]
[72,"Arm237","主变3_1G刀闸常开",2167]
[72,"Arm238","主变3_2G刀闸常开",2168]
[72,"Arm239","主变3_1G刀闸位置",2169]
[72,"Arm240","主变3_2G刀闸位置",2170]
[72,"Arm241","主变4_三相启动失灵开入",2171]
[72,"Arm242","主变4解闭锁开入",2172]
[72,"Arm243","主变4_1G刀闸常开",2173]
[72,"Arm244","主变4_2G刀闸常开",2174]
[72,"Arm245","主变4_1G刀闸位置",2175]
[72,"Arm246","主变4_2G刀闸位置",2176]
[72,"Arm247","支路16_A相启动失灵开入",2177]
[72,"Arm248","支路16_B相启动失灵开入",2178]
[72,"Arm249","支路16_C相启动失灵开入",2179]
[72,"Arm250","支路16_三相启动失灵开入",2180]
[72,"Arm251","支路16_1G刀闸常开",2181]
[72,"Arm252","支路16_2G刀闸常开",2182]
[72,"Arm253","支路16_1G刀闸位置",2183]
[72,"Arm254","支路16_2G刀闸位置",2184]
[72,"Arm255","支路17_A相启动失灵开入",2185]
[72,"Arm256","支路17_B相启动失灵开入",2186]
[72,"Arm257","支路17_C相启动失灵开入",2187]
[72,"Arm258","支路17_三相启动失灵开入",2188]
[72,"Arm259","支路17_1G刀闸常开",2189]
[72,"Arm260","支路17_2G刀闸常开",2190]
[72,"Arm261","支路17_1G刀闸位置",2191]
[72,"Arm262","支路17_2G刀闸位置",2192]
[72,"Arm263","支路18_A相启动失灵开入",2193]
[72,"Arm264","支路18_B相启动失灵开入",2194]
[72,"Arm265","支路18_C相启动失灵开入",2195]
[72,"Arm266","支路18_三相启动失灵开入",2196]
[72,"Arm267","支路18_1G刀闸常开",2197]
[72,"Arm268","支路18_2G刀闸常开",2198]
[72,"Arm269","支路18_1G刀闸位置",2199]
[72,"Arm270","支路18_2G刀闸位置",2200]
[72,"Arm271","支路19_A相启动失灵开入",2201]
[72,"Arm272","支路19_B相启动失灵开入",2202]
[72,"Arm273","支路19_C相启动失灵开入",2203]
[72,"Arm274","支路19_三相启动失灵开入",2204]
[72,"Arm275","支路19_1G刀闸常开",2205]
[72,"Arm276","支路19_2G刀闸常开",2206]
[72,"Arm277","支路19_1G刀闸位置",2207]
[72,"Arm278","支路19_2G刀闸位置",2208]
[72,"Arm279","支路20_A相启动失灵开入",2209]
[72,"Arm280","支路20_B相启动失灵开入",2210]
[72,"Arm281","支路20_C相启动失灵开入",2211]
[72,"Arm282","支路20_三相启动失灵开入",2212]
[72,"Arm283","支路20_1G刀闸常开",2213]
[72,"Arm284","支路20_2G刀闸常开",2214]
[72,"Arm285","支路20_1G刀闸位置",2215]
[72,"Arm286","支路20_2G刀闸位置",2216]
[72,"Arm287","支路21_A相启动失灵开入",2217]
[72,"Arm288","支路21_B相启动失灵开入",2218]
[72,"Arm289","支路21_C相启动失灵开入",2219]
[72,"Arm290","支路21_三相启动失灵开入",2220]
[72,"Arm291","支路21_1G刀闸常开",2221]
[72,"Arm292","支路21_2G刀闸常开",2222]
[72,"Arm293","支路21_1G刀闸位置",2223]
[72,"Arm294","支路21_2G刀闸位置",2224]
[72,"Arm295","支路22_A相启动失灵开入",2225]
[72,"Arm296","支路22_B相启动失灵开入",2226]
[72,"Arm297","支路22_C相启动失灵开入",2227]
[72,"Arm298","支路22_三相启动失灵开入",2228]
[72,"Arm299","支路22_1G刀闸常开",2229]
[72,"Arm300","支路22_2G刀闸常开",2230]
[72,"Arm301","支路22_1G刀闸位置",2231]
[72,"Arm302","支路22_2G刀闸位置",2232]
[72,"Arm303","差动保护硬压板",2233]
[72,"Arm304","外部闭锁母差",2234]
[72,"Arm305","失灵保护硬压板",2235]
[72,"Arm306","母线互联硬压板",2236]
[72,"Arm307","解除电压闭锁开入",2237]
[72,"Arm308","主变1_1G刀闸常开",2238]
[72,"Arm309","主变1_2G刀闸常开",2239]
[72,"Arm310","主变1_1G刀闸位置",2240]
[72,"Arm311","主变1_2G刀闸位置",2241]
[72,"Arm312","主变2_1G刀闸常开",2242]
[72,"Arm313","主变2_2G刀闸常开",2243]
[72,"Arm314","主变2_1G刀闸位置",2244]
[72,"Arm315","主变2_2G刀闸位置",2245]
[72,"Arm316","分段1TWJ",2246]
[72,"Arm317","分段1SHJ",2247]
[72,"Arm318","分段1_三相启动失灵开入",2248]
[72,"Arm319","分段1_对侧失灵开入",2249]
[72,"Arm320","分段2TWJ",2250]
[72,"Arm321","分段2SHJ",2251]
[72,"Arm322","分段2_三相启动失灵开入",2252]
[72,"Arm323","分段2_对侧失灵开入",2253]
[72,"Arm324","母联_1G刀闸位置",2254]
[72,"Arm325","母联_2G刀闸位置",2255]
[72,"Arm326","分段1_1G刀闸位置",2256]
[72,"Arm327","分段1_2G刀闸位置",2257]
[72,"Arm328","分段2_1G刀闸位置",2258]
[72,"Arm329","分段2_2G刀闸位置",2259]
[72,"Arm330","保护启动",2260]
[72,"Arm331","差动保护启动",2261]
[72,"Arm332","失灵保护启动",2262]
[72,"Arm333","手动录波触发",2263]
[72,"Arm334","远方触发录波",2264]
[72,"Arm335","变化量差动跳Ⅰ母",2265]
[72,"Arm336","变化量差动跳Ⅱ母",2266]
[72,"Arm337","稳态量差动跳Ⅰ母",2267]
[72,"Arm338","稳态量差动跳Ⅱ母",2268]
[72,"Arm339","大差后备一段动作",2269]
[72,"Arm340","大差后备二段动作",2270]
[72,"Arm341","Ⅰ母差动动作",2271]
[72,"Arm342","Ⅱ母差动动作",2272]
[72,"Arm343","Ⅰ母失灵保护动作",2273]
[72,"Arm344","Ⅱ母失灵保护动作",2274]
[72,"Arm345","差动保护跳母联",2275]
[72,"Arm346","失灵保护跳母联",2276]
[72,"Arm347","母联失灵保护动作",2277]
[72,"Arm348","母联死区",2278]
[72,"Arm349","母联",2279]
[72,"Arm350","变压器1失灵联跳",2280]
[72,"Arm351","主变1",2281]
[72,"Arm352","变压器2失灵联跳",2282]
[72,"Arm353","主变2",2283]
[72,"Arm354","支路4",2284]
[72,"Arm355","支路5",2285]
[72,"Arm356","支路6",2286]
[72,"Arm357","支路7",2287]
[72,"Arm358","支路8",2288]
[72,"Arm359","支路9",2289]
[72,"Arm360","支路10",2290]
[72,"Arm361","支路11",2291]
[72,"Arm362","支路12",2292]
[72,"Arm363","支路13",2293]
[72,"Arm364","变压器3失灵联跳",2294]
[72,"Arm365","主变3",2295]
[72,"Arm366","变压器4失灵联跳",2296]
[72,"Arm367","主变4",2297]
[72,"Arm368","支路16",2298]
[72,"Arm369","支路17",2299]
[72,"Arm370","支路18",2300]
[72,"Arm371","支路19",2301]
[72,"Arm372","支路20",2302]
[72,"Arm373","支路21",2303]
[72,"Arm374","支路22",2304]
[72,"Arm375","差动保护跳分段1",2305]
[72,"Arm376","失灵保护跳分段1",2306]
[72,"Arm377","分段1失灵保护动作",2307]
[72,"Arm378","分段1死区",2308]
[72,"Arm379","分段1启动失灵",2309]
[72,"Arm380","分段1",2310]
[72,"Arm381","差动保护跳分段2",2311]
[72,"Arm382","失灵保护跳分段2",2312]
[72,"Arm383","分段2失灵保护动作",2313]
[72,"Arm384","分段2死区",2314]
[72,"Arm385","分段2启动失灵",2315]
[72,"Arm386","分段2",2316]
[72,"Arm387","模拟量采集错",2317]
[72,"Arm388","开出异常",2318]
[72,"Arm389","保护CPU插件异常",2319]
[72,"Arm390","2号板内存出错",2320]
[72,"Arm391","3号板内存出错",2321]
[72,"Arm392","对时异常",2322]
[72,"Arm393","装置长期启动报警",2323]
[72,"Arm394","失灵启动开入异常",2324]
[72,"Arm395","支路刀闸位置异常",2325]
[72,"Arm396","母联/分段CT断线",2326]
[72,"Arm397","母联失灵启动异常",2327]
[72,"Arm398","分段1失灵启动异常",2328]
[72,"Arm399","分段2失灵启动异常",2329]
[72,"Arm400","失灵公共开入异常-1",2330]
[72,"Arm401","失灵公共开入异常-2",2331]
[72,"Arm402","失灵公共开入异常-3",2332]
[72,"Arm403","失灵公共开入异常-4",2333]
[72,"Arm404","母联CT断线",2334]
[72,"Arm405","母联CT异常",2335]
[72,"Arm406","母联代路刀闸位置异常",2336]
[72,"Arm407","母联A相CT断线",2337]
[72,"Arm408","母联B相CT断线",2338]
[72,"Arm409","母联C相CT断线",2339]
[72,"Arm410","母联A相CT异常",2340]
[72,"Arm411","母联B相CT异常",2341]
[72,"Arm412","母联C相CT异常",2342]
[72,"Arm413","母联跳位异常",2343]
[72,"Arm414","母联手合开入异常",2344]
[72,"Arm415","母联代路失灵启动异常",2345]
[72,"Arm416","母联失灵长期启动",2346]
[72,"Arm417","母联_三相失灵启动异常",2347]
[72,"Arm418","母联三相启动失灵开入2异常",2348]
[72,"Arm419","主变1刀闸位置异常",2349]
[72,"Arm420","主变1失灵启动开入异常",2350]
[72,"Arm421","主变1解闭锁开入异常",2351]
[72,"Arm422","主变2刀闸位置异常",2352]
[72,"Arm423","主变2失灵启动开入异常",2353]
[72,"Arm424","主变2解闭锁开入异常",2354]
[72,"Arm425","支路4刀闸位置异常",2355]
[72,"Arm426","支路4CT断线",2356]
[72,"Arm427","支路4CT异常",2357]
[72,"Arm428","支路4失灵启动开入异常",2358]
[72,"Arm429","支路5刀闸位置异常",2359]
[72,"Arm430","支路5CT断线",2360]
[72,"Arm431","支路5CT异常",2361]
[72,"Arm432","支路5失灵启动开入异常",2362]
[72,"Arm433","支路6刀闸位置异常",2363]
[72,"Arm434","支路6CT断线",2364]
[72,"Arm435","支路6CT异常",2365]
[72,"Arm436","支路6失灵启动开入异常",2366]
[72,"Arm437","支路7刀闸位置异常",2367]
[72,"Arm438","支路7CT断线",2368]
[72,"Arm439","支路7CT异常",2369]
[72,"Arm440","支路7失灵启动开入异常",2370]
[72,"Arm441","支路8刀闸位置异常",2371]
[72,"Arm442","支路8CT断线",2372]
[72,"Arm443","支路8CT异常",2373]
[72,"Arm444","支路8失灵启动开入异常",2374]
[72,"Arm445","支路9刀闸位置异常",2375]
[72,"Arm446","支路9CT断线",2376]
[72,"Arm447","支路9CT异常",2377]
[72,"Arm448","支路9失灵启动开入异常",2378]
[72,"Arm449","支路10刀闸位置异常",2379]
[72,"Arm450","支路10CT断线",2380]
[72,"Arm451","支路10CT异常",2381]
[72,"Arm452","支路10失灵启动开入异常",2382]
[72,"Arm453","支路11刀闸位置异常",2383]
[72,"Arm454","支路11CT断线",2384]
[72,"Arm455","支路11CT异常",2385]
[72,"Arm456","支路11失灵启动开入异常",2386]
[72,"Arm457","支路12刀闸位置异常",2387]
[72,"Arm458","支路12CT断线",2388]
[72,"Arm459","支路12CT异常",2389]
[72,"Arm460","支路12失灵启动开入异常",2390]
[72,"Arm461","支路13刀闸位置异常",2391]
[72,"Arm462","支路13CT断线",2392]
[72,"Arm463","支路13CT异常",2393]
[72,"Arm464","支路13失灵启动开入异常",2394]
[72,"Arm465","主变3刀闸位置异常",2395]
[72,"Arm466","主变3CT断线",2396]
[72,"Arm467","主变3CT异常",2397]
[72,"Arm468","主变3失灵启动开入异常",2398]
[72,"Arm469","主变3解闭锁开入异常",2399]
[72,"Arm470","主变4刀闸位置异常",2400]
[72,"Arm471","主变4CT断线",2401]
[72,"Arm472","主变4CT异常",2402]
[72,"Arm473","主变4失灵启动开入异常",2403]
[72,"Arm474","主变4解闭锁开入异常",2404]
[72,"Arm475","支路16刀闸位置异常",2405]
[72,"Arm476","支路16CT断线",2406]
[72,"Arm477","支路19刀闸位置异常",2407]
[72,"Arm478","支路16失灵启动开入异常",2408]
[72,"Arm479","支路17刀闸位置异常",2409]
[72,"Arm480","支路17CT断线",2410]
[72,"Arm481","支路17CT异常",2411]
[72,"Arm482","支路17失灵启动开入异常",2412]
[72,"Arm483","支路18刀闸位置异常",2413]
[72,"Arm484","支路18CT断线",2414]
[72,"Arm485","支路18CT异常",2415]
[72,"Arm486","支路18失灵启动开入异常",2416]
[72,"Arm487","支路19刀闸位置异常",2417]
[72,"Arm488","支路19CT断线",2418]
[72,"Arm489","支路19CT异常",2419]
[72,"Arm490","支路19失灵启动开入异常",2420]
[72,"Arm491","支路20刀闸位置异常",2421]
[72,"Arm492","支路20CT断线",2422]
[72,"Arm493","支路20CT异常",2423]
[72,"Arm494","支路20失灵启动开入异常",2424]
[72,"Arm495","支路21刀闸位置异常",2425]
[72,"Arm496","支路21CT断线",2426]
[72,"Arm497","支路21CT异常",2427]
[72,"Arm498","支路21失灵启动开入异常",2428]
[72,"Arm499","支路22刀闸位置异常",2429]
[72,"Arm500","支路22CT断线",2430]
[72,"Arm501","支路22CT异常",2431]
[72,"Arm502","支路22失灵启动开入异常",2432]
[72,"Arm503","Ⅰ母PT断线",2433]
[72,"Arm504","Ⅰ母电压闭锁开放",2434]
[72,"Arm505","Ⅱ母PT断线",2435]
[72,"Arm506","Ⅱ母电压闭锁开放",2436]
[72,"Arm507","外部闭锁母差开入异常",2437]
[72,"Arm508","稳态量差动长期启动",2438]
[72,"Arm509","支路CT断线",2439]
[72,"Arm510","支路CT异常",2440]
[72,"Arm511","支路A相CT断线",2441]
[72,"Arm512","支路B相CT断线",2442]
[72,"Arm513","支路C相CT断线",2443]
[72,"Arm514","支路A相CT异常",2444]
[72,"Arm515","支路B相CT异常",2445]
[72,"Arm516","支路C相CT异常",2446]
[72,"Arm517","失灵长期启动",2447]
[72,"Arm518","装置长期闭锁报警",2448]
[72,"Arm519","母线互联运行",2449]
[72,"Arm520","主变1CT断线",2450]
[72,"Arm521","主变1CT异常",2451]
[72,"Arm522","主变2CT断线",2452]
[72,"Arm523","主变2CT异常",2453]
[72,"Arm524","分段1CT断线",2454]
[72,"Arm525","分段1CT异常",2455]
[72,"Arm526","分段1跳位异常",2456]
[72,"Arm527","分段1手合开入异常",2457]
[72,"Arm528","分段1失灵长期启动",2458]
[72,"Arm529","分段1_三相失灵启动异常",2459]
[72,"Arm530","分段1对侧失灵开入异常",2460]
[72,"Arm531","分段2CT断线",2461]
[72,"Arm532","分段2CT异常",2462]
[72,"Arm533","分段2跳位异常",2463]
[72,"Arm534","分段2手合开入异常",2464]
[72,"Arm535","分段2失灵长期启动",2465]
[72,"Arm536","分段2_三相失灵启动异常",2466]
[72,"Arm537","分段2对侧失灵开入异常",2467]
[72,"Arm538","接点传动报警",2468]
[72,"Arm539","远方修改定值软压板",2469]
[72,"Arm540","远方投退压板软压板",2470]
[72,"Arm541","远方切换定值区软压板",2471]
[72,"Arm542","母联分列软压板",2472]
[72,"Arm543","差动保护软压板",2473]
[72,"Arm544","失灵保护软压板",2474]
[72,"Arm545","母线互联软压板",2475]
[72,"Arm546","分段1分列软压板",2476]
[72,"Arm547","分段2分列软压板",2477]
[72,"Arm548","母差动作",2478]
[72,"Arm549","失灵动作",2479]
[72,"Arm550","其他动作",2480]
[72,"Arm551","保护动作",2481]
[72,"Arm552","保护动作保持",2482]
[72,"Arm553","网络状态1",2483]
[72,"Arm554","网络状态2",2484]
[72,"Arm555","装置通讯状态",2485]
[72,"Arm556","检修状态",2486]
[72,"Arm557","参数变化",2487]
[72,"Arm558","就地状态虚遥信",2488]
[72,"Arm559","遥控解除闭锁",2489]
[72,"Arm560","A网中断",2490]
[72,"Arm561","B网中断",2491]
[72,"Arm562","网络中断",2492]
[73,"Arm1","I类告警总",2493]
[73,"Arm2","模拟量采集错",2494]
[73,"Arm3","设备参数错",2495]
[73,"Arm4","ROM和校验错",2496]
[73,"Arm5","定值错",2497]
[73,"Arm6","定值区指针错",2498]
[73,"Arm7","软压板错",2499]
[73,"Arm8","系统配置错",2500]
[73,"Arm9","开出异常",2501]
[73,"Arm10","开出配置错",2502]
[73,"Arm11","保护CPU插件异常",2503]
[73,"Arm12","CPU通讯中断",2504]
[73,"Arm13","召唤配置无应答",2505]
[73,"Arm14","对时异常",2506]
[73,"Arm15","对时信号状态",2507]
[73,"Arm16","对时服务状态",2508]
[73,"Arm17","时间跳变侦测状态",2509]
[73,"Arm18","充电过流保护硬压板",2510]
[73,"Arm19","远方操作硬压板",2511]
[73,"Arm20","保护检修状态硬压板",2512]
[73,"Arm21","充电过流保护总压板",2513]
[73,"Arm22","运行",2514]
[73,"Arm23","异常",2515]
[73,"Arm24","检修",2516]
[73,"Arm25","保护跳闸",2517]
[73,"Arm26","充电过流Ⅰ段有效",2518]
[73,"Arm27","充电过流Ⅱ段有效",2519]
[73,"Arm28","充电零序过流有效",2520]
[73,"Arm29","闭锁充电保护",2521]
[73,"Arm30","充电过流保护投入",2522]
[73,"Arm31","录波完成",2523]
[73,"Arm32","录波启动",2524]
[73,"Arm33","充电过流保护软压板",2525]
[73,"Arm34","远方投退压板软压板",2526]
[73,"Arm35","远方切换定值区软压板",2527]
[73,"Arm36","远方修改定值软压板",2528]
[73,"Arm37","信号复归",2529]
[73,"Arm38","保护动作",2530]
[73,"Arm39","保护启动",2531]
[73,"Arm40","故障相电流",2532]
[73,"Arm41","充电过流Ⅰ段动作",2533]
[73,"Arm42","充电过流Ⅱ段动作",2534]
[73,"Arm43","充电零序过流动作",2535]
[73,"Arm44","II类告警总",2536]
[73,"Arm45","跳闸失败",2537]
[73,"Arm46","SRAM自检异常",2538]
[73,"Arm47","FLASH自检异常",2539]
[73,"Arm48","开入异常",2540]
[73,"Arm49","开出通讯中断",2541]
[73,"Arm50","传动状态未复归",2542]
[73,"Arm51","开入击穿",2543]
[73,"Arm52","开入输入不正常",2544]
[73,"Arm53","开入自检回路出错",2545]
[73,"Arm54","开入EEPROM出错",2546]
[73,"Arm55","开出EEPROM出错",2547]
[73,"Arm56","CT断线",2548]
[73,"Arm57","模拟通道异常",2549]
[73,"Arm58","电流相序不对应",2550]
[73,"Arm59","工作于调试定值区",2551]
[73,"Arm60","网络状态1",2552]
[73,"Arm61","网络状态2",2553]
[73,"Arm62","装置通讯状态",2554]
[73,"Arm63","检修状态",2555]
[73,"Arm64","参数变化",2556]
[73,"Arm65","就地状态虚遥信",2557]
[73,"Arm66","遥控解除闭锁",2558]
[73,"Arm67","A网中断",2559]
[73,"Arm68","B网中断",2560]
[73,"Arm69","网络中断",2561]
[74,"Arm1","启动打印",2562]
[74,"Arm2","保护检修状态硬压板",2563]
[74,"Arm3","信号复归",2564]
[74,"Arm4","远方操作硬压板",2565]
[74,"Arm5","手动录波触发",2566]
[74,"Arm6","远方触发录波",2567]
[74,"Arm7","装置闭锁",2568]
[74,"Arm8","CID文件错误",2569]
[74,"Arm9","定值超范围",2570]
[74,"Arm10","板卡配置错误",2571]
[74,"Arm11","定值项变化告警",2572]
[74,"Arm12","插件8异常",2573]
[74,"Arm13","装置报警",2574]
[74,"Arm14","通信传动报警",2575]
[74,"Arm15","对时信号状态",2576]
[74,"Arm16","对时服务状态",2577]
[74,"Arm17","时间跳变侦测状态",2578]
[74,"Arm18","对时异常",2579]
[74,"Arm19","版本错误报警",2580]
[74,"Arm20","定值校验出错",2581]
[74,"Arm21","定值区不一致",2582]
[74,"Arm22","定值修改",2583]
[74,"Arm23","定值区切换",2584]
[74,"Arm24","内存不足",2585]
[74,"Arm25","IEC103配置文件无效",2586]
[74,"Arm26","插件8光耦电源异常",2587]
[74,"Arm27","电源异常",2588]
[74,"Arm28","接点传动状态告警",2589]
[74,"Arm29","装置高温告警",2590]
[74,"Arm30","装置低温告警",2591]
[74,"Arm31","保护2.5V电压上限告警",2592]
[74,"Arm32","保护2.5V电压下限告警",2593]
[74,"Arm33","启动2.5V电压上限告警",2594]
[74,"Arm34","启动2.5V电压下限告警",2595]
[74,"Arm35","装置电源监视告警",2596]
[74,"Arm36","运行",2597]
[74,"Arm37","异常",2598]
[74,"Arm38","检修",2599]
[74,"Arm39","保护跳闸",2600]
[74,"Arm40","闭锁充电保护",2601]
[74,"Arm41","充电过流Ⅰ段有效",2602]
[74,"Arm42","充电过流Ⅱ段有效",2603]
[74,"Arm43","充电零序过流有效",2604]
[74,"Arm44","充电过流保护投入",2605]
[74,"Arm45","录波完成",2606]
[74,"Arm46","充电过流保护硬压板",2607]
[74,"Arm47","跳闸出口",2608]
[74,"Arm48","装置异常启动录波",2609]
[74,"Arm49","保护启动",2610]
[74,"Arm50","保护动作",2611]
[74,"Arm51","充电过流Ⅰ段动作",2612]
[74,"Arm52","充电过流Ⅱ段动作",2613]
[74,"Arm53","充电零序过流动作",2614]
[74,"Arm54","保护CPU插件异常",2615]
[74,"Arm55","开出异常",2616]
[74,"Arm56","模拟量采集错",2617]
[74,"Arm57","保护DSP装置类型配置错",2618]
[74,"Arm58","保护DSP定值出错",2619]
[74,"Arm59","保护DSP内存出错",2620]
[74,"Arm60","保护DSP采样出错",2621]
[74,"Arm61","跳合出口回路异常",2622]
[74,"Arm62","保护DSP校验出错",2623]
[74,"Arm63","启动DSP装置类型配置错",2624]
[74,"Arm64","启动DSP定值出错",2625]
[74,"Arm65","启动DSP内存出错",2626]
[74,"Arm66","启动DSP采样出错",2627]
[74,"Arm67","启动DSP校验出错",2628]
[74,"Arm68","CT断线",2629]
[74,"Arm69","长期启动报警",2630]
[74,"Arm70","充电过流保护软压板",2631]
[74,"Arm71","远方投退压板软压板",2632]
[74,"Arm72","远方切换定值区软压板",2633]
[74,"Arm73","远方修改定值软压板",2634]
[74,"Arm74","网络状态1",2635]
[74,"Arm75","网络状态2",2636]
[74,"Arm76","装置通讯状态",2637]
[74,"Arm77","检修状态",2638]
[74,"Arm78","参数变化",2639]
[74,"Arm79","就地状态虚遥信",2640]
[74,"Arm80","遥控解除闭锁",2641]
[74,"Arm81","A网中断",2642]
[74,"Arm82","B网中断",2643]
[74,"Arm83","网络中断",2644]
[75,"Arm1","I类告警总",2645]
[75,"Arm2","模拟量采集错",2646]
[75,"Arm3","ROM和校验错",2647]
[75,"Arm4","定值错",2648]
[75,"Arm5","定值区指针错",2649]
[75,"Arm6","开出不响应",2650]
[75,"Arm7","开出击穿",2651]
[75,"Arm8","设备参数错",2652]
[75,"Arm9","软压板错",2653]
[75,"Arm10","系统配置错",2654]
[75,"Arm11","开出模件异常",2655]
[75,"Arm12","开出配置错",2656]
[75,"Arm13","开出EEPROM出错",2657]
[75,"Arm14","保护CPU插件异常",2658]
[75,"Arm15","开出异常",2659]
[75,"Arm16","CPU通讯中断",2660]
[75,"Arm17","设备参数不一致",2661]
[75,"Arm18","定值区号不一致",2662]
[75,"Arm19","定值不一致",2663]
[75,"Arm20","压板不一致",2664]
[75,"Arm21","召唤配置无应答",2665]
[75,"Arm22","对时异常",2666]
[75,"Arm23","面板配置不一致",2667]
[75,"Arm24","对时信号状态",2668]
[75,"Arm25","对时服务状态",2669]
[75,"Arm26","时间跳变侦测状态",2670]
[75,"Arm27","主保护硬压板",2671]
[75,"Arm28","高压侧后备保护硬压板",2672]
[75,"Arm29","高压侧电压硬压板",2673]
[75,"Arm30","低压1分支后备保护硬压板",2674]
[75,"Arm31","低压1分支电压硬压板",2675]
[75,"Arm32","低压2分支后备保护硬压板",2676]
[75,"Arm33","低压2分支电压硬压板",2677]
[75,"Arm34","远方操作硬压板",2678]
[75,"Arm35","保护检修状态硬压板",2679]
[75,"Arm36","主保护总压板",2680]
[75,"Arm37","高压侧后备保护总压板",2681]
[75,"Arm38","低压1分支后备保护总压板",2682]
[75,"Arm39","低压2分支后备保护总压板",2683]
[75,"Arm40","运行",2684]
[75,"Arm41","异常",2685]
[75,"Arm42","检修",2686]
[75,"Arm43","差动保护闭锁",2687]
[75,"Arm44","保护跳闸",2688]
[75,"Arm45","纵差差动速断有效",2689]
[75,"Arm46","纵差变化量差动有效",2690]
[75,"Arm47","纵差保护有效",2691]
[75,"Arm48","高相间阻抗有效",2692]
[75,"Arm49","高接地阻抗有效",2693]
[75,"Arm50","高复流Ⅰ段有效",2694]
[75,"Arm51","高复流Ⅱ段有效",2695]
[75,"Arm52","高复流Ⅲ段有效",2696]
[75,"Arm53","高零流Ⅰ段有效",2697]
[75,"Arm54","高零流Ⅱ段有效",2698]
[75,"Arm55","高零流Ⅲ段有效",2699]
[75,"Arm56","高失灵联跳有效",2700]
[75,"Arm57","高间隙过流有效",2701]
[75,"Arm58","高零序过压有效",2702]
[75,"Arm59","低1复流Ⅰ段有效",2703]
[75,"Arm60","低1复流Ⅱ段有效",2704]
[75,"Arm61","低2复流Ⅰ段有效",2705]
[75,"Arm62","低2复流Ⅱ段有效",2706]
[75,"Arm63","闭锁主保护",2707]
[75,"Arm64","闭锁后备保护",2708]
[75,"Arm65","主保护投入",2709]
[75,"Arm66","高压侧后备保护投入",2710]
[75,"Arm67","低压1分支后备保护投入",2711]
[75,"Arm68","低压2分支后备保护投入",2712]
[75,"Arm69","录波完成",2713]
[75,"Arm70","录波启动",2714]
[75,"Arm71","主保护软压板",2715]
[75,"Arm72","高压侧后备保护软压板",2716]
[75,"Arm73","低压1分支后备保护软压板",2717]
[75,"Arm74","低压2分支后备保护软压板",2718]
[75,"Arm75","远方投退压板软压板",2719]
[75,"Arm76","远方切换定值区软压板",2720]
[75,"Arm77","远方修改定值软压板",2721]
[75,"Arm78","高压侧失灵联跳开入",2722]
[75,"Arm79","信号复归",2723]
[75,"Arm80","保护动作",2724]
[75,"Arm81","保护启动",2725]
[75,"Arm82","纵差保护",2726]
[75,"Arm83","纵差差动速断",2727]
[75,"Arm84","高相间阻抗1时限",2728]
[75,"Arm85","高相间阻抗2时限",2729]
[75,"Arm86","高相间阻抗3时限",2730]
[75,"Arm87","高接地阻抗1时限",2731]
[75,"Arm88","高接地阻抗2时限",2732]
[75,"Arm89","高接地阻抗3时限",2733]
[75,"Arm90","高复流Ⅰ段1时限",2734]
[75,"Arm91","低1复流Ⅰ段1时限",2735]
[75,"Arm92","低2复流Ⅰ段1时限",2736]
[75,"Arm93","高复流Ⅰ段2时限",2737]
[75,"Arm94","高复流Ⅰ段3时限",2738]
[75,"Arm95","高复流Ⅱ段2时限",2739]
[75,"Arm96","高复流Ⅱ段3时限",2740]
[75,"Arm97","高复流Ⅲ段2时限",2741]
[75,"Arm98","低1复流Ⅰ段2时限",2742]
[75,"Arm99","低1复流Ⅰ段3时限",2743]
[75,"Arm100","低1复流Ⅱ段2时限",2744]
[75,"Arm101","低1复流Ⅱ段3时限",2745]
[75,"Arm102","低2复流Ⅰ段2时限",2746]
[75,"Arm103","低2复流Ⅰ段3时限",2747]
[75,"Arm104","低2复流Ⅱ段2时限",2748]
[75,"Arm105","低2复流Ⅱ段3时限",2749]
[75,"Arm106","高复流Ⅱ段1时限",2750]
[75,"Arm107","高复流Ⅲ段1时限",2751]
[75,"Arm108","低1复流Ⅱ段1时限",2752]
[75,"Arm109","低2复流Ⅱ段1时限",2753]
[75,"Arm110","高零流Ⅰ段1时限",2754]
[75,"Arm111","高零流Ⅱ段1时限",2755]
[75,"Arm112","高零流Ⅰ段2时限",2756]
[75,"Arm113","高零流Ⅰ段3时限",2757]
[75,"Arm114","高零流Ⅱ段2时限",2758]
[75,"Arm115","高零流Ⅱ段3时限",2759]
[75,"Arm116","高零流Ⅲ段2时限",2760]
[75,"Arm117","高间隙过流",2761]
[75,"Arm118","高零流Ⅲ段1时限",2762]
[75,"Arm119","高零序过压",2763]
[75,"Arm120","高断路器失灵联跳",2764]
[75,"Arm121","故障分量差动",2765]
[75,"Arm122","II类告警总",2766]
[75,"Arm123","开入击穿",2767]
[75,"Arm124","开入输入不正常",2768]
[75,"Arm125","双位置输入不一致",2769]
[75,"Arm126","失灵开入异常",2770]
[75,"Arm127","CAN通讯中断",2771]
[75,"Arm128","CAN通讯恢复",2772]
[75,"Arm129","开入模件异常",2773]
[75,"Arm130","开入配置错",2774]
[75,"Arm131","开入通讯中断",2775]
[75,"Arm132","开出通讯中断",2776]
[75,"Arm133","传动状态未复归",2777]
[75,"Arm134","开入自检回路出错",2778]
[75,"Arm135","开入EEPROM出错",2779]
[75,"Arm136","SRAM自检异常",2780]
[75,"Arm137","FLASH自检异常",2781]
[75,"Arm138","开入异常",2782]
[75,"Arm139","高压1侧CT断线",2783]
[75,"Arm140","高压2侧CT断线",2784]
[75,"Arm141","低压1分支CT断线",2785]
[75,"Arm142","低压2分支CT断线",2786]
[75,"Arm143","差流越限",2787]
[75,"Arm144","高压侧PT断线",2788]
[75,"Arm145","高压侧过负荷",2789]
[75,"Arm146","低1零序过压告警",2790]
[75,"Arm147","低压1分支PT断线",2791]
[75,"Arm148","低压侧过负荷",2792]
[75,"Arm149","低2零序过压告警",2793]
[75,"Arm150","低压2分支PT断线",2794]
[75,"Arm151","电流零漂越限告警",2795]
[75,"Arm152","工作于调试定值区",2796]
[75,"Arm153","低压1分支CT异常",2797]
[75,"Arm154","低压2分支CT异常",2798]
[75,"Arm155","网络状态1",2799]
[75,"Arm156","网络状态2",2800]
[75,"Arm157","装置通讯状态",2801]
[75,"Arm158","检修状态",2802]
[75,"Arm159","参数变化",2803]
[75,"Arm160","就地状态虚遥信",2804]
[75,"Arm161","遥控解除闭锁",2805]
[75,"Arm162","A网中断",2806]
[75,"Arm163","B网中断",2807]
[75,"Arm164","网络中断",2808]
[76,"Arm1","手动录波触发",2809]
[76,"Arm2","远方触发录波",2810]
[76,"Arm3","开入触发录波",2811]
[76,"Arm4","保护板告警触发录波",2812]
[76,"Arm5","保护板闭锁触发录波",2813]
[76,"Arm6","启动板告警触发录波",2814]
[76,"Arm7","启动板闭锁触发录波",2815]
[76,"Arm8","装置闭锁",2816]
[76,"Arm9","定值超范围",2817]
[76,"Arm10","板卡配置错误",2818]
[76,"Arm11","定值项变化告警",2819]
[76,"Arm12","CCD文件错误",2820]
[76,"Arm13","CID文件错误",2821]
[76,"Arm14","保护CPU插件异常",2822]
[76,"Arm15","模拟量采集错",2823]
[76,"Arm16","开出异常",2824]
[76,"Arm17","保护板定值出错",2825]
[76,"Arm18","保护板内存出错",2826]
[76,"Arm19","保护板采样出错",2827]
[76,"Arm20","保护板配置出错",2828]
[76,"Arm21","启动板DSP出错",2829]
[76,"Arm22","保护板长期闭锁告警",2830]
[76,"Arm23","启动板定值出错",2831]
[76,"Arm24","启动板内存出错",2832]
[76,"Arm25","启动板采样出错",2833]
[76,"Arm26","启动板配置出错",2834]
[76,"Arm27","保护板DSP出错",2835]
[76,"Arm28","启动板长期闭锁告警",2836]
[76,"Arm29","B13.跳闸出口异常",2837]
[76,"Arm30","B14.跳闸出口异常",2838]
[76,"Arm31","装置报警",2839]
[76,"Arm32","通信传动报警",2840]
[76,"Arm33","开出传动报警",2841]
[76,"Arm34","对时异常",2842]
[76,"Arm35","版本错误报警",2843]
[76,"Arm36","定值校验出错",2844]
[76,"Arm37","定值区不一致",2845]
[76,"Arm38","定值修改",2846]
[76,"Arm39","定值区切换",2847]
[76,"Arm40","对时信号状态",2848]
[76,"Arm41","对时服务状态",2849]
[76,"Arm42","时间跳变侦测状态",2850]
[76,"Arm43","内存不足",2851]
[76,"Arm44","IEC103配置文件无效",2852]
[76,"Arm45","装置过温告警",2853]
[76,"Arm46","装置低温告警",2854]
[76,"Arm47","装置温度异常告警",2855]
[76,"Arm48","保护板装置电源过压报警",2856]
[76,"Arm49","保护板装置电源低压报警",2857]
[76,"Arm50","保护板装置电源异常报警",2858]
[76,"Arm51","启动板装置电源过压报警",2859]
[76,"Arm52","启动板装置电源低压报警",2860]
[76,"Arm53","启动板装置电源异常报警",2861]
[76,"Arm54","B12.开入电源异常",2862]
[76,"Arm55","B12.板卡异常",2863]
[76,"Arm56","B13.板卡异常",2864]
[76,"Arm57","B14.板卡异常",2865]
[76,"Arm58","B15.信号出口异常",2866]
[76,"Arm59","B15.板卡异常",2867]
[76,"Arm60","运行",2868]
[76,"Arm61","异常",2869]
[76,"Arm62","检修",2870]
[76,"Arm63","差动保护闭锁",2871]
[76,"Arm64","保护跳闸",2872]
[76,"Arm65","闭锁主保护",2873]
[76,"Arm66","闭锁后备保护",2874]
[76,"Arm67","纵差差动速断有效",2875]
[76,"Arm68","纵差保护有效",2876]
[76,"Arm69","纵差变化量保护有效",2877]
[76,"Arm70","高相间阻抗有效",2878]
[76,"Arm71","高接地阻抗有效",2879]
[76,"Arm72","高复流Ⅰ段有效",2880]
[76,"Arm73","高复流Ⅱ段有效",2881]
[76,"Arm74","高复流Ⅲ段有效",2882]
[76,"Arm75","高零流Ⅰ段有效",2883]
[76,"Arm76","高零流Ⅱ段有效",2884]
[76,"Arm77","高零流Ⅲ段有效",2885]
[76,"Arm78","高零序过压有效",2886]
[76,"Arm79","高间隙过流有效",2887]
[76,"Arm80","高失灵联跳有效",2888]
[76,"Arm81","中相间阻抗有效",2889]
[76,"Arm82","中接地阻抗有效",2890]
[76,"Arm83","中复流Ⅰ段有效",2891]
[76,"Arm84","中复流Ⅱ段有效",2892]
[76,"Arm85","中复流Ⅲ段有效",2893]
[76,"Arm86","中零流Ⅰ段有效",2894]
[76,"Arm87","中零流Ⅱ段有效",2895]
[76,"Arm88","中零流Ⅲ段有效",2896]
[76,"Arm89","中间隙过流有效",2897]
[76,"Arm90","中零序过压有效",2898]
[76,"Arm91","中失灵联跳有效",2899]
[76,"Arm92","低1复流Ⅰ段有效",2900]
[76,"Arm93","低1复流Ⅱ段有效",2901]
[76,"Arm94","低2复流Ⅰ段有效",2902]
[76,"Arm95","低2复流Ⅱ段有效",2903]
[76,"Arm96","主保护投入",2904]
[76,"Arm97","高压侧后备保护投入",2905]
[76,"Arm98","中压侧后备保护投入",2906]
[76,"Arm99","低压1分支后备保护投入",2907]
[76,"Arm100","低压2分支后备保护投入",2908]
[76,"Arm101","录波完成",2909]
[76,"Arm102","纵差差动速断保护起动",2910]
[76,"Arm103","纵差比率差动保护起动",2911]
[76,"Arm104","纵差工频变化量差动保护起动",2912]
[76,"Arm105","高压侧阻抗起动",2913]
[76,"Arm106","高压侧复压过流Ⅰ段起动",2914]
[76,"Arm107","高压侧复压过流Ⅱ段起动",2915]
[76,"Arm108","高压侧复压过流Ⅲ段起动",2916]
[76,"Arm109","高压侧零序过流Ⅱ段起动",2917]
[76,"Arm110","高压侧零序过流Ⅲ段起动",2918]
[76,"Arm111","高压侧间隙过流起动",2919]
[76,"Arm112","高压侧间隙保护起动",2920]
[76,"Arm113","高压侧间隙过压起动",2921]
[76,"Arm114","高压侧失灵联跳起动",2922]
[76,"Arm115","中压侧阻抗起动",2923]
[76,"Arm116","中压侧复压过流Ⅰ段起动",2924]
[76,"Arm117","中压侧复压过流Ⅱ段起动",2925]
[76,"Arm118","中压侧复压过流Ⅲ段起动",2926]
[76,"Arm119","中压侧零序过流Ⅲ段起动",2927]
[76,"Arm120","中压侧间隙过流1时限起动",2928]
[76,"Arm121","中压侧间隙保护1时限起动",2929]
[76,"Arm122","中压侧间隙过流2时限起动",2930]
[76,"Arm123","中压侧间隙保护2时限起动",2931]
[76,"Arm124","中压侧间隙过压1时限起动",2932]
[76,"Arm125","中压侧间隙过压2时限起动",2933]
[76,"Arm126","中压侧失灵联跳起动",2934]
[76,"Arm127","低压1分支过流Ⅰ段起动",2935]
[76,"Arm128","低压1分支过流Ⅱ段起动",2936]
[76,"Arm129","低压2分支过流Ⅰ段起动",2937]
[76,"Arm130","低压2分支过流Ⅱ段起动",2938]
[76,"Arm131","高压侧零序过流Ⅰ段起动",2939]
[76,"Arm132","中压侧零序过流Ⅰ段起动",2940]
[76,"Arm133","中压侧零序过流Ⅱ段起动",2941]
[76,"Arm134","跳闸信号",2942]
[76,"Arm135","启动打印",2943]
[76,"Arm136","保护检修状态硬压板",2944]
[76,"Arm137","信号复归",2945]
[76,"Arm138","高压侧电压硬压板",2946]
[76,"Arm139","中压侧电压硬压板",2947]
[76,"Arm140","低压1分支电压硬压板",2948]
[76,"Arm141","低压2分支电压硬压板",2949]
[76,"Arm142","主保护硬压板",2950]
[76,"Arm143","高压侧后备保护硬压板",2951]
[76,"Arm144","中压侧后备保护硬压板",2952]
[76,"Arm145","低压1分支后备保护硬压板",2953]
[76,"Arm146","低压2分支后备保护硬压板",2954]
[76,"Arm147","高压侧失灵联跳开入",2955]
[76,"Arm148","中压侧失灵联跳开入",2956]
[76,"Arm149","远方操作硬压板",2957]
[76,"Arm150","高压侧TWJ",2958]
[76,"Arm151","中压侧TWJ",2959]
[76,"Arm152","纵差差动速断",2960]
[76,"Arm153","纵差保护",2961]
[76,"Arm154","纵差工频变化量差动",2962]
[76,"Arm155","高相间阻抗1时限",2963]
[76,"Arm156","高相间阻抗2时限",2964]
[76,"Arm157","高相间阻抗3时限",2965]
[76,"Arm158","高接地阻抗1时限",2966]
[76,"Arm159","高接地阻抗2时限",2967]
[76,"Arm160","高接地阻抗3时限",2968]
[76,"Arm161","高复流Ⅰ段1时限",2969]
[76,"Arm162","高复流Ⅰ段2时限",2970]
[76,"Arm163","高复流Ⅰ段3时限",2971]
[76,"Arm164","高复流Ⅱ段1时限",2972]
[76,"Arm165","高复流Ⅱ段2时限",2973]
[76,"Arm166","高复流Ⅱ段3时限",2974]
[76,"Arm167","高复流Ⅲ段1时限",2975]
[76,"Arm168","高复流Ⅲ段2时限",2976]
[76,"Arm169","高零流Ⅰ段1时限",2977]
[76,"Arm170","高零流Ⅰ段2时限",2978]
[76,"Arm171","高零流Ⅰ段3时限",2979]
[76,"Arm172","高零流Ⅱ段1时限",2980]
[76,"Arm173","高零流Ⅱ段2时限",2981]
[76,"Arm174","高零流Ⅱ段3时限",2982]
[76,"Arm175","高零流Ⅲ段1时限",2983]
[76,"Arm176","高零流Ⅲ段2时限",2984]
[76,"Arm177","高间隙过流",2985]
[76,"Arm178","高零序过压",2986]
[76,"Arm179","高断路器失灵联跳",2987]
[76,"Arm180","中相间阻抗1时限",2988]
[76,"Arm181","中相间阻抗2时限",2989]
[76,"Arm182","中相间阻抗3时限",2990]
[76,"Arm183","中接地阻抗1时限",2991]
[76,"Arm184","中接地阻抗2时限",2992]
[76,"Arm185","中接地阻抗3时限",2993]
[76,"Arm186","中复流Ⅰ段1时限",2994]
[76,"Arm187","中复流Ⅰ段2时限",2995]
[76,"Arm188","中复流Ⅰ段3时限",2996]
[76,"Arm189","中复流Ⅱ段1时限",2997]
[76,"Arm190","中复流Ⅱ段2时限",2998]
[76,"Arm191","中复流Ⅱ段3时限",2999]
[76,"Arm192","中复流Ⅲ段1时限",3000]
[76,"Arm193","中复流Ⅲ段2时限",3001]
[76,"Arm194","中零流Ⅰ段1时限",3002]
[76,"Arm195","中零流Ⅰ段2时限",3003]
[76,"Arm196","中零流Ⅰ段3时限",3004]
[76,"Arm197","中零流Ⅱ段1时限",3005]
[76,"Arm198","中零流Ⅱ段2时限",3006]
[76,"Arm199","中零流Ⅱ段3时限",3007]
[76,"Arm200","中零流Ⅲ段1时限",3008]
[76,"Arm201","中零流Ⅲ段2时限",3009]
[76,"Arm202","中间隙过流1时限",3010]
[76,"Arm203","中间隙过流2时限",3011]
[76,"Arm204","中零序过压1时限",3012]
[76,"Arm205","中零序过压2时限",3013]
[76,"Arm206","中断路器失灵联跳",3014]
[76,"Arm207","低1复流Ⅰ段1时限",3015]
[76,"Arm208","低1复流Ⅰ段2时限",3016]
[76,"Arm209","低1复流Ⅰ段3时限",3017]
[76,"Arm210","低1复流Ⅱ段1时限",3018]
[76,"Arm211","低1复流Ⅱ段2时限",3019]
[76,"Arm212","低1复流Ⅱ段3时限",3020]
[76,"Arm213","低2复流Ⅰ段1时限",3021]
[76,"Arm214","低2复流Ⅰ段2时限",3022]
[76,"Arm215","低2复流Ⅰ段3时限",3023]
[76,"Arm216","低2复流Ⅱ段1时限",3024]
[76,"Arm217","低2复流Ⅱ段2时限",3025]
[76,"Arm218","低2复流Ⅱ段3时限",3026]
[76,"Arm219","跳高压侧",3027]
[76,"Arm220","跳高压侧母联",3028]
[76,"Arm221","跳中压侧",3029]
[76,"Arm222","跳中压侧母联",3030]
[76,"Arm223","跳低压1分支",3031]
[76,"Arm224","跳低压1分段",3032]
[76,"Arm225","跳低压2分支",3033]
[76,"Arm226","跳低压2分段",3034]
[76,"Arm227","闭锁中压侧备自投",3035]
[76,"Arm228","闭锁低压1分支备自投",3036]
[76,"Arm229","闭锁低压2分支备自投",3037]
[76,"Arm230","跳备用出口1~4",3038]
[76,"Arm231","保护启动",3039]
[76,"Arm232","高压侧过负荷",3040]
[76,"Arm233","中压侧过负荷",3041]
[76,"Arm234","低压1分支零序过压报警",3042]
[76,"Arm235","低压2分支零序过压报警",3043]
[76,"Arm236","低压侧过负荷",3044]
[76,"Arm237","失灵开入异常",3045]
[76,"Arm238","高压1侧CT异常",3046]
[76,"Arm239","高压1侧CT断线",3047]
[76,"Arm240","高压2侧CT异常",3048]
[76,"Arm241","高压2侧CT断线",3049]
[76,"Arm242","中压侧CT异常",3050]
[76,"Arm243","中压侧CT断线",3051]
[76,"Arm244","低压1分支CT异常",3052]
[76,"Arm245","低压1分支CT断线",3053]
[76,"Arm246","低压2分支CT异常",3054]
[76,"Arm247","低压2分支CT断线",3055]
[76,"Arm248","高压侧PT断线",3056]
[76,"Arm249","中压侧PT断线",3057]
[76,"Arm250","低压1分支PT断线",3058]
[76,"Arm251","低压2分支PT断线",3059]
[76,"Arm252","频率异常告警",3060]
[76,"Arm253","差流越限",3061]
[76,"Arm254","纵差回路断线告警",3062]
[76,"Arm255","高压侧失灵联跳节点告警",3063]
[76,"Arm256","高压侧失灵联跳电流告警",3064]
[76,"Arm257","中压侧失灵联跳节点告警",3065]
[76,"Arm258","中压侧失灵联跳电流告警",3066]
[76,"Arm259","保护板长期启动",3067]
[76,"Arm260","启动板长期启动",3068]
[76,"Arm261","主保护软压板",3069]
[76,"Arm262","高压侧后备保护软压板",3070]
[76,"Arm263","中压侧后备保护软压板",3071]
[76,"Arm264","低压1分支后备保护软压板",3072]
[76,"Arm265","低压2分支后备保护软压板",3073]
[76,"Arm266","远方投退压板软压板",3074]
[76,"Arm267","远方切换定值区软压板",3075]
[76,"Arm268","远方修改定值软压板",3076]
[76,"Arm269","网络状态1",3077]
[76,"Arm270","网络状态2",3078]
[76,"Arm271","装置通讯状态",3079]
[76,"Arm272","检修状态",3080]
[76,"Arm273","参数变化",3081]
[76,"Arm274","就地状态虚遥信",3082]
[76,"Arm275","遥控解除闭锁",3083]
[76,"Arm276","A网中断",3084]
[76,"Arm277","B网中断",3085]
[76,"Arm278","网络中断",3086]
[77,"Arm1","模拟量采集错",3087]
[77,"Arm2","跳闸失败",3088]
[77,"Arm3","设备参数错",3089]
[77,"Arm4","ROM和校验错",3090]
[77,"Arm5","定值错",3091]
[77,"Arm6","定值区指针错",3092]
[77,"Arm7","开出不响应",3093]
[77,"Arm8","开出击穿",3094]
[77,"Arm9","压板模式未确认",3095]
[77,"Arm10","SRAM自检异常",3096]
[77,"Arm11","FLASH自检异常",3097]
[77,"Arm12","自描述错",3098]
[77,"Arm13","开入状态未复归",3099]
[77,"Arm14","软压板错",3100]
[77,"Arm15","系统配置错",3101]
[77,"Arm16","CAN通讯中断",3102]
[77,"Arm17","CAN通讯恢复",3103]
[77,"Arm18","开入模件异常",3104]
[77,"Arm19","开出模件异常",3105]
[77,"Arm20","开入配置错",3106]
[77,"Arm21","开出配置错",3107]
[77,"Arm22","开入通讯中断",3108]
[77,"Arm23","开出通讯中断",3109]
[77,"Arm24","传动状态未复归",3110]
[77,"Arm25","开入击穿",3111]
[77,"Arm26","开入输入不正常",3112]
[77,"Arm27","双位置输入不一致",3113]
[77,"Arm28","开入自检回路出错",3114]
[77,"Arm29","开入EEPROM出错",3115]
[77,"Arm30","开出EEPROM出错",3116]
[77,"Arm31","X12-a6输入3T1",3117]
[77,"Arm32","X12-a6输入3T2",3118]
[77,"Arm33","X12-a6输入3T3",3119]
[77,"Arm34","X12-a6输入3",3120]
[77,"Arm35","X12-c6输入4",3121]
[77,"Arm36","X12-a4输入1",3122]
[77,"Arm37","X12-c4输入2",3123]
[77,"Arm38","X3-a4输入1",3124]
[77,"Arm39","X3-c4输入2",3125]
[77,"Arm40","X3-a6输入3",3126]
[77,"Arm41","X3-c6输入4",3127]
[77,"Arm42","X4-a4输入1",3128]
[77,"Arm43","X4-c4输入2",3129]
[77,"Arm44","X4-a6输入3",3130]
[77,"Arm45","X4-c6输入4",3131]
[77,"Arm46","X5-a4输入1",3132]
[77,"Arm47","X5-c4输入2",3133]
[77,"Arm48","X5-a6输入3",3134]
[77,"Arm49","X5-c6输入4",3135]
[77,"Arm50","X13-a4输入1",3136]
[77,"Arm51","X13-c4输入2",3137]
[77,"Arm52","X13-a6输入3",3138]
[77,"Arm53","X13-c6输入4",3139]
[77,"Arm54","CPU异常",3140]
[77,"Arm55","设备参数不一致",3141]
[77,"Arm56","定值区号不一致",3142]
[77,"Arm57","定值不一致",3143]
[77,"Arm58","压板不一致",3144]
[77,"Arm59","LON1通讯中断",3145]
[77,"Arm60","LON2通讯中断",3146]
[77,"Arm61","压板模式不一致",3147]
[77,"Arm62","召唤配置无应答",3148]
[77,"Arm63","PLC逻辑校验出错",3149]
[77,"Arm64","信号复归",3150]
[77,"Arm65","X12-a6输入3_(重复1)",3151]
[77,"Arm66","X12-c6输入4_(重复1)",3152]
[77,"Arm67","X12-a4输入1_(重复1)",3153]
[77,"Arm68","X12-c4输入2_(重复1)",3154]
[77,"Arm69","X3-a4输入1_(重复1)",3155]
[77,"Arm70","X3-c4输入2_(重复1)",3156]
[77,"Arm71","X3-a6输入3_(重复1)",3157]
[77,"Arm72","X3-c6输入4_(重复1)",3158]
[77,"Arm73","X4-a4输入1_(重复1)",3159]
[77,"Arm74","X4-c4输入2_(重复1)",3160]
[77,"Arm75","X4-a6输入3_(重复1)",3161]
[77,"Arm76","X4-c6输入4_(重复1)",3162]
[77,"Arm77","X5-a4输入1_(重复1)",3163]
[77,"Arm78","X5-c4输入2_(重复1)",3164]
[77,"Arm79","X5-a6输入3_(重复1)",3165]
[77,"Arm80","X5-c6输入4_(重复1)",3166]
[77,"Arm81","X13-a4输入1_(重复1)",3167]
[77,"Arm82","X13-c4输入2_(重复1)",3168]
[77,"Arm83","X13-a6输入3_(重复1)",3169]
[77,"Arm84","X13-c6输入4_(重复1)",3170]
[77,"Arm85","检修状态压板",3171]
[77,"Arm86","远方修改定值",3172]
[77,"Arm87","保护启动",3173]
[77,"Arm88","X3-a4输入1_(重复2)",3174]
[77,"Arm89","X3-c4输入2_(重复2)",3175]
[77,"Arm90","X3-a6输入3_(重复2)",3176]
[77,"Arm91","X3-c6输入4_(重复2)",3177]
[77,"Arm92","X4-a4输入1_(重复2)",3178]
[77,"Arm93","X4-c4输入2_(重复2)",3179]
[77,"Arm94","X4-a6输入3_(重复2)",3180]
[77,"Arm95","X4-c6输入4_(重复2)",3181]
[77,"Arm96","X5-a4输入1_(重复2)",3182]
[77,"Arm97","X5-c4输入2_(重复2)",3183]
[77,"Arm98","X5-a6输入3_(重复2)",3184]
[77,"Arm99","X5-c6输入4_(重复2)",3185]
[77,"Arm100","X13-a4输入1_(重复2)",3186]
[77,"Arm101","X13-c4输入2_(重复2)",3187]
[77,"Arm102","X13-a6输入3_(重复2)",3188]
[77,"Arm103","X13-c6输入4_(重复2)",3189]
[77,"Arm104","X12-a6输入3T1_(重复1)",3190]
[77,"Arm105","X12-a6输入3T2_(重复1)",3191]
[77,"Arm106","X12-a6输入3T3_(重复1)",3192]
[77,"Arm107","X12-a6输入3_(重复2)",3193]
[77,"Arm108","X12-c6输入4_(重复2)",3194]
[77,"Arm109","X12-a4输入1_(重复2)",3195]
[77,"Arm110","X12-c4输入2_(重复2)",3196]
[77,"Arm111","录波完成",3197]
[77,"Arm112","录波启动",3198]
[77,"Arm113","网络状态1",3199]
[77,"Arm114","网络状态2",3200]
[77,"Arm115","装置通讯状态",3201]
[77,"Arm116","检修状态",3202]
[77,"Arm117","参数变化",3203]
[77,"Arm118","就地状态虚遥信",3204]
[77,"Arm119","遥控解除闭锁",3205]
[77,"Arm120","A网中断",3206]
[77,"Arm121","B网中断",3207]
[77,"Arm122","网络中断",3208]
[78,"Arm1","I类告警总",3209]
[78,"Arm2","模拟量采集错",3210]
[78,"Arm3","ROM和校验错",3211]
[78,"Arm4","定值错",3212]
[78,"Arm5","定值区指针错",3213]
[78,"Arm6","开出不响应",3214]
[78,"Arm7","开出击穿",3215]
[78,"Arm8","设备参数错",3216]
[78,"Arm9","软压板错",3217]
[78,"Arm10","系统配置错",3218]
[78,"Arm11","开出模件异常",3219]
[78,"Arm12","开出配置错",3220]
[78,"Arm13","开出EEPROM出错",3221]
[78,"Arm14","保护CPU插件异常",3222]
[78,"Arm15","开出异常",3223]
[78,"Arm16","CPU通讯中断",3224]
[78,"Arm17","设备参数不一致",3225]
[78,"Arm18","定值区号不一致",3226]
[78,"Arm19","定值不一致",3227]
[78,"Arm20","压板不一致",3228]
[78,"Arm21","召唤配置无应答",3229]
[78,"Arm22","对时异常",3230]
[78,"Arm23","面板配置不一致",3231]
[78,"Arm24","对时信号状态",3232]
[78,"Arm25","对时服务状态",3233]
[78,"Arm26","时间跳变侦测状态",3234]
[78,"Arm27","主保护硬压板",3235]
[78,"Arm28","高压侧后备保护硬压板",3236]
[78,"Arm29","高压侧电压硬压板",3237]
[78,"Arm30","低压1分支后备保护硬压板",3238]
[78,"Arm31","低压1分支电压硬压板",3239]
[78,"Arm32","低压2分支后备保护硬压板",3240]
[78,"Arm33","低压2分支电压硬压板",3241]
[78,"Arm34","远方操作硬压板",3242]
[78,"Arm35","保护检修状态硬压板",3243]
[78,"Arm36","主保护总压板",3244]
[78,"Arm37","高压侧后备保护总压板",3245]
[78,"Arm38","低压1分支后备保护总压板",3246]
[78,"Arm39","低压2分支后备保护总压板",3247]
[78,"Arm40","运行",3248]
[78,"Arm41","异常",3249]
[78,"Arm42","检修",3250]
[78,"Arm43","差动保护闭锁",3251]
[78,"Arm44","保护跳闸",3252]
[78,"Arm45","纵差差动速断有效",3253]
[78,"Arm46","纵差变化量差动有效",3254]
[78,"Arm47","纵差保护有效",3255]
[78,"Arm48","高相间阻抗有效",3256]
[78,"Arm49","高接地阻抗有效",3257]
[78,"Arm50","高复流Ⅰ段有效",3258]
[78,"Arm51","高复流Ⅱ段有效",3259]
[78,"Arm52","高复流Ⅲ段有效",3260]
[78,"Arm53","高零流Ⅰ段有效",3261]
[78,"Arm54","高零流Ⅱ段有效",3262]
[78,"Arm55","高零流Ⅲ段有效",3263]
[78,"Arm56","高失灵联跳有效",3264]
[78,"Arm57","高间隙过流有效",3265]
[78,"Arm58","高零序过压有效",3266]
[78,"Arm59","低1复流Ⅰ段有效",3267]
[78,"Arm60","低1复流Ⅱ段有效",3268]
[78,"Arm61","低2复流Ⅰ段有效",3269]
[78,"Arm62","低2复流Ⅱ段有效",3270]
[78,"Arm63","闭锁主保护",3271]
[78,"Arm64","闭锁后备保护",3272]
[78,"Arm65","主保护投入",3273]
[78,"Arm66","高压侧后备保护投入",3274]
[78,"Arm67","低压1分支后备保护投入",3275]
[78,"Arm68","低压2分支后备保护投入",3276]
[78,"Arm69","录波完成",3277]
[78,"Arm70","录波启动",3278]
[78,"Arm71","主保护软压板",3279]
[78,"Arm72","高压侧后备保护软压板",3280]
[78,"Arm73","低压1分支后备保护软压板",3281]
[78,"Arm74","低压2分支后备保护软压板",3282]
[78,"Arm75","远方投退压板软压板",3283]
[78,"Arm76","远方切换定值区软压板",3284]
[78,"Arm77","远方修改定值软压板",3285]
[78,"Arm78","高压侧失灵联跳开入",3286]
[78,"Arm79","信号复归",3287]
[78,"Arm80","保护动作",3288]
[78,"Arm81","保护启动",3289]
[78,"Arm82","纵差保护",3290]
[78,"Arm83","纵差差动速断",3291]
[78,"Arm84","高相间阻抗1时限",3292]
[78,"Arm85","高相间阻抗2时限",3293]
[78,"Arm86","高相间阻抗3时限",3294]
[78,"Arm87","高接地阻抗1时限",3295]
[78,"Arm88","高接地阻抗2时限",3296]
[78,"Arm89","高接地阻抗3时限",3297]
[78,"Arm90","高复流Ⅰ段1时限",3298]
[78,"Arm91","低1复流Ⅰ段1时限",3299]
[78,"Arm92","低2复流Ⅰ段1时限",3300]
[78,"Arm93","高复流Ⅰ段2时限",3301]
[78,"Arm94","高复流Ⅰ段3时限",3302]
[78,"Arm95","高复流Ⅱ段2时限",3303]
[78,"Arm96","高复流Ⅱ段3时限",3304]
[78,"Arm97","高复流Ⅲ段2时限",3305]
[78,"Arm98","低1复流Ⅰ段2时限",3306]
[78,"Arm99","低1复流Ⅰ段3时限",3307]
[78,"Arm100","低1复流Ⅱ段2时限",3308]
[78,"Arm101","低1复流Ⅱ段3时限",3309]
[78,"Arm102","低2复流Ⅰ段2时限",3310]
[78,"Arm103","低2复流Ⅰ段3时限",3311]
[78,"Arm104","低2复流Ⅱ段2时限",3312]
[78,"Arm105","低2复流Ⅱ段3时限",3313]
[78,"Arm106","高复流Ⅱ段1时限",3314]
[78,"Arm107","高复流Ⅲ段1时限",3315]
[78,"Arm108","低1复流Ⅱ段1时限",3316]
[78,"Arm109","低2复流Ⅱ段1时限",3317]
[78,"Arm110","高零流Ⅰ段1时限",3318]
[78,"Arm111","高零流Ⅱ段1时限",3319]
[78,"Arm112","高零流Ⅰ段2时限",3320]
[78,"Arm113","高零流Ⅰ段3时限",3321]
[78,"Arm114","高零流Ⅱ段2时限",3322]
[78,"Arm115","高零流Ⅱ段3时限",3323]
[78,"Arm116","高零流Ⅲ段2时限",3324]
[78,"Arm117","高间隙过流",3325]
[78,"Arm118","高零流Ⅲ段1时限",3326]
[78,"Arm119","高零序过压",3327]
[78,"Arm120","高断路器失灵联跳",3328]
[78,"Arm121","故障分量差动",3329]
[78,"Arm122","II类告警总",3330]
[78,"Arm123","开入击穿",3331]
[78,"Arm124","开入输入不正常",3332]
[78,"Arm125","双位置输入不一致",3333]
[78,"Arm126","失灵开入异常",3334]
[78,"Arm127","CAN通讯中断",3335]
[78,"Arm128","CAN通讯恢复",3336]
[78,"Arm129","开入模件异常",3337]
[78,"Arm130","开入配置错",3338]
[78,"Arm131","开入通讯中断",3339]
[78,"Arm132","开出通讯中断",3340]
[78,"Arm133","传动状态未复归",3341]
[78,"Arm134","开入自检回路出错",3342]
[78,"Arm135","开入EEPROM出错",3343]
[78,"Arm136","SRAM自检异常",3344]
[78,"Arm137","FLASH自检异常",3345]
[78,"Arm138","开入异常",3346]
[78,"Arm139","高压1侧CT断线",3347]
[78,"Arm140","高压2侧CT断线",3348]
[78,"Arm141","低压1分支CT断线",3349]
[78,"Arm142","低压2分支CT断线",3350]
[78,"Arm143","差流越限",3351]
[78,"Arm144","高压侧PT断线",3352]
[78,"Arm145","高压侧过负荷",3353]
[78,"Arm146","低1零序过压告警",3354]
[78,"Arm147","低压1分支PT断线",3355]
[78,"Arm148","低压侧过负荷",3356]
[78,"Arm149","低2零序过压告警",3357]
[78,"Arm150","低压2分支PT断线",3358]
[78,"Arm151","电流零漂越限告警",3359]
[78,"Arm152","工作于调试定值区",3360]
[78,"Arm153","低压1分支CT异常",3361]
[78,"Arm154","低压2分支CT异常",3362]
[78,"Arm155","网络状态1",3363]
[78,"Arm156","网络状态2",3364]
[78,"Arm157","装置通讯状态",3365]
[78,"Arm158","检修状态",3366]
[78,"Arm159","参数变化",3367]
[78,"Arm160","就地状态虚遥信",3368]
[78,"Arm161","遥控解除闭锁",3369]
[78,"Arm162","A网中断",3370]
[78,"Arm163","B网中断",3371]
[78,"Arm164","网络中断",3372]
[79,"Arm1","手动录波触发",3373]
[79,"Arm2","远方触发录波",3374]
[79,"Arm3","开入触发录波",3375]
[79,"Arm4","保护板告警触发录波",3376]
[79,"Arm5","保护板闭锁触发录波",3377]
[79,"Arm6","启动板告警触发录波",3378]
[79,"Arm7","启动板闭锁触发录波",3379]
[79,"Arm8","装置闭锁",3380]
[79,"Arm9","定值超范围",3381]
[79,"Arm10","板卡配置错误",3382]
[79,"Arm11","定值项变化告警",3383]
[79,"Arm12","CCD文件错误",3384]
[79,"Arm13","CID文件错误",3385]
[79,"Arm14","保护CPU插件异常",3386]
[79,"Arm15","模拟量采集错",3387]
[79,"Arm16","开出异常",3388]
[79,"Arm17","保护板定值出错",3389]
[79,"Arm18","保护板内存出错",3390]
[79,"Arm19","保护板采样出错",3391]
[79,"Arm20","保护板配置出错",3392]
[79,"Arm21","启动板DSP出错",3393]
[79,"Arm22","保护板长期闭锁告警",3394]
[79,"Arm23","启动板定值出错",3395]
[79,"Arm24","启动板内存出错",3396]
[79,"Arm25","启动板采样出错",3397]
[79,"Arm26","启动板配置出错",3398]
[79,"Arm27","保护板DSP出错",3399]
[79,"Arm28","启动板长期闭锁告警",3400]
[79,"Arm29","B13.跳闸出口异常",3401]
[79,"Arm30","B14.跳闸出口异常",3402]
[79,"Arm31","装置报警",3403]
[79,"Arm32","通信传动报警",3404]
[79,"Arm33","开出传动报警",3405]
[79,"Arm34","对时异常",3406]
[79,"Arm35","装置过温告警",3407]
[79,"Arm36","定值校验出错",3408]
[79,"Arm37","定值区不一致",3409]
[79,"Arm38","定值修改",3410]
[79,"Arm39","定值区切换",3411]
[79,"Arm40","对时信号状态",3412]
[79,"Arm41","对时服务状态",3413]
[79,"Arm42","时间跳变侦测状态",3414]
[79,"Arm43","内存不足",3415]
[79,"Arm44","IEC103配置文件无效",3416]
[79,"Arm45","装置过温告警",3417]
[79,"Arm46","装置低温告警",3418]
[79,"Arm47","装置温度异常告警",3419]
[79,"Arm48","保护板装置电源过压报警",3420]
[79,"Arm49","保护板装置电源低压报警",3421]
[79,"Arm50","保护板装置电源异常报警",3422]
[79,"Arm51","启动板装置电源过压报警",3423]
[79,"Arm52","启动板装置电源低压报警",3424]
[79,"Arm53","启动板装置电源异常报警",3425]
[79,"Arm54","B12.开入电源异常",3426]
[79,"Arm55","B12.板卡异常",3427]
[79,"Arm56","B13.板卡异常",3428]
[79,"Arm57","B14.板卡异常",3429]
[79,"Arm58","B15.信号出口异常",3430]
[79,"Arm59","B15.板卡异常",3431]
[79,"Arm60","运行",3432]
[79,"Arm61","异常",3433]
[79,"Arm62","检修",3434]
[79,"Arm63","差动保护闭锁",3435]
[79,"Arm64","保护跳闸",3436]
[79,"Arm65","闭锁主保护",3437]
[79,"Arm66","闭锁后备保护",3438]
[79,"Arm67","纵差差动速断有效",3439]
[79,"Arm68","纵差保护有效",3440]
[79,"Arm69","纵差变化量保护有效",3441]
[79,"Arm70","高相间阻抗有效",3442]
[79,"Arm71","高接地阻抗有效",3443]
[79,"Arm72","高复流Ⅰ段有效",3444]
[79,"Arm73","高复流Ⅱ段有效",3445]
[79,"Arm74","高复流Ⅲ段有效",3446]
[79,"Arm75","高零流Ⅰ段有效",3447]
[79,"Arm76","高零流Ⅱ段有效",3448]
[79,"Arm77","高零流Ⅲ段有效",3449]
[79,"Arm78","高零序过压有效",3450]
[79,"Arm79","高间隙过流有效",3451]
[79,"Arm80","高失灵联跳有效",3452]
[79,"Arm81","中相间阻抗有效",3453]
[79,"Arm82","中接地阻抗有效",3454]
[79,"Arm83","中复流Ⅰ段有效",3455]
[79,"Arm84","中复流Ⅱ段有效",3456]
[79,"Arm85","中复流Ⅲ段有效",3457]
[79,"Arm86","中零流Ⅰ段有效",3458]
[79,"Arm87","中零流Ⅱ段有效",3459]
[79,"Arm88","中零流Ⅲ段有效",3460]
[79,"Arm89","中间隙过流有效",3461]
[79,"Arm90","中零序过压有效",3462]
[79,"Arm91","中失灵联跳有效",3463]
[79,"Arm92","低1复流Ⅰ段有效",3464]
[79,"Arm93","低1复流Ⅱ段有效",3465]
[79,"Arm94","低2复流Ⅰ段有效",3466]
[79,"Arm95","低2复流Ⅱ段有效",3467]
[79,"Arm96","主保护投入",3468]
[79,"Arm97","高压侧后备保护投入",3469]
[79,"Arm98","中压侧后备保护投入",3470]
[79,"Arm99","低压1分支后备保护投入",3471]
[79,"Arm100","低压2分支后备保护投入",3472]
[79,"Arm101","录波完成",3473]
[79,"Arm102","纵差差动速断保护起动",3474]
[79,"Arm103","纵差比率差动保护起动",3475]
[79,"Arm104","纵差工频变化量差动保护起动",3476]
[79,"Arm105","高压侧阻抗起动",3477]
[79,"Arm106","高压侧复压过流Ⅰ段起动",3478]
[79,"Arm107","高压侧复压过流Ⅱ段起动",3479]
[79,"Arm108","高压侧复压过流Ⅲ段起动",3480]
[79,"Arm109","高压侧零序过流Ⅱ段起动",3481]
[79,"Arm110","高压侧零序过流Ⅲ段起动",3482]
[79,"Arm111","高压侧间隙过流起动",3483]
[79,"Arm112","高压侧间隙保护起动",3484]
[79,"Arm113","高压侧间隙过压起动",3485]
[79,"Arm114","高压侧失灵联跳起动",3486]
[79,"Arm115","中压侧阻抗起动",3487]
[79,"Arm116","中压侧复压过流Ⅰ段起动",3488]
[79,"Arm117","中压侧复压过流Ⅱ段起动",3489]
[79,"Arm118","中压侧复压过流Ⅲ段起动",3490]
[79,"Arm119","中压侧零序过流Ⅲ段起动",3491]
[79,"Arm120","中压侧间隙过流1时限起动",3492]
[79,"Arm121","中压侧间隙保护1时限起动",3493]
[79,"Arm122","中压侧间隙过流2时限起动",3494]
[79,"Arm123","中压侧间隙保护2时限起动",3495]
[79,"Arm124","中压侧间隙过压1时限起动",3496]
[79,"Arm125","中压侧间隙过压2时限起动",3497]
[79,"Arm126","中压侧失灵联跳起动",3498]
[79,"Arm127","低压1分支过流Ⅰ段起动",3499]
[79,"Arm128","低压1分支过流Ⅱ段起动",3500]
[79,"Arm129","低压2分支过流Ⅰ段起动",3501]
[79,"Arm130","低压2分支过流Ⅱ段起动",3502]
[79,"Arm131","高压侧零序过流Ⅰ段起动",3503]
[79,"Arm132","中压侧零序过流Ⅰ段起动",3504]
[79,"Arm133","中压侧零序过流Ⅱ段起动",3505]
[79,"Arm134","跳闸信号",3506]
[79,"Arm135","启动打印",3507]
[79,"Arm136","保护检修状态硬压板",3508]
[79,"Arm137","信号复归",3509]
[79,"Arm138","高压侧电压硬压板",3510]
[79,"Arm139","中压侧电压硬压板",3511]
[79,"Arm140","低压1分支电压硬压板",3512]
[79,"Arm141","低压2分支电压硬压板",3513]
[79,"Arm142","主保护硬压板",3514]
[79,"Arm143","高压侧后备保护硬压板",3515]
[79,"Arm144","中压侧后备保护硬压板",3516]
[79,"Arm145","低压1分支后备保护硬压板",3517]
[79,"Arm146","低压2分支后备保护硬压板",3518]
[79,"Arm147","高压侧失灵联跳开入",3519]
[79,"Arm148","中压侧失灵联跳开入",3520]
[79,"Arm149","远方操作硬压板",3521]
[79,"Arm150","高压侧TWJ",3522]
[79,"Arm151","中压侧TWJ",3523]
[79,"Arm152","纵差差动速断",3524]
[79,"Arm153","纵差保护",3525]
[79,"Arm154","纵差工频变化量差动",3526]
[79,"Arm155","高相间阻抗1时限",3527]
[79,"Arm156","高相间阻抗2时限",3528]
[79,"Arm157","高相间阻抗3时限",3529]
[79,"Arm158","高接地阻抗1时限",3530]
[79,"Arm159","高接地阻抗2时限",3531]
[79,"Arm160","高接地阻抗3时限",3532]
[79,"Arm161","高复流Ⅰ段1时限",3533]
[79,"Arm162","高复流Ⅰ段2时限",3534]
[79,"Arm163","高复流Ⅰ段3时限",3535]
[79,"Arm164","高复流Ⅱ段1时限",3536]
[79,"Arm165","高复流Ⅱ段2时限",3537]
[79,"Arm166","高复流Ⅱ段3时限",3538]
[79,"Arm167","高复流Ⅲ段1时限",3539]
[79,"Arm168","高复流Ⅲ段2时限",3540]
[79,"Arm169","高零流Ⅰ段1时限",3541]
[79,"Arm170","高零流Ⅰ段2时限",3542]
[79,"Arm171","高零流Ⅰ段3时限",3543]
[79,"Arm172","高零流Ⅱ段1时限",3544]
[79,"Arm173","高零流Ⅱ段2时限",3545]
[79,"Arm174","高零流Ⅱ段3时限",3546]
[79,"Arm175","高零流Ⅲ段1时限",3547]
[79,"Arm176","高零流Ⅲ段2时限",3548]
[79,"Arm177","高间隙过流",3549]
[79,"Arm178","高零序过压",3550]
[79,"Arm179","高断路器失灵联跳",3551]
[79,"Arm180","中相间阻抗1时限",3552]
[79,"Arm181","中相间阻抗2时限",3553]
[79,"Arm182","中相间阻抗3时限",3554]
[79,"Arm183","中接地阻抗1时限",3555]
[79,"Arm184","中接地阻抗2时限",3556]
[79,"Arm185","中接地阻抗3时限",3557]
[79,"Arm186","中复流Ⅰ段1时限",3558]
[79,"Arm187","中复流Ⅰ段2时限",3559]
[79,"Arm188","中复流Ⅰ段3时限",3560]
[79,"Arm189","中复流Ⅱ段1时限",3561]
[79,"Arm190","中复流Ⅱ段2时限",3562]
[79,"Arm191","中复流Ⅱ段3时限",3563]
[79,"Arm192","中复流Ⅲ段1时限",3564]
[79,"Arm193","中复流Ⅲ段2时限",3565]
[79,"Arm194","中零流Ⅰ段1时限",3566]
[79,"Arm195","中零流Ⅰ段2时限",3567]
[79,"Arm196","中零流Ⅰ段3时限",3568]
[79,"Arm197","中零流Ⅱ段1时限",3569]
[79,"Arm198","中零流Ⅱ段2时限",3570]
[79,"Arm199","中零流Ⅱ段3时限",3571]
[79,"Arm200","中零流Ⅲ段1时限",3572]
[79,"Arm201","中零流Ⅲ段2时限",3573]
[79,"Arm202","中间隙过流1时限",3574]
[79,"Arm203","中间隙过流2时限",3575]
[79,"Arm204","中零序过压1时限",3576]
[79,"Arm205","中零序过压2时限",3577]
[79,"Arm206","中断路器失灵联跳",3578]
[79,"Arm207","低1复流Ⅰ段1时限",3579]
[79,"Arm208","低1复流Ⅰ段2时限",3580]
[79,"Arm209","低1复流Ⅰ段3时限",3581]
[79,"Arm210","低1复流Ⅱ段1时限",3582]
[79,"Arm211","低1复流Ⅱ段2时限",3583]
[79,"Arm212","低1复流Ⅱ段3时限",3584]
[79,"Arm213","低2复流Ⅰ段1时限",3585]
[79,"Arm214","低2复流Ⅰ段2时限",3586]
[79,"Arm215","低2复流Ⅰ段3时限",3587]
[79,"Arm216","低2复流Ⅱ段1时限",3588]
[79,"Arm217","低2复流Ⅱ段2时限",3589]
[79,"Arm218","低2复流Ⅱ段3时限",3590]
[79,"Arm219","跳高压侧",3591]
[79,"Arm220","跳高压侧母联",3592]
[79,"Arm221","跳中压侧",3593]
[79,"Arm222","跳中压侧母联",3594]
[79,"Arm223","跳低压1分支",3595]
[79,"Arm224","跳低压1分段",3596]
[79,"Arm225","跳低压2分支",3597]
[79,"Arm226","跳低压2分段",3598]
[79,"Arm227","闭锁中压侧备自投",3599]
[79,"Arm228","闭锁低压1分支备自投",3600]
[79,"Arm229","闭锁低压2分支备自投",3601]
[79,"Arm230","跳备用出口1~4",3602]
[79,"Arm231","保护启动",3603]
[79,"Arm232","高压侧过负荷",3604]
[79,"Arm233","中压侧过负荷",3605]
[79,"Arm234","低压1分支零序过压报警",3606]
[79,"Arm235","低压2分支零序过压报警",3607]
[79,"Arm236","低压侧过负荷",3608]
[79,"Arm237","失灵开入异常",3609]
[79,"Arm238","高压1侧CT异常",3610]
[79,"Arm239","高压1侧CT断线",3611]
[79,"Arm240","高压2侧CT异常",3612]
[79,"Arm241","高压2侧CT断线",3613]
[79,"Arm242","中压侧CT异常",3614]
[79,"Arm243","中压侧CT断线",3615]
[79,"Arm244","低压1分支CT异常",3616]
[79,"Arm245","低压1分支CT断线",3617]
[79,"Arm246","低压2分支CT异常",3618]
[79,"Arm247","低压2分支CT断线",3619]
[79,"Arm248","高压侧PT断线",3620]
[79,"Arm249","中压侧PT断线",3621]
[79,"Arm250","低压1分支PT断线",3622]
[79,"Arm251","低压2分支PT断线",3623]
[79,"Arm252","频率异常告警",3624]
[79,"Arm253","差流越限",3625]
[79,"Arm254","纵差回路断线告警",3626]
[79,"Arm255","高压侧失灵联跳节点告警",3627]
[79,"Arm256","高压侧失灵联跳电流告警",3628]
[79,"Arm257","中压侧失灵联跳节点告警",3629]
[79,"Arm258","中压侧失灵联跳电流告警",3630]
[79,"Arm259","保护板长期启动",3631]
[79,"Arm260","启动板长期启动",3632]
[79,"Arm261","主保护软压板",3633]
[79,"Arm262","高压侧后备保护软压板",3634]
[79,"Arm263","中压侧后备保护软压板",3635]
[79,"Arm264","低压1分支后备保护软压板",3636]
[79,"Arm265","低压2分支后备保护软压板",3637]
[79,"Arm266","远方投退压板软压板",3638]
[79,"Arm267","远方切换定值区软压板",3639]
[79,"Arm268","远方修改定值软压板",3640]
[79,"Arm269","网络状态1",3641]
[79,"Arm270","网络状态2",3642]
[79,"Arm271","装置通讯状态",3643]
[79,"Arm272","检修状态",3644]
[79,"Arm273","参数变化",3645]
[79,"Arm274","就地状态虚遥信",3646]
[79,"Arm275","遥控解除闭锁",3647]
[79,"Arm276","A网中断",3648]
[79,"Arm277","B网中断",3649]
[79,"Arm278","网络中断",3650]
[80,"Arm1","模拟量采集错",3651]
[80,"Arm2","跳闸失败",3652]
[80,"Arm3","设备参数错",3653]
[80,"Arm4","ROM和校验错",3654]
[80,"Arm5","定值错",3655]
[80,"Arm6","定值区指针错",3656]
[80,"Arm7","开出不响应",3657]
[80,"Arm8","开出击穿",3658]
[80,"Arm9","压板模式未确认",3659]
[80,"Arm10","SRAM自检异常",3660]
[80,"Arm11","FLASH自检异常",3661]
[80,"Arm12","自描述错",3662]
[80,"Arm13","开入状态未复归",3663]
[80,"Arm14","软压板错",3664]
[80,"Arm15","系统配置错",3665]
[80,"Arm16","CAN通讯中断",3666]
[80,"Arm17","CAN通讯恢复",3667]
[80,"Arm18","开入模件异常",3668]
[80,"Arm19","开出模件异常",3669]
[80,"Arm20","开入配置错",3670]
[80,"Arm21","开出配置错",3671]
[80,"Arm22","开入通讯中断",3672]
[80,"Arm23","开出通讯中断",3673]
[80,"Arm24","传动状态未复归",3674]
[80,"Arm25","开入击穿",3675]
[80,"Arm26","开入输入不正常",3676]
[80,"Arm27","双位置输入不一致",3677]
[80,"Arm28","开入自检回路出错",3678]
[80,"Arm29","开入EEPROM出错",3679]
[80,"Arm30","开出EEPROM出错",3680]
[80,"Arm31","X12-a6输入3T1",3681]
[80,"Arm32","X12-a6输入3T2",3682]
[80,"Arm33","X12-a6输入3T3",3683]
[80,"Arm34","X12-a6输入3",3684]
[80,"Arm35","X12-c6输入4",3685]
[80,"Arm36","X12-a4输入1",3686]
[80,"Arm37","X12-c4输入2",3687]
[80,"Arm38","X3-a4输入1",3688]
[80,"Arm39","X3-c4输入2",3689]
[80,"Arm40","X3-a6输入3",3690]
[80,"Arm41","X3-c6输入4",3691]
[80,"Arm42","X4-a4输入1",3692]
[80,"Arm43","X4-c4输入2",3693]
[80,"Arm44","X4-a6输入3",3694]
[80,"Arm45","X4-c6输入4",3695]
[80,"Arm46","X5-a4输入1",3696]
[80,"Arm47","X5-c4输入2",3697]
[80,"Arm48","X5-a6输入3",3698]
[80,"Arm49","X5-c6输入4",3699]
[80,"Arm50","X13-a4输入1",3700]
[80,"Arm51","X13-c4输入2",3701]
[80,"Arm52","X13-a6输入3",3702]
[80,"Arm53","X13-c6输入4",3703]
[80,"Arm54","CPU异常",3704]
[80,"Arm55","设备参数不一致",3705]
[80,"Arm56","定值区号不一致",3706]
[80,"Arm57","定值不一致",3707]
[80,"Arm58","压板不一致",3708]
[80,"Arm59","LON1通讯中断",3709]
[80,"Arm60","LON2通讯中断",3710]
[80,"Arm61","压板模式不一致",3711]
[80,"Arm62","召唤配置无应答",3712]
[80,"Arm63","PLC逻辑校验出错",3713]
[80,"Arm64","信号复归",3714]
[80,"Arm65","X12-a6输入3_(重复1)",3715]
[80,"Arm66","X12-c6输入4_(重复1)",3716]
[80,"Arm67","X12-a4输入1_(重复1)",3717]
[80,"Arm68","X12-c4输入2_(重复1)",3718]
[80,"Arm69","X3-a4输入1_(重复1)",3719]
[80,"Arm70","X3-c4输入2_(重复1)",3720]
[80,"Arm71","X3-a6输入3_(重复1)",3721]
[80,"Arm72","X3-c6输入4_(重复1)",3722]
[80,"Arm73","X4-a4输入1_(重复1)",3723]
[80,"Arm74","X4-c4输入2_(重复1)",3724]
[80,"Arm75","X4-a6输入3_(重复1)",3725]
[80,"Arm76","X4-c6输入4_(重复1)",3726]
[80,"Arm77","X5-a4输入1_(重复1)",3727]
[80,"Arm78","X5-c4输入2_(重复1)",3728]
[80,"Arm79","X5-a6输入3_(重复1)",3729]
[80,"Arm80","X5-c6输入4_(重复1)",3730]
[80,"Arm81","X13-a4输入1_(重复1)",3731]
[80,"Arm82","X13-c4输入2_(重复1)",3732]
[80,"Arm83","X13-a6输入3_(重复1)",3733]
[80,"Arm84","X13-c6输入4_(重复1)",3734]
[80,"Arm85","检修状态压板",3735]
[80,"Arm86","远方修改定值",3736]
[80,"Arm87","保护启动",3737]
[80,"Arm88","X3-a4输入1_(重复2)",3738]
[80,"Arm89","X3-c4输入2_(重复2)",3739]
[80,"Arm90","X3-a6输入3_(重复2)",3740]
[80,"Arm91","X3-c6输入4_(重复2)",3741]
[80,"Arm92","X4-a4输入1_(重复2)",3742]
[80,"Arm93","X4-c4输入2_(重复2)",3743]
[80,"Arm94","X4-a6输入3_(重复2)",3744]
[80,"Arm95","X4-c6输入4_(重复2)",3745]
[80,"Arm96","X5-a4输入1_(重复2)",3746]
[80,"Arm97","X5-c4输入2_(重复2)",3747]
[80,"Arm98","X5-a6输入3_(重复2)",3748]
[80,"Arm99","X5-c6输入4_(重复2)",3749]
[80,"Arm100","X13-a4输入1_(重复2)",3750]
[80,"Arm101","X13-c4输入2_(重复2)",3751]
[80,"Arm102","X13-a6输入3_(重复2)",3752]
[80,"Arm103","X13-c6输入4_(重复2)",3753]
[80,"Arm104","X12-a6输入3T1_(重复1)",3754]
[80,"Arm105","X12-a6输入3T2_(重复1)",3755]
[80,"Arm106","X12-a6输入3T3_(重复1)",3756]
[80,"Arm107","X12-a6输入3_(重复2)",3757]
[80,"Arm108","X12-c6输入4_(重复2)",3758]
[80,"Arm109","X12-a4输入1_(重复2)",3759]
[80,"Arm110","X12-c4输入2_(重复2)",3760]
[80,"Arm111","录波完成",3761]
[80,"Arm112","录波启动",3762]
[80,"Arm113","网络状态1",3763]
[80,"Arm114","网络状态2",3764]
[80,"Arm115","装置通讯状态",3765]
[80,"Arm116","检修状态",3766]
[80,"Arm117","参数变化",3767]
[80,"Arm118","就地状态虚遥信",3768]
[80,"Arm119","遥控解除闭锁",3769]
[80,"Arm120","A网中断",3770]
[80,"Arm121","B网中断",3771]
[80,"Arm122","网络中断",3772]
[81,"Arm1","I类告警总",3773]
[81,"Arm2","模拟量采集错",3774]
[81,"Arm3","ROM和校验错",3775]
[81,"Arm4","定值错",3776]
[81,"Arm5","定值区指针错",3777]
[81,"Arm6","开出不响应",3778]
[81,"Arm7","开出击穿",3779]
[81,"Arm8","设备参数错",3780]
[81,"Arm9","软压板错",3781]
[81,"Arm10","系统配置错",3782]
[81,"Arm11","开出模件异常",3783]
[81,"Arm12","开出配置错",3784]
[81,"Arm13","开出EEPROM出错",3785]
[81,"Arm14","保护CPU插件异常",3786]
[81,"Arm15","开出异常",3787]
[81,"Arm16","CPU通讯中断",3788]
[81,"Arm17","设备参数不一致",3789]
[81,"Arm18","定值区号不一致",3790]
[81,"Arm19","定值不一致",3791]
[81,"Arm20","压板不一致",3792]
[81,"Arm21","召唤配置无应答",3793]
[81,"Arm22","对时异常",3794]
[81,"Arm23","面板配置不一致",3795]
[81,"Arm24","对时信号状态",3796]
[81,"Arm25","对时服务状态",3797]
[81,"Arm26","时间跳变侦测状态",3798]
[81,"Arm27","主保护硬压板",3799]
[81,"Arm28","高压侧后备保护硬压板",3800]
[81,"Arm29","高压侧电压硬压板",3801]
[81,"Arm30","低压1分支后备保护硬压板",3802]
[81,"Arm31","低压1分支电压硬压板",3803]
[81,"Arm32","低压2分支后备保护硬压板",3804]
[81,"Arm33","低压2分支电压硬压板",3805]
[81,"Arm34","远方操作硬压板",3806]
[81,"Arm35","保护检修状态硬压板",3807]
[81,"Arm36","主保护总压板",3808]
[81,"Arm37","高压侧后备保护总压板",3809]
[81,"Arm38","低压1分支后备保护总压板",3810]
[81,"Arm39","低压2分支后备保护总压板",3811]
[81,"Arm40","运行",3812]
[81,"Arm41","异常",3813]
[81,"Arm42","检修",3814]
[81,"Arm43","差动保护闭锁",3815]
[81,"Arm44","保护跳闸",3816]
[81,"Arm45","纵差差动速断有效",3817]
[81,"Arm46","纵差变化量差动有效",3818]
[81,"Arm47","纵差保护有效",3819]
[81,"Arm48","高相间阻抗有效",3820]
[81,"Arm49","高接地阻抗有效",3821]
[81,"Arm50","高复流Ⅰ段有效",3822]
[81,"Arm51","高复流Ⅱ段有效",3823]
[81,"Arm52","高复流Ⅲ段有效",3824]
[81,"Arm53","高零流Ⅰ段有效",3825]
[81,"Arm54","高零流Ⅱ段有效",3826]
[81,"Arm55","高零流Ⅲ段有效",3827]
[81,"Arm56","高失灵联跳有效",3828]
[81,"Arm57","高间隙过流有效",3829]
[81,"Arm58","高零序过压有效",3830]
[81,"Arm59","低1复流Ⅰ段有效",3831]
[81,"Arm60","低1复流Ⅱ段有效",3832]
[81,"Arm61","低2复流Ⅰ段有效",3833]
[81,"Arm62","低2复流Ⅱ段有效",3834]
[81,"Arm63","闭锁主保护",3835]
[81,"Arm64","闭锁后备保护",3836]
[81,"Arm65","主保护投入",3837]
[81,"Arm66","高压侧后备保护投入",3838]
[81,"Arm67","低压1分支后备保护投入",3839]
[81,"Arm68","低压2分支后备保护投入",3840]
[81,"Arm69","录波完成",3841]
[81,"Arm70","录波启动",3842]
[81,"Arm71","主保护软压板",3843]
[81,"Arm72","高压侧后备保护软压板",3844]
[81,"Arm73","低压1分支后备保护软压板",3845]
[81,"Arm74","低压2分支后备保护软压板",3846]
[81,"Arm75","远方投退压板软压板",3847]
[81,"Arm76","远方切换定值区软压板",3848]
[81,"Arm77","远方修改定值软压板",3849]
[81,"Arm78","高压侧失灵联跳开入",3850]
[81,"Arm79","信号复归",3851]
[81,"Arm80","保护动作",3852]
[81,"Arm81","保护启动",3853]
[81,"Arm82","纵差保护",3854]
[81,"Arm83","纵差差动速断",3855]
[81,"Arm84","高相间阻抗1时限",3856]
[81,"Arm85","高相间阻抗2时限",3857]
[81,"Arm86","高相间阻抗3时限",3858]
[81,"Arm87","高接地阻抗1时限",3859]
[81,"Arm88","高接地阻抗2时限",3860]
[81,"Arm89","高接地阻抗3时限",3861]
[81,"Arm90","高复流Ⅰ段1时限",3862]
[81,"Arm91","低1复流Ⅰ段1时限",3863]
[81,"Arm92","低2复流Ⅰ段1时限",3864]
[81,"Arm93","高复流Ⅰ段2时限",3865]
[81,"Arm94","高复流Ⅰ段3时限",3866]
[81,"Arm95","高复流Ⅱ段2时限",3867]
[81,"Arm96","高复流Ⅱ段3时限",3868]
[81,"Arm97","高复流Ⅲ段2时限",3869]
[81,"Arm98","低1复流Ⅰ段2时限",3870]
[81,"Arm99","低1复流Ⅰ段3时限",3871]
[81,"Arm100","低1复流Ⅱ段2时限",3872]
[81,"Arm101","低1复流Ⅱ段3时限",3873]
[81,"Arm102","低2复流Ⅰ段2时限",3874]
[81,"Arm103","低2复流Ⅰ段3时限",3875]
[81,"Arm104","低2复流Ⅱ段2时限",3876]
[81,"Arm105","低2复流Ⅱ段3时限",3877]
[81,"Arm106","高复流Ⅱ段1时限",3878]
[81,"Arm107","高复流Ⅲ段1时限",3879]
[81,"Arm108","低1复流Ⅱ段1时限",3880]
[81,"Arm109","低2复流Ⅱ段1时限",3881]
[81,"Arm110","高零流Ⅰ段1时限",3882]
[81,"Arm111","高零流Ⅱ段1时限",3883]
[81,"Arm112","高零流Ⅰ段2时限",3884]
[81,"Arm113","高零流Ⅰ段3时限",3885]
[81,"Arm114","高零流Ⅱ段2时限",3886]
[81,"Arm115","高零流Ⅱ段3时限",3887]
[81,"Arm116","高零流Ⅲ段2时限",3888]
[81,"Arm117","高间隙过流",3889]
[81,"Arm118","高零流Ⅲ段1时限",3890]
[81,"Arm119","高零序过压",3891]
[81,"Arm120","高断路器失灵联跳",3892]
[81,"Arm121","故障分量差动",3893]
[81,"Arm122","II类告警总",3894]
[81,"Arm123","开入击穿",3895]
[81,"Arm124","开入输入不正常",3896]
[81,"Arm125","双位置输入不一致",3897]
[81,"Arm126","失灵开入异常",3898]
[81,"Arm127","CAN通讯中断",3899]
[81,"Arm128","CAN通讯恢复",3900]
[81,"Arm129","开入模件异常",3901]
[81,"Arm130","开入配置错",3902]
[81,"Arm131","开入通讯中断",3903]
[81,"Arm132","开出通讯中断",3904]
[81,"Arm133","传动状态未复归",3905]
[81,"Arm134","开入自检回路出错",3906]
[81,"Arm135","开入EEPROM出错",3907]
[81,"Arm136","SRAM自检异常",3908]
[81,"Arm137","FLASH自检异常",3909]
[81,"Arm138","开入异常",3910]
[81,"Arm139","高压1侧CT断线",3911]
[81,"Arm140","高压2侧CT断线",3912]
[81,"Arm141","低压1分支CT断线",3913]
[81,"Arm142","低压2分支CT断线",3914]
[81,"Arm143","差流越限",3915]
[81,"Arm144","高压侧PT断线",3916]
[81,"Arm145","高压侧过负荷",3917]
[81,"Arm146","低1零序过压告警",3918]
[81,"Arm147","低压1分支PT断线",3919]
[81,"Arm148","低压侧过负荷",3920]
[81,"Arm149","低2零序过压告警",3921]
[81,"Arm150","低压2分支PT断线",3922]
[81,"Arm151","电流零漂越限告警",3923]
[81,"Arm152","工作于调试定值区",3924]
[81,"Arm153","低压1分支CT异常",3925]
[81,"Arm154","低压2分支CT异常",3926]
[81,"Arm155","网络状态1",3927]
[81,"Arm156","网络状态2",3928]
[81,"Arm157","装置通讯状态",3929]
[81,"Arm158","检修状态",3930]
[81,"Arm159","参数变化",3931]
[81,"Arm160","就地状态虚遥信",3932]
[81,"Arm161","遥控解除闭锁",3933]
[81,"Arm162","A网中断",3934]
[81,"Arm163","B网中断",3935]
[81,"Arm164","网络中断",3936]
[82,"Arm1","手动录波触发",3937]
[82,"Arm2","远方触发录波",3938]
[82,"Arm3","开入触发录波",3939]
[82,"Arm4","保护板告警触发录波",3940]
[82,"Arm5","保护板闭锁触发录波",3941]
[82,"Arm6","启动板告警触发录波",3942]
[82,"Arm7","启动板闭锁触发录波",3943]
[82,"Arm8","装置闭锁",3944]
[82,"Arm9","定值超范围",3945]
[82,"Arm10","板卡配置错误",3946]
[82,"Arm11","定值项变化告警",3947]
[82,"Arm12","CCD文件错误",3948]
[82,"Arm13","CID文件错误",3949]
[82,"Arm14","保护CPU插件异常",3950]
[82,"Arm15","模拟量采集错",3951]
[82,"Arm16","开出异常",3952]
[82,"Arm17","保护板定值出错",3953]
[82,"Arm18","保护板内存出错",3954]
[82,"Arm19","保护板采样出错",3955]
[82,"Arm20","保护板配置出错",3956]
[82,"Arm21","启动板DSP出错",3957]
[82,"Arm22","保护板长期闭锁告警",3958]
[82,"Arm23","启动板定值出错",3959]
[82,"Arm24","启动板内存出错",3960]
[82,"Arm25","启动板采样出错",3961]
[82,"Arm26","启动板配置出错",3962]
[82,"Arm27","保护板DSP出错",3963]
[82,"Arm28","启动板长期闭锁告警",3964]
[82,"Arm29","B13.跳闸出口异常",3965]
[82,"Arm30","B14.跳闸出口异常",3966]
[82,"Arm31","装置报警",3967]
[82,"Arm32","通信传动报警",3968]
[82,"Arm33","开出传动报警",3969]
[82,"Arm34","对时异常",3970]
[82,"Arm35","版本错误报警",3971]
[82,"Arm36","定值校验出错",3972]
[82,"Arm37","定值区不一致",3973]
[82,"Arm38","定值修改",3974]
[82,"Arm39","定值区切换",3975]
[82,"Arm40","对时信号状态",3976]
[82,"Arm41","对时服务状态",3977]
[82,"Arm42","时间跳变侦测状态",3978]
[82,"Arm43","内存不足",3979]
[82,"Arm44","IEC103配置文件无效",3980]
[82,"Arm45","装置过温告警",3981]
[82,"Arm46","装置低温告警",3982]
[82,"Arm47","装置温度异常告警",3983]
[82,"Arm48","保护板装置电源过压报警",3984]
[82,"Arm49","保护板装置电源低压报警",3985]
[82,"Arm50","保护板装置电源异常报警",3986]
[82,"Arm51","启动板装置电源过压报警",3987]
[82,"Arm52","启动板装置电源低压报警",3988]
[82,"Arm53","启动板装置电源异常报警",3989]
[82,"Arm54","B12.开入电源异常",3990]
[82,"Arm55","B12.板卡异常",3991]
[82,"Arm56","B13.板卡异常",3992]
[82,"Arm57","B14.板卡异常",3993]
[82,"Arm58","B15.信号出口异常",3994]
[82,"Arm59","B15.板卡异常",3995]
[82,"Arm60","运行",3996]
[82,"Arm61","异常",3997]
[82,"Arm62","检修",3998]
[82,"Arm63","差动保护闭锁",3999]
[82,"Arm64","保护跳闸",4000]
[82,"Arm65","闭锁主保护",4001]
[82,"Arm66","闭锁后备保护",4002]
[82,"Arm67","纵差差动速断有效",4003]
[82,"Arm68","纵差保护有效",4004]
[82,"Arm69","纵差变化量保护有效",4005]
[82,"Arm70","高相间阻抗有效",4006]
[82,"Arm71","高接地阻抗有效",4007]
[82,"Arm72","高复流Ⅰ段有效",4008]
[82,"Arm73","高复流Ⅱ段有效",4009]
[82,"Arm74","高复流Ⅲ段有效",4010]
[82,"Arm75","高零流Ⅰ段有效",4011]
[82,"Arm76","高零流Ⅱ段有效",4012]
[82,"Arm77","高零流Ⅲ段有效",4013]
[82,"Arm78","高零序过压有效",4014]
[82,"Arm79","高间隙过流有效",4015]
[82,"Arm80","高失灵联跳有效",4016]
[82,"Arm81","中相间阻抗有效",4017]
[82,"Arm82","中接地阻抗有效",4018]
[82,"Arm83","中复流Ⅰ段有效",4019]
[82,"Arm84","中复流Ⅱ段有效",4020]
[82,"Arm85","中复流Ⅲ段有效",4021]
[82,"Arm86","中零流Ⅰ段有效",4022]
[82,"Arm87","中零流Ⅱ段有效",4023]
[82,"Arm88","中零流Ⅲ段有效",4024]
[82,"Arm89","中间隙过流有效",4025]
[82,"Arm90","中零序过压有效",4026]
[82,"Arm91","中失灵联跳有效",4027]
[82,"Arm92","低1复流Ⅰ段有效",4028]
[82,"Arm93","低1复流Ⅱ段有效",4029]
[82,"Arm94","低2复流Ⅰ段有效",4030]
[82,"Arm95","低2复流Ⅱ段有效",4031]
[82,"Arm96","主保护投入",4032]
[82,"Arm97","高压侧后备保护投入",4033]
[82,"Arm98","中压侧后备保护投入",4034]
[82,"Arm99","低压1分支后备保护投入",4035]
[82,"Arm100","低压2分支后备保护投入",4036]
[82,"Arm101","录波完成",4037]
[82,"Arm102","纵差差动速断保护起动",4038]
[82,"Arm103","纵差比率差动保护起动",4039]
[82,"Arm104","纵差工频变化量差动保护起动",4040]
[82,"Arm105","高压侧阻抗起动",4041]
[82,"Arm106","高压侧复压过流Ⅰ段起动",4042]
[82,"Arm107","高压侧复压过流Ⅱ段起动",4043]
[82,"Arm108","高压侧复压过流Ⅲ段起动",4044]
[82,"Arm109","高压侧零序过流Ⅱ段起动",4045]
[82,"Arm110","高压侧零序过流Ⅲ段起动",4046]
[82,"Arm111","高压侧间隙过流起动",4047]
[82,"Arm112","高压侧间隙保护起动",4048]
[82,"Arm113","高压侧间隙过压起动",4049]
[82,"Arm114","高压侧失灵联跳起动",4050]
[82,"Arm115","中压侧阻抗起动",4051]
[82,"Arm116","中压侧复压过流Ⅰ段起动",4052]
[82,"Arm117","中压侧复压过流Ⅱ段起动",4053]
[82,"Arm118","中压侧复压过流Ⅲ段起动",4054]
[82,"Arm119","中压侧零序过流Ⅲ段起动",4055]
[82,"Arm120","中压侧间隙过流1时限起动",4056]
[82,"Arm121","中压侧间隙保护1时限起动",4057]
[82,"Arm122","中压侧间隙过流2时限起动",4058]
[82,"Arm123","中压侧间隙保护2时限起动",4059]
[82,"Arm124","中压侧间隙过压1时限起动",4060]
[82,"Arm125","中压侧间隙过压2时限起动",4061]
[82,"Arm126","中压侧失灵联跳起动",4062]
[82,"Arm127","低压1分支过流Ⅰ段起动",4063]
[82,"Arm128","低压1分支过流Ⅱ段起动",4064]
[82,"Arm129","低压2分支过流Ⅰ段起动",4065]
[82,"Arm130","低压2分支过流Ⅱ段起动",4066]
[82,"Arm131","高压侧零序过流Ⅰ段起动",4067]
[82,"Arm132","中压侧零序过流Ⅰ段起动",4068]
[82,"Arm133","中压侧零序过流Ⅱ段起动",4069]
[82,"Arm134","跳闸信号",4070]
[82,"Arm135","启动打印",4071]
[82,"Arm136","保护检修状态硬压板",4072]
[82,"Arm137","信号复归",4073]
[82,"Arm138","高压侧电压硬压板",4074]
[82,"Arm139","中压侧电压硬压板",4075]
[82,"Arm140","低压1分支电压硬压板",4076]
[82,"Arm141","低压2分支电压硬压板",4077]
[82,"Arm142","主保护硬压板",4078]
[82,"Arm143","高压侧后备保护硬压板",4079]
[82,"Arm144","中压侧后备保护硬压板",4080]
[82,"Arm145","低压1分支后备保护硬压板",4081]
[82,"Arm146","低压2分支后备保护硬压板",4082]
[82,"Arm147","高压侧失灵联跳开入",4083]
[82,"Arm148","中压侧失灵联跳开入",4084]
[82,"Arm149","远方操作硬压板",4085]
[82,"Arm150","高压侧TWJ",4086]
[82,"Arm151","中压侧TWJ",4087]
[82,"Arm152","频率异常告警",4088]
[82,"Arm153","差流越限",4089]
[82,"Arm154","纵差回路断线告警",4090]
[82,"Arm155","高压侧失灵联跳节点告警",4091]
[82,"Arm156","高压侧失灵联跳电流告警",4092]
[82,"Arm157","中压侧失灵联跳节点告警",4093]
[82,"Arm158","中压侧失灵联跳电流告警",4094]
[82,"Arm159","保护板长期启动",4095]
[82,"Arm160","启动板长期启动",4096]
[82,"Arm161","主保护软压板",4097]
[82,"Arm162","高复流Ⅰ段2时限",4098]
[82,"Arm163","高复流Ⅰ段3时限",4099]
[82,"Arm164","高复流Ⅱ段1时限",4100]
[82,"Arm165","高复流Ⅱ段2时限",4101]
[82,"Arm166","高复流Ⅱ段3时限",4102]
[82,"Arm167","高复流Ⅲ段1时限",4103]
[82,"Arm168","高复流Ⅲ段2时限",4104]
[82,"Arm169","高零流Ⅰ段1时限",4105]
[82,"Arm170","高零流Ⅰ段2时限",4106]
[82,"Arm171","高零流Ⅰ段3时限",4107]
[82,"Arm172","高零流Ⅱ段1时限",4108]
[82,"Arm173","高零流Ⅱ段2时限",4109]
[82,"Arm174","高零流Ⅱ段3时限",4110]
[82,"Arm175","高零流Ⅲ段1时限",4111]
[82,"Arm176","高零流Ⅲ段2时限",4112]
[82,"Arm177","高间隙过流",4113]
[82,"Arm178","高零序过压",4114]
[82,"Arm179","高断路器失灵联跳",4115]
[82,"Arm180","中相间阻抗1时限",4116]
[82,"Arm181","中相间阻抗2时限",4117]
[82,"Arm182","中相间阻抗3时限",4118]
[82,"Arm183","中接地阻抗1时限",4119]
[82,"Arm184","中接地阻抗2时限",4120]
[82,"Arm185","中接地阻抗3时限",4121]
[82,"Arm186","中复流Ⅰ段1时限",4122]
[82,"Arm187","中复流Ⅰ段2时限",4123]
[82,"Arm188","中复流Ⅰ段3时限",4124]
[82,"Arm189","中复流Ⅱ段1时限",4125]
[82,"Arm190","中复流Ⅱ段2时限",4126]
[82,"Arm191","中复流Ⅱ段3时限",4127]
[82,"Arm192","中复流Ⅲ段1时限",4128]
[82,"Arm193","中复流Ⅲ段2时限",4129]
[82,"Arm194","中零流Ⅰ段1时限",4130]
[82,"Arm195","中零流Ⅰ段2时限",4131]
[82,"Arm196","中零流Ⅰ段3时限",4132]
[82,"Arm197","中零流Ⅱ段1时限",4133]
[82,"Arm198","中零流Ⅱ段2时限",4134]
[82,"Arm199","中零流Ⅱ段3时限",4135]
[82,"Arm200","中零流Ⅲ段1时限",4136]
[82,"Arm201","中零流Ⅲ段2时限",4137]
[82,"Arm202","中间隙过流1时限",4138]
[82,"Arm203","中间隙过流2时限",4139]
[82,"Arm204","中零序过压1时限",4140]
[82,"Arm205","中零序过压2时限",4141]
[82,"Arm206","中断路器失灵联跳",4142]
[82,"Arm207","低1复流Ⅰ段1时限",4143]
[82,"Arm208","低1复流Ⅰ段2时限",4144]
[82,"Arm209","低1复流Ⅰ段3时限",4145]
[82,"Arm210","低1复流Ⅱ段1时限",4146]
[82,"Arm211","低1复流Ⅱ段2时限",4147]
[82,"Arm212","低1复流Ⅱ段3时限",4148]
[82,"Arm213","低2复流Ⅰ段1时限",4149]
[82,"Arm214","低2复流Ⅰ段2时限",4150]
[82,"Arm215","低2复流Ⅰ段3时限",4151]
[82,"Arm216","低2复流Ⅱ段1时限",4152]
[82,"Arm217","低2复流Ⅱ段2时限",4153]
[82,"Arm218","低2复流Ⅱ段3时限",4154]
[82,"Arm219","跳高压侧",4155]
[82,"Arm220","跳高压侧母联",4156]
[82,"Arm221","跳中压侧",4157]
[82,"Arm222","跳中压侧母联",4158]
[82,"Arm223","跳低压1分支",4159]
[82,"Arm224","跳低压1分段",4160]
[82,"Arm225","跳低压2分支",4161]
[82,"Arm226","跳低压2分段",4162]
[82,"Arm227","闭锁中压侧备自投",4163]
[82,"Arm228","闭锁低压1分支备自投",4164]
[82,"Arm229","闭锁低压2分支备自投",4165]
[82,"Arm230","跳备用出口1~4",4166]
[82,"Arm231","保护启动",4167]
[82,"Arm232","高压侧过负荷",4168]
[82,"Arm233","中压侧过负荷",4169]
[82,"Arm234","低压1分支零序过压报警",4170]
[82,"Arm235","低压2分支零序过压报警",4171]
[82,"Arm236","低压侧过负荷",4172]
[82,"Arm237","失灵开入异常",4173]
[82,"Arm238","高压1侧CT异常",4174]
[82,"Arm239","高压1侧CT断线",4175]
[82,"Arm240","高压2侧CT异常",4176]
[82,"Arm241","高压2侧CT断线",4177]
[82,"Arm242","中压侧CT异常",4178]
[82,"Arm243","中压侧CT断线",4179]
[82,"Arm244","低压1分支CT异常",4180]
[82,"Arm245","低压1分支CT断线",4181]
[82,"Arm246","低压2分支CT异常",4182]
[82,"Arm247","低压2分支CT断线",4183]
[82,"Arm248","高压侧PT断线",4184]
[82,"Arm249","中压侧PT断线",4185]
[82,"Arm250","低压1分支PT断线",4186]
[82,"Arm251","低压2分支PT断线",4187]
[82,"Arm252","频率异常告警",4188]
[82,"Arm253","差流越限",4189]
[82,"Arm254","纵差回路断线告警",4190]
[82,"Arm255","高压侧失灵联跳节点告警",4191]
[82,"Arm256","高压侧失灵联跳电流告警",4192]
[82,"Arm257","中压侧失灵联跳节点告警",4193]
[82,"Arm258","中压侧失灵联跳电流告警",4194]
[82,"Arm259","保护板长期启动",4195]
[82,"Arm260","启动板长期启动",4196]
[82,"Arm261","主保护软压板",4197]
[82,"Arm262","高压侧后备保护软压板",4198]
[82,"Arm263","中压侧后备保护软压板",4199]
[82,"Arm264","低压1分支后备保护软压板",4200]
[82,"Arm265","低压2分支后备保护软压板",4201]
[82,"Arm266","远方投退压板软压板",4202]
[82,"Arm267","远方切换定值区软压板",4203]
[82,"Arm268","远方修改定值软压板",4204]
[82,"Arm269","网络状态1",4205]
[82,"Arm270","网络状态2",4206]
[82,"Arm271","装置通讯状态",4207]
[82,"Arm272","检修状态",4208]
[82,"Arm273","参数变化",4209]
[82,"Arm274","就地状态虚遥信",4210]
[82,"Arm275","遥控解除闭锁",4211]
[82,"Arm276","A网中断",4212]
[82,"Arm277","B网中断",4213]
[82,"Arm278","网络中断",4214]
[83,"Arm1","模拟量采集错",4215]
[83,"Arm2","跳闸失败",4216]
[83,"Arm3","设备参数错",4217]
[83,"Arm4","ROM和校验错",4218]
[83,"Arm5","定值错",4219]
[83,"Arm6","定值区指针错",4220]
[83,"Arm7","开出不响应",4221]
[83,"Arm8","开出击穿",4222]
[83,"Arm9","压板模式未确认",4223]
[83,"Arm10","SRAM自检异常",4224]
[83,"Arm11","FLASH自检异常",4225]
[83,"Arm12","自描述错",4226]
[83,"Arm13","开入状态未复归",4227]
[83,"Arm14","软压板错",4228]
[83,"Arm15","系统配置错",4229]
[83,"Arm16","CAN通讯中断",4230]
[83,"Arm17","CAN通讯恢复",4231]
[83,"Arm18","开入模件异常",4232]
[83,"Arm19","开出模件异常",4233]
[83,"Arm20","开入配置错",4234]
[83,"Arm21","开出配置错",4235]
[83,"Arm22","开入通讯中断",4236]
[83,"Arm23","开出通讯中断",4237]
[83,"Arm24","传动状态未复归",4238]
[83,"Arm25","开入击穿",4239]
[83,"Arm26","开入输入不正常",4240]
[83,"Arm27","双位置输入不一致",4241]
[83,"Arm28","开入自检回路出错",4242]
[83,"Arm29","开入EEPROM出错",4243]
[83,"Arm30","开出EEPROM出错",4244]
[83,"Arm31","X12-a6输入3T1",4245]
[83,"Arm32","X12-a6输入3T2",4246]
[83,"Arm33","X12-a6输入3T3",4247]
[83,"Arm34","X12-a6输入3",4248]
[83,"Arm35","X12-c6输入4",4249]
[83,"Arm36","X12-a4输入1",4250]
[83,"Arm37","X12-c4输入2",4251]
[83,"Arm38","X3-a4输入1",4252]
[83,"Arm39","X3-c4输入2",4253]
[83,"Arm40","X3-a6输入3",4254]
[83,"Arm41","X3-c6输入4",4255]
[83,"Arm42","X4-a4输入1",4256]
[83,"Arm43","X4-c4输入2",4257]
[83,"Arm44","X4-a6输入3",4258]
[83,"Arm45","X4-c6输入4",4259]
[83,"Arm46","X5-a4输入1",4260]
[83,"Arm47","X5-c4输入2",4261]
[83,"Arm48","X5-a6输入3",4262]
[83,"Arm49","X5-c6输入4",4263]
[83,"Arm50","X13-a4输入1",4264]
[83,"Arm51","X13-c4输入2",4265]
[83,"Arm52","X13-a6输入3",4266]
[83,"Arm53","X13-c6输入4",4267]
[83,"Arm54","CPU异常",4268]
[83,"Arm55","设备参数不一致",4269]
[83,"Arm56","定值区号不一致",4270]
[83,"Arm57","定值不一致",4271]
[83,"Arm58","压板不一致",4272]
[83,"Arm59","LON1通讯中断",4273]
[83,"Arm60","LON2通讯中断",4274]
[83,"Arm61","压板模式不一致",4275]
[83,"Arm62","召唤配置无应答",4276]
[83,"Arm63","PLC逻辑校验出错",4277]
[83,"Arm64","信号复归",4278]
[83,"Arm65","X12-a6输入3_(重复1)",4279]
[83,"Arm66","X12-c6输入4_(重复1)",4280]
[83,"Arm67","X12-a4输入1_(重复1)",4281]
[83,"Arm68","X12-c4输入2_(重复1)",4282]
[83,"Arm69","X3-a4输入1_(重复1)",4283]
[83,"Arm70","X3-c4输入2_(重复1)",4284]
[83,"Arm71","X3-a6输入3_(重复1)",4285]
[83,"Arm72","X3-c6输入4_(重复1)",4286]
[83,"Arm73","X4-a4输入1_(重复1)",4287]
[83,"Arm74","X4-c4输入2_(重复1)",4288]
[83,"Arm75","X4-a6输入3_(重复1)",4289]
[83,"Arm76","X4-c6输入4_(重复1)",4290]
[83,"Arm77","X5-a4输入1_(重复1)",4291]
[83,"Arm78","X5-c4输入2_(重复1)",4292]
[83,"Arm79","X5-a6输入3_(重复1)",4293]
[83,"Arm80","X5-c6输入4_(重复1)",4294]
[83,"Arm81","X13-a4输入1_(重复1)",4295]
[83,"Arm82","X13-c4输入2_(重复1)",4296]
[83,"Arm83","X13-a6输入3_(重复1)",4297]
[83,"Arm84","X13-c6输入4_(重复1)",4298]
[83,"Arm85","检修状态压板",4299]
[83,"Arm86","远方修改定值",4300]
[83,"Arm87","保护启动",4301]
[83,"Arm88","X3-a4输入1_(重复2)",4302]
[83,"Arm89","X3-c4输入2_(重复2)",4303]
[83,"Arm90","X3-a6输入3_(重复2)",4304]
[83,"Arm91","X3-c6输入4_(重复2)",4305]
[83,"Arm92","X4-a4输入1_(重复2)",4306]
[83,"Arm93","X4-c4输入2_(重复2)",4307]
[83,"Arm94","X4-a6输入3_(重复2)",4308]
[83,"Arm95","X4-c6输入4_(重复2)",4309]
[83,"Arm96","X5-a4输入1_(重复2)",4310]
[83,"Arm97","X5-c4输入2_(重复2)",4311]
[83,"Arm98","X5-a6输入3_(重复2)",4312]
[83,"Arm99","X5-c6输入4_(重复2)",4313]
[83,"Arm100","X13-a4输入1_(重复2)",4314]
[83,"Arm101","X13-c4输入2_(重复2)",4315]
[83,"Arm102","X13-a6输入3_(重复2)",4316]
[83,"Arm103","X13-c6输入4_(重复2)",4317]
[83,"Arm104","X12-a6输入3T1_(重复1)",4318]
[83,"Arm105","X12-a6输入3T2_(重复1)",4319]
[83,"Arm106","X12-a6输入3T3_(重复1)",4320]
[83,"Arm107","X12-a6输入3_(重复2)",4321]
[83,"Arm108","X12-c6输入4_(重复2)",4322]
[83,"Arm109","X12-a4输入1_(重复2)",4323]
[83,"Arm110","X12-c4输入2_(重复2)",4324]
[83,"Arm111","录波完成",4325]
[83,"Arm112","录波启动",4326]
[83,"Arm113","网络状态1",4327]
[83,"Arm114","网络状态2",4328]
[83,"Arm115","装置通讯状态",4329]
[83,"Arm116","检修状态",4330]
[83,"Arm117","参数变化",4331]
[83,"Arm118","就地状态虚遥信",4332]
[83,"Arm119","遥控解除闭锁",4333]
[83,"Arm120","A网中断",4334]
[83,"Arm121","B网中断",4335]
[83,"Arm122","网络中断",4336]
[84,"Arm1","I类告警总",4337]
[84,"Arm2","模拟量采集错",4338]
[84,"Arm3","ROM和校验错",4339]
[84,"Arm4","定值错",4340]
[84,"Arm5","定值区指针错",4341]
[84,"Arm6","开出不响应",4342]
[84,"Arm7","开出击穿",4343]
[84,"Arm8","设备参数错",4344]
[84,"Arm9","软压板错",4345]
[84,"Arm10","系统配置错",4346]
[84,"Arm11","开出模件异常",4347]
[84,"Arm12","开出配置错",4348]
[84,"Arm13","开出EEPROM出错",4349]
[84,"Arm14","保护CPU插件异常",4350]
[84,"Arm15","开出异常",4351]
[84,"Arm16","CPU通讯中断",4352]
[84,"Arm17","设备参数不一致",4353]
[84,"Arm18","定值区号不一致",4354]
[84,"Arm19","定值不一致",4355]
[84,"Arm20","压板不一致",4356]
[84,"Arm21","召唤配置无应答",4357]
[84,"Arm22","对时异常",4358]
[84,"Arm23","面板配置不一致",4359]
[84,"Arm24","对时信号状态",4360]
[84,"Arm25","对时服务状态",4361]
[84,"Arm26","时间跳变侦测状态",4362]
[84,"Arm27","主保护硬压板",4363]
[84,"Arm28","高压侧后备保护硬压板",4364]
[84,"Arm29","高压侧电压硬压板",4365]
[84,"Arm30","低压1分支后备保护硬压板",4366]
[84,"Arm31","低压1分支电压硬压板",4367]
[84,"Arm32","低压2分支后备保护硬压板",4368]
[84,"Arm33","低压2分支电压硬压板",4369]
[84,"Arm34","远方操作硬压板",4370]
[84,"Arm35","保护检修状态硬压板",4371]
[84,"Arm36","主保护总压板",4372]
[84,"Arm37","高压侧后备保护总压板",4373]
[84,"Arm38","低压1分支后备保护总压板",4374]
[84,"Arm39","低压2分支后备保护总压板",4375]
[84,"Arm40","运行",4376]
[84,"Arm41","异常",4377]
[84,"Arm42","检修",4378]
[84,"Arm43","差动保护闭锁",4379]
[84,"Arm44","保护跳闸",4380]
[84,"Arm45","纵差差动速断有效",4381]
[84,"Arm46","纵差变化量差动有效",4382]
[84,"Arm47","纵差保护有效",4383]
[84,"Arm48","高相间阻抗有效",4384]
[84,"Arm49","高接地阻抗有效",4385]
[84,"Arm50","高复流Ⅰ段有效",4386]
[84,"Arm51","高复流Ⅱ段有效",4387]
[84,"Arm52","高复流Ⅲ段有效",4388]
[84,"Arm53","高零流Ⅰ段有效",4389]
[84,"Arm54","高零流Ⅱ段有效",4390]
[84,"Arm55","高零流Ⅲ段有效",4391]
[84,"Arm56","高失灵联跳有效",4392]
[84,"Arm57","高间隙过流有效",4393]
[84,"Arm58","高零序过压有效",4394]
[84,"Arm59","低1复流Ⅰ段有效",4395]
[84,"Arm60","低1复流Ⅱ段有效",4396]
[84,"Arm61","低2复流Ⅰ段有效",4397]
[84,"Arm62","低2复流Ⅱ段有效",4398]
[84,"Arm63","闭锁主保护",4399]
[84,"Arm64","闭锁后备保护",4400]
[84,"Arm65","主保护投入",4401]
[84,"Arm66","高压侧后备保护投入",4402]
[84,"Arm67","低压1分支后备保护投入",4403]
[84,"Arm68","低压2分支后备保护投入",4404]
[84,"Arm69","录波完成",4405]
[84,"Arm70","录波启动",4406]
[84,"Arm71","保护启动",4407]
[84,"Arm72","高压侧后备保护软压板",4408]
[84,"Arm73","低压1分支后备保护软压板",4409]
[84,"Arm74","低压2分支后备保护软压板",4410]
[84,"Arm75","远方投退压板软压板",4411]
[84,"Arm76","远方切换定值区软压板",4412]
[84,"Arm77","远方修改定值软压板",4413]
[84,"Arm78","高压侧失灵联跳开入",4414]
[84,"Arm79","信号复归",4415]
[84,"Arm80","保护动作",4416]
[84,"Arm81","保护启动",4417]
[84,"Arm82","纵差保护",4418]
[84,"Arm83","纵差差动速断",4419]
[84,"Arm84","高相间阻抗1时限",4420]
[84,"Arm85","高相间阻抗2时限",4421]
[84,"Arm86","高相间阻抗3时限",4422]
[84,"Arm87","高接地阻抗1时限",4423]
[84,"Arm88","高接地阻抗2时限",4424]
[84,"Arm89","高接地阻抗3时限",4425]
[84,"Arm90","高复流Ⅰ段1时限",4426]
[84,"Arm91","低1复流Ⅰ段1时限",4427]
[84,"Arm92","低2复流Ⅰ段1时限",4428]
[84,"Arm93","高复流Ⅰ段2时限",4429]
[84,"Arm94","高复流Ⅰ段3时限",4430]
[84,"Arm95","高复流Ⅱ段2时限",4431]
[84,"Arm96","高复流Ⅱ段3时限",4432]
[84,"Arm97","高复流Ⅲ段2时限",4433]
[84,"Arm98","低1复流Ⅰ段2时限",4434]
[84,"Arm99","低1复流Ⅰ段3时限",4435]
[84,"Arm100","低1复流Ⅱ段2时限",4436]
[84,"Arm101","低1复流Ⅱ段3时限",4437]
[84,"Arm102","低2复流Ⅰ段2时限",4438]
[84,"Arm103","低2复流Ⅰ段3时限",4439]
[84,"Arm104","低2复流Ⅱ段2时限",4440]
[84,"Arm105","低2复流Ⅱ段3时限",4441]
[84,"Arm106","高复流Ⅱ段1时限",4442]
[84,"Arm107","高复流Ⅲ段1时限",4443]
[84,"Arm108","低1复流Ⅱ段1时限",4444]
[84,"Arm109","低2复流Ⅱ段1时限",4445]
[84,"Arm110","高零流Ⅰ段1时限",4446]
[84,"Arm111","高零流Ⅱ段1时限",4447]
[84,"Arm112","高零流Ⅰ段2时限",4448]
[84,"Arm113","高零流Ⅰ段3时限",4449]
[84,"Arm114","高零流Ⅱ段2时限",4450]
[84,"Arm115","高零流Ⅱ段3时限",4451]
[84,"Arm116","高零流Ⅲ段2时限",4452]
[84,"Arm117","高间隙过流",4453]
[84,"Arm118","高零流Ⅲ段1时限",4454]
[84,"Arm119","高零序过压",4455]
[84,"Arm120","高断路器失灵联跳",4456]
[84,"Arm121","故障分量差动",4457]
[84,"Arm122","II类告警总",4458]
[84,"Arm123","开入击穿",4459]
[84,"Arm124","开入输入不正常",4460]
[84,"Arm125","双位置输入不一致",4461]
[84,"Arm126","失灵开入异常",4462]
[84,"Arm127","CAN通讯中断",4463]
[84,"Arm128","CAN通讯恢复",4464]
[84,"Arm129","开入模件异常",4465]
[84,"Arm130","开入配置错",4466]
[84,"Arm131","开入通讯中断",4467]
[84,"Arm132","开出通讯中断",4468]
[84,"Arm133","传动状态未复归",4469]
[84,"Arm134","开入自检回路出错",4470]
[84,"Arm135","开入EEPROM出错",4471]
[84,"Arm136","SRAM自检异常",4472]
[84,"Arm137","FLASH自检异常",4473]
[84,"Arm138","开入异常",4474]
[84,"Arm139","高压1侧CT断线",4475]
[84,"Arm140","高压2侧CT断线",4476]
[84,"Arm141","低压1分支CT断线",4477]
[84,"Arm142","低压2分支CT断线",4478]
[84,"Arm143","差流越限",4479]
[84,"Arm144","高压侧PT断线",4480]
[84,"Arm145","高压侧过负荷",4481]
[84,"Arm146","低1零序过压告警",4482]
[84,"Arm147","低压1分支PT断线",4483]
[84,"Arm148","低压侧过负荷",4484]
[84,"Arm149","低2零序过压告警",4485]
[84,"Arm150","低压2分支PT断线",4486]
[84,"Arm151","电流零漂越限告警",4487]
[84,"Arm152","工作于调试定值区",4488]
[84,"Arm153","低压1分支CT异常",4489]
[84,"Arm154","低压2分支CT异常",4490]
[84,"Arm155","网络状态1",4491]
[84,"Arm156","网络状态2",4492]
[84,"Arm157","装置通讯状态",4493]
[84,"Arm158","检修状态",4494]
[84,"Arm159","参数变化",4495]
[84,"Arm160","就地状态虚遥信",4496]
[84,"Arm161","遥控解除闭锁",4497]
[84,"Arm162","A网中断",4498]
[84,"Arm163","B网中断",4499]
[84,"Arm164","网络中断",4500]
[85,"Arm1","手动录波触发",4501]
[85,"Arm2","远方触发录波",4502]
[85,"Arm3","开入触发录波",4503]
[85,"Arm4","保护板告警触发录波",4504]
[85,"Arm5","保护板闭锁触发录波",4505]
[85,"Arm6","启动板告警触发录波",4506]
[85,"Arm7","启动板闭锁触发录波",4507]
[85,"Arm8","装置闭锁",4508]
[85,"Arm9","定值超范围",4509]
[85,"Arm10","板卡配置错误",4510]
[85,"Arm11","定值项变化告警",4511]
[85,"Arm12","CCD文件错误",4512]
[85,"Arm13","CID文件错误",4513]
[85,"Arm14","保护CPU插件异常",4514]
[85,"Arm15","模拟量采集错",4515]
[85,"Arm16","开出异常",4516]
[85,"Arm17","保护板定值出错",4517]
[85,"Arm18","保护板内存出错",4518]
[85,"Arm19","保护板采样出错",4519]
[85,"Arm20","保护板配置出错",4520]
[85,"Arm21","启动板DSP出错",4521]
[85,"Arm22","保护板长期闭锁告警",4522]
[85,"Arm23","启动板定值出错",4523]
[85,"Arm24","启动板内存出错",4524]
[85,"Arm25","启动板采样出错",4525]
[85,"Arm26","启动板配置出错",4526]
[85,"Arm27","保护板DSP出错",4527]
[85,"Arm28","启动板长期闭锁告警",4528]
[85,"Arm29","B13.跳闸出口异常",4529]
[85,"Arm30","B14.跳闸出口异常",4530]
[85,"Arm31","装置报警",4531]
[85,"Arm32","通信传动报警",4532]
[85,"Arm33","开出传动报警",4533]
[85,"Arm34","对时异常",4534]
[85,"Arm35","版本错误报警",4535]
[85,"Arm36","定值校验出错",4536]
[85,"Arm37","定值区不一致",4537]
[85,"Arm38","定值修改",4538]
[85,"Arm39","定值区切换",4539]
[85,"Arm40","对时信号状态",4540]
[85,"Arm41","对时服务状态",4541]
[85,"Arm42","时间跳变侦测状态",4542]
[85,"Arm43","内存不足",4543]
[85,"Arm44","IEC103配置文件无效",4544]
[85,"Arm45","装置过温告警",4545]
[85,"Arm46","装置低温告警",4546]
[85,"Arm47","装置温度异常告警",4547]
[85,"Arm48","保护板装置电源过压报警",4548]
[85,"Arm49","保护板装置电源低压报警",4549]
[85,"Arm50","保护板装置电源异常报警",4550]
[85,"Arm51","启动板装置电源过压报警",4551]
[85,"Arm52","启动板装置电源低压报警",4552]
[85,"Arm53","启动板装置电源异常报警",4553]
[85,"Arm54","B12.开入电源异常",4554]
[85,"Arm55","B12.板卡异常",4555]
[85,"Arm56","B13.板卡异常",4556]
[85,"Arm57","B14.板卡异常",4557]
[85,"Arm58","B15.信号出口异常",4558]
[85,"Arm59","B15.板卡异常",4559]
[85,"Arm60","运行",4560]
[85,"Arm61","异常",4561]
[85,"Arm62","检修",4562]
[85,"Arm63","差动保护闭锁",4563]
[85,"Arm64","保护跳闸",4564]
[85,"Arm65","闭锁主保护",4565]
[85,"Arm66","闭锁后备保护",4566]
[85,"Arm67","纵差差动速断有效",4567]
[85,"Arm68","纵差保护有效",4568]
[85,"Arm69","纵差变化量保护有效",4569]
[85,"Arm70","高相间阻抗有效",4570]
[85,"Arm71","高接地阻抗有效",4571]
[85,"Arm72","高复流Ⅰ段有效",4572]
[85,"Arm73","高复流Ⅱ段有效",4573]
[85,"Arm74","高复流Ⅲ段有效",4574]
[85,"Arm75","高零流Ⅰ段有效",4575]
[85,"Arm76","高零流Ⅱ段有效",4576]
[85,"Arm77","高零流Ⅲ段有效",4577]
[85,"Arm78","高零序过压有效",4578]
[85,"Arm79","高间隙过流有效",4579]
[85,"Arm80","高失灵联跳有效",4580]
[85,"Arm81","中相间阻抗有效",4581]
[85,"Arm82","中接地阻抗有效",4582]
[85,"Arm83","中复流Ⅰ段有效",4583]
[85,"Arm84","中复流Ⅱ段有效",4584]
[85,"Arm85","中复流Ⅲ段有效",4585]
[85,"Arm86","中零流Ⅰ段有效",4586]
[85,"Arm87","中零流Ⅱ段有效",4587]
[85,"Arm88","中零流Ⅲ段有效",4588]
[85,"Arm89","中间隙过流有效",4589]
[85,"Arm90","中零序过压有效",4590]
[85,"Arm91","中失灵联跳有效",4591]
[85,"Arm92","低1复流Ⅰ段有效",4592]
[85,"Arm93","低1复流Ⅱ段有效",4593]
[85,"Arm94","低2复流Ⅰ段有效",4594]
[85,"Arm95","低2复流Ⅱ段有效",4595]
[85,"Arm96","主保护投入",4596]
[85,"Arm97","高压侧后备保护投入",4597]
[85,"Arm98","中压侧后备保护投入",4598]
[85,"Arm99","低压1分支后备保护投入",4599]
[85,"Arm100","低压2分支后备保护投入",4600]
[85,"Arm101","录波完成",4601]
[85,"Arm102","纵差差动速断保护起动",4602]
[85,"Arm103","纵差比率差动保护起动",4603]
[85,"Arm104","纵差工频变化量差动保护起动",4604]
[85,"Arm105","高压侧阻抗起动",4605]
[85,"Arm106","高压侧复压过流Ⅰ段起动",4606]
[85,"Arm107","高压侧复压过流Ⅱ段起动",4607]
[85,"Arm108","高压侧复压过流Ⅲ段起动",4608]
[85,"Arm109","高压侧零序过流Ⅱ段起动",4609]
[85,"Arm110","高压侧零序过流Ⅲ段起动",4610]
[85,"Arm111","高压侧间隙过流起动",4611]
[85,"Arm112","高压侧间隙保护起动",4612]
[85,"Arm113","高压侧间隙过压起动",4613]
[85,"Arm114","高压侧失灵联跳起动",4614]
[85,"Arm115","中压侧阻抗起动",4615]
[85,"Arm116","中压侧复压过流Ⅰ段起动",4616]
[85,"Arm117","中压侧复压过流Ⅱ段起动",4617]
[85,"Arm118","中压侧复压过流Ⅲ段起动",4618]
[85,"Arm119","中压侧零序过流Ⅲ段起动",4619]
[85,"Arm120","中压侧间隙过流1时限起动",4620]
[85,"Arm121","中压侧间隙保护1时限起动",4621]
[85,"Arm122","中压侧间隙过流2时限起动",4622]
[85,"Arm123","中压侧间隙保护2时限起动",4623]
[85,"Arm124","中压侧间隙过压1时限起动",4624]
[85,"Arm125","中压侧间隙过压2时限起动",4625]
[85,"Arm126","中压侧失灵联跳起动",4626]
[85,"Arm127","低压1分支过流Ⅰ段起动",4627]
[85,"Arm128","低压1分支过流Ⅱ段起动",4628]
[85,"Arm129","低压2分支过流Ⅰ段起动",4629]
[85,"Arm130","低压2分支过流Ⅱ段起动",4630]
[85,"Arm131","高压侧零序过流Ⅰ段起动",4631]
[85,"Arm132","中压侧零序过流Ⅰ段起动",4632]
[85,"Arm133","中压侧零序过流Ⅱ段起动",4633]
[85,"Arm134","跳闸信号",4634]
[85,"Arm135","启动打印",4635]
[85,"Arm136","保护检修状态硬压板",4636]
[85,"Arm137","信号复归",4637]
[85,"Arm138","高压侧电压硬压板",4638]
[85,"Arm139","中压侧电压硬压板",4639]
[85,"Arm140","低压1分支电压硬压板",4640]
[85,"Arm141","低压2分支电压硬压板",4641]
[85,"Arm142","主保护硬压板",4642]
[85,"Arm143","高压侧后备保护硬压板",4643]
[85,"Arm144","中压侧后备保护硬压板",4644]
[85,"Arm145","低压1分支后备保护硬压板",4645]
[85,"Arm146","低压2分支后备保护硬压板",4646]
[85,"Arm147","高压侧失灵联跳开入",4647]
[85,"Arm148","中压侧失灵联跳开入",4648]
[85,"Arm149","远方操作硬压板",4649]
[85,"Arm150","高压侧TWJ",4650]
[85,"Arm151","中压侧TWJ",4651]
[85,"Arm152","纵差差动速断",4652]
[85,"Arm153","纵差保护",4653]
[85,"Arm154","纵差工频变化量差动",4654]
[85,"Arm155","高相间阻抗1时限",4655]
[85,"Arm156","高相间阻抗2时限",4656]
[85,"Arm157","高相间阻抗3时限",4657]
[85,"Arm158","高接地阻抗1时限",4658]
[85,"Arm159","高接地阻抗2时限",4659]
[85,"Arm160","高接地阻抗3时限",4660]
[85,"Arm161","高复流Ⅰ段1时限",4661]
[85,"Arm162","高复流Ⅰ段2时限",4662]
[85,"Arm163","高复流Ⅰ段3时限",4663]
[85,"Arm164","高复流Ⅱ段1时限",4664]
[85,"Arm165","高复流Ⅱ段2时限",4665]
[85,"Arm166","高复流Ⅱ段3时限",4666]
[85,"Arm167","高复流Ⅲ段1时限",4667]
[85,"Arm168","高复流Ⅲ段2时限",4668]
[85,"Arm169","高零流Ⅰ段1时限",4669]
[85,"Arm170","高零流Ⅰ段2时限",4670]
[85,"Arm171","高零流Ⅰ段3时限",4671]
[85,"Arm172","高零流Ⅱ段1时限",4672]
[85,"Arm173","高零流Ⅱ段2时限",4673]
[85,"Arm174","高零流Ⅱ段3时限",4674]
[85,"Arm175","高零流Ⅲ段1时限",4675]
[85,"Arm176","高零流Ⅲ段2时限",4676]
[85,"Arm177","高间隙过流",4677]
[85,"Arm178","高零序过压",4678]
[85,"Arm179","高断路器失灵联跳",4679]
[85,"Arm180","中相间阻抗1时限",4680]
[85,"Arm181","中相间阻抗2时限",4681]
[85,"Arm182","中相间阻抗3时限",4682]
[85,"Arm183","中接地阻抗1时限",4683]
[85,"Arm184","中接地阻抗2时限",4684]
[85,"Arm185","中接地阻抗3时限",4685]
[85,"Arm186","中复流Ⅰ段1时限",4686]
[85,"Arm187","中复流Ⅰ段2时限",4687]
[85,"Arm188","中复流Ⅰ段3时限",4688]
[85,"Arm189","中复流Ⅱ段1时限",4689]
[85,"Arm190","中复流Ⅱ段2时限",4690]
[85,"Arm191","中复流Ⅱ段3时限",4691]
[85,"Arm192","中复流Ⅲ段1时限",4692]
[85,"Arm193","中复流Ⅲ段2时限",4693]
[85,"Arm194","中零流Ⅰ段1时限",4694]
[85,"Arm195","中零流Ⅰ段2时限",4695]
[85,"Arm196","中零流Ⅰ段3时限",4696]
[85,"Arm197","中零流Ⅱ段1时限",4697]
[85,"Arm198","中零流Ⅱ段2时限",4698]
[85,"Arm199","中零流Ⅱ段3时限",4699]
[85,"Arm200","中零流Ⅲ段1时限",4700]
[85,"Arm201","中零流Ⅲ段2时限",4701]
[85,"Arm202","中间隙过流1时限",4702]
[85,"Arm203","中间隙过流2时限",4703]
[85,"Arm204","中零序过压1时限",4704]
[85,"Arm205","中零序过压2时限",4705]
[85,"Arm206","中断路器失灵联跳",4706]
[85,"Arm207","低1复流Ⅰ段1时限",4707]
[85,"Arm208","低1复流Ⅰ段2时限",4708]
[85,"Arm209","低1复流Ⅰ段3时限",4709]
[85,"Arm210","低1复流Ⅱ段1时限",4710]
[85,"Arm211","低1复流Ⅱ段2时限",4711]
[85,"Arm212","低1复流Ⅱ段3时限",4712]
[85,"Arm213","低2复流Ⅰ段1时限",4713]
[85,"Arm214","低2复流Ⅰ段2时限",4714]
[85,"Arm215","低2复流Ⅰ段3时限",4715]
[85,"Arm216","低2复流Ⅱ段1时限",4716]
[85,"Arm217","低2复流Ⅱ段2时限",4717]
[85,"Arm218","低2复流Ⅱ段3时限",4718]
[85,"Arm219","跳高压侧",4719]
[85,"Arm220","跳高压侧母联",4720]
[85,"Arm221","跳中压侧",4721]
[85,"Arm222","跳中压侧母联",4722]
[85,"Arm223","跳低压1分支",4723]
[85,"Arm224","跳低压1分段",4724]
[85,"Arm225","跳低压2分支",4725]
[85,"Arm226","跳低压2分段",4726]
[85,"Arm227","闭锁中压侧备自投",4727]
[85,"Arm228","闭锁低压1分支备自投",4728]
[85,"Arm229","闭锁低压2分支备自投",4729]
[85,"Arm230","跳备用出口1~4",4730]
[85,"Arm231","保护启动",4731]
[85,"Arm232","高压侧过负荷",4732]
[85,"Arm233","中压侧过负荷",4733]
[85,"Arm234","低压1分支零序过压报警",4734]
[85,"Arm235","低压2分支零序过压报警",4735]
[85,"Arm236","低压侧过负荷",4736]
[85,"Arm237","失灵开入异常",4737]
[85,"Arm238","高压1侧CT异常",4738]
[85,"Arm239","高压1侧CT断线",4739]
[85,"Arm240","高压2侧CT异常",4740]
[85,"Arm241","高压2侧CT断线",4741]
[85,"Arm242","中压侧CT异常",4742]
[85,"Arm243","中压侧CT断线",4743]
[85,"Arm244","低压1分支CT异常",4744]
[85,"Arm245","低压1分支CT断线",4745]
[85,"Arm246","低压2分支CT异常",4746]
[85,"Arm247","低压2分支CT断线",4747]
[85,"Arm248","高压侧PT断线",4748]
[85,"Arm249","中压侧PT断线",4749]
[85,"Arm250","低压1分支PT断线",4750]
[85,"Arm251","低压2分支PT断线",4751]
[85,"Arm252","频率异常告警",4752]
[85,"Arm253","差流越限",4753]
[85,"Arm254","纵差回路断线告警",4754]
[85,"Arm255","高压侧失灵联跳节点告警",4755]
[85,"Arm256","高压侧失灵联跳电流告警",4756]
[85,"Arm257","中压侧失灵联跳节点告警",4757]
[85,"Arm258","中压侧失灵联跳电流告警",4758]
[85,"Arm259","保护板长期启动",4759]
[85,"Arm260","启动板长期启动",4760]
[85,"Arm261","主保护软压板",4761]
[85,"Arm262","高压侧后备保护软压板",4762]
[85,"Arm263","中压侧后备保护软压板",4763]
[85,"Arm264","低压1分支后备保护软压板",4764]
[85,"Arm265","低压2分支后备保护软压板",4765]
[85,"Arm266","远方投退压板软压板",4766]
[85,"Arm267","远方切换定值区软压板",4767]
[85,"Arm268","远方修改定值软压板",4768]
[85,"Arm269","网络状态1",4769]
[85,"Arm270","网络状态2",4770]
[85,"Arm271","装置通讯状态",4771]
[85,"Arm272","检修状态",4772]
[85,"Arm273","参数变化",4773]
[85,"Arm274","就地状态虚遥信",4774]
[85,"Arm275","遥控解除闭锁",4775]
[85,"Arm276","A网中断",4776]
[85,"Arm277","B网中断",4777]
[85,"Arm278","网络中断",4778]
[86,"Arm1","模拟量采集错",4779]
[86,"Arm2","跳闸失败",4780]
[86,"Arm3","设备参数错",4781]
[86,"Arm4","ROM和校验错",4782]
[86,"Arm5","定值错",4783]
[86,"Arm6","定值区指针错",4784]
[86,"Arm7","开出不响应",4785]
[86,"Arm8","开出击穿",4786]
[86,"Arm9","压板模式未确认",4787]
[86,"Arm10","SRAM自检异常",4788]
[86,"Arm11","FLASH自检异常",4789]
[86,"Arm12","自描述错",4790]
[86,"Arm13","开入状态未复归",4791]
[86,"Arm14","软压板错",4792]
[86,"Arm15","系统配置错",4793]
[86,"Arm16","CAN通讯中断",4794]
[86,"Arm17","CAN通讯恢复",4795]
[86,"Arm18","开入模件异常",4796]
[86,"Arm19","开出模件异常",4797]
[86,"Arm20","开入配置错",4798]
[86,"Arm21","开出配置错",4799]
[86,"Arm22","开入通讯中断",4800]
[86,"Arm23","开出通讯中断",4801]
[86,"Arm24","传动状态未复归",4802]
[86,"Arm25","开入击穿",4803]
[86,"Arm26","开入输入不正常",4804]
[86,"Arm27","双位置输入不一致",4805]
[86,"Arm28","开入自检回路出错",4806]
[86,"Arm29","开入EEPROM出错",4807]
[86,"Arm30","开出EEPROM出错",4808]
[86,"Arm31","X12-a6输入3T1",4809]
[86,"Arm32","X12-a6输入3T2",4810]
[86,"Arm33","X12-a6输入3T3",4811]
[86,"Arm34","X12-a6输入3",4812]
[86,"Arm35","X12-c6输入4",4813]
[86,"Arm36","X12-a4输入1",4814]
[86,"Arm37","X12-c4输入2",4815]
[86,"Arm38","X3-a4输入1",4816]
[86,"Arm39","X3-c4输入2",4817]
[86,"Arm40","X3-a6输入3",4818]
[86,"Arm41","X3-c6输入4",4819]
[86,"Arm42","X4-a4输入1",4820]
[86,"Arm43","X4-c4输入2",4821]
[86,"Arm44","X4-a6输入3",4822]
[86,"Arm45","X4-c6输入4",4823]
[86,"Arm46","X5-a4输入1",4824]
[86,"Arm47","X5-c4输入2",4825]
[86,"Arm48","X5-a6输入3",4826]
[86,"Arm49","X5-c6输入4",4827]
[86,"Arm50","X13-a4输入1",4828]
[86,"Arm51","X13-c4输入2",4829]
[86,"Arm52","X13-a6输入3",4830]
[86,"Arm53","X13-c6输入4",4831]
[86,"Arm54","CPU异常",4832]
[86,"Arm55","设备参数不一致",4833]
[86,"Arm56","定值区号不一致",4834]
[86,"Arm57","定值不一致",4835]
[86,"Arm58","压板不一致",4836]
[86,"Arm59","LON1通讯中断",4837]
[86,"Arm60","LON2通讯中断",4838]
[86,"Arm61","压板模式不一致",4839]
[86,"Arm62","召唤配置无应答",4840]
[86,"Arm63","PLC逻辑校验出错",4841]
[86,"Arm64","信号复归",4842]
[86,"Arm65","X12-a6输入3_(重复1)",4843]
[86,"Arm66","X12-c6输入4_(重复1)",4844]
[86,"Arm67","X12-a4输入1_(重复1)",4845]
[86,"Arm68","X12-c4输入2_(重复1)",4846]
[86,"Arm69","X3-a4输入1_(重复1)",4847]
[86,"Arm70","X3-c4输入2_(重复1)",4848]
[86,"Arm71","X3-a6输入3_(重复1)",4849]
[86,"Arm72","X3-c6输入4_(重复1)",4850]
[86,"Arm73","X4-a4输入1_(重复1)",4851]
[86,"Arm74","X4-c4输入2_(重复1)",4852]
[86,"Arm75","X4-a6输入3_(重复1)",4853]
[86,"Arm76","X4-c6输入4_(重复1)",4854]
[86,"Arm77","X5-a4输入1_(重复1)",4855]
[86,"Arm78","X5-c4输入2_(重复1)",4856]
[86,"Arm79","X5-a6输入3_(重复1)",4857]
[86,"Arm80","X5-c6输入4_(重复1)",4858]
[86,"Arm81","X13-a4输入1_(重复1)",4859]
[86,"Arm82","X13-c4输入2_(重复1)",4860]
[86,"Arm83","X13-a6输入3_(重复1)",4861]
[86,"Arm84","X13-c6输入4_(重复1)",4862]
[86,"Arm85","检修状态压板",4863]
[86,"Arm86","远方修改定值",4864]
[86,"Arm87","保护启动",4865]
[86,"Arm88","X3-a4输入1_(重复2)",4866]
[86,"Arm89","X3-c4输入2_(重复2)",4867]
[86,"Arm90","X3-a6输入3_(重复2)",4868]
[86,"Arm91","X3-c6输入4_(重复2)",4869]
[86,"Arm92","X4-a4输入1_(重复2)",4870]
[86,"Arm93","X4-c4输入2_(重复2)",4871]
[86,"Arm94","X4-a6输入3_(重复2)",4872]
[86,"Arm95","X4-c6输入4_(重复2)",4873]
[86,"Arm96","X5-a4输入1_(重复2)",4874]
[86,"Arm97","X5-c4输入2_(重复2)",4875]
[86,"Arm98","X5-a6输入3_(重复2)",4876]
[86,"Arm99","X5-c6输入4_(重复2)",4877]
[86,"Arm100","X13-a4输入1_(重复2)",4878]
[86,"Arm101","X13-c4输入2_(重复2)",4879]
[86,"Arm102","X13-a6输入3_(重复2)",4880]
[86,"Arm103","X13-c6输入4_(重复2)",4881]
[86,"Arm104","X12-a6输入3T1_(重复1)",4882]
[86,"Arm105","X12-a6输入3T2_(重复1)",4883]
[86,"Arm106","X12-a6输入3T3_(重复1)",4884]
[86,"Arm107","X12-a6输入3_(重复2)",4885]
[86,"Arm108","X12-c6输入4_(重复2)",4886]
[86,"Arm109","X12-a4输入1_(重复2)",4887]
[86,"Arm110","X12-c4输入2_(重复2)",4888]
[86,"Arm111","录波完成",4889]
[86,"Arm112","录波启动",4890]
[86,"Arm113","网络状态1",4891]
[86,"Arm114","网络状态2",4892]
[86,"Arm115","装置通讯状态",4893]
[86,"Arm116","检修状态",4894]
[86,"Arm117","参数变化",4895]
[86,"Arm118","就地状态虚遥信",4896]
[86,"Arm119","遥控解除闭锁",4897]
[86,"Arm120","A网中断",4898]
[86,"Arm121","B网中断",4899]
[86,"Arm122","网络中断",4900]
[87,"Arm1","光纤通道一硬压板",4901]
[87,"Arm2","光纤通道二硬压板",4902]
[87,"Arm3","距离保护硬压板",4903]
[87,"Arm4","零序过流保护硬压板",4904]
[87,"Arm5","停用重合闸硬压板",4905]
[87,"Arm6","远方操作硬压板",4906]
[87,"Arm7","保护检修状态硬压板",4907]
[87,"Arm8","启动打印",4908]
[87,"Arm9","信号复归",4909]
[87,"Arm10","模拟量采集错",4910]
[87,"Arm11","工程配置文件错误",4911]
[87,"Arm12","定值自检出错",4912]
[87,"Arm13","开出异常",4913]
[87,"Arm14","保护程序校验出错",4914]
[87,"Arm15","保护CPU插件异常",4915]
[87,"Arm16","FLASH自检出错",4916]
[87,"Arm17","对时信号状态",4917]
[87,"Arm18","通信中断",4918]
[87,"Arm19","时间跳变侦测状态",4919]
[87,"Arm20","对时服务状态",4920]
[87,"Arm21","双CPU通讯中断",4921]
[87,"Arm22","对时异常",4922]
[87,"Arm23","运行",4923]
[87,"Arm24","异常",4924]
[87,"Arm25","检修",4925]
[87,"Arm26","纵联保护闭锁",4926]
[87,"Arm27","充电完成",4927]
[87,"Arm28","保护跳闸",4928]
[87,"Arm29","重合闸",4929]
[87,"Arm30","光纤通道一投入",4930]
[87,"Arm31","光纤通道二投入",4931]
[87,"Arm32","距离保护投入",4932]
[87,"Arm33","零序过流保护投入",4933]
[87,"Arm34","差动A相有效",4934]
[87,"Arm35","差动B相有效",4935]
[87,"Arm36","差动C相有效",4936]
[87,"Arm37","零序差动有效",4937]
[87,"Arm38","远方其它保护有效",4938]
[87,"Arm39","距离保护Ⅰ段有效",4939]
[87,"Arm40","距离保护Ⅱ段有效",4940]
[87,"Arm41","距离保护Ⅲ段有效",4941]
[87,"Arm42","零序过流Ⅱ段有效",4942]
[87,"Arm43","零序过流Ⅲ段有效",4943]
[87,"Arm44","零序反时限有效",4944]
[87,"Arm45","重合闸有效",4945]
[87,"Arm46","闭锁主保护",4946]
[87,"Arm47","闭锁后备保护",4947]
[87,"Arm48","闭锁重合闸_(重复1)",4948]
[87,"Arm49","闭锁远方其它保护",4949]
[87,"Arm50","录波就绪",4950]
[87,"Arm51","光纤通道一软压板",4951]
[87,"Arm52","光纤通道二软压板",4952]
[87,"Arm53","距离保护软压板",4953]
[87,"Arm54","零序过流保护软压板",4954]
[87,"Arm55","停用重合闸软压板",4955]
[87,"Arm56","远方投退压板软压板",4956]
[87,"Arm57","远方切换定值区软压板",4957]
[87,"Arm58","远方修改定值软压板",4958]
[87,"Arm59","装置长期启动",4959]
[87,"Arm60","零序反时限长期启动",4960]
[87,"Arm61","通道一两侧差动投退不一致",4961]
[87,"Arm62","通道二两侧差动投退不一致",4962]
[87,"Arm63","通道一对侧异常",4963]
[87,"Arm64","通道二对侧异常",4964]
[87,"Arm65","事故总",4965]
[87,"Arm66","预告总",4966]
[87,"Arm67","PT断线",4967]
[87,"Arm68","CT断线",4968]
[87,"Arm69","通道一长期有差流",4969]
[87,"Arm70","A相跳位有流",4970]
[87,"Arm71","B相跳位有流",4971]
[87,"Arm72","C相跳位有流",4972]
[87,"Arm73","重合方式整定出错",4973]
[87,"Arm74","同期电压异常",4974]
[87,"Arm75","纵联通道一接收中断",4975]
[87,"Arm76","纵联通道一装置混联",4976]
[87,"Arm77","纵联通道一混联",4977]
[87,"Arm78","通道一自环与整定异常",4978]
[87,"Arm79","纵联通道一误码高告警",4979]
[87,"Arm80","纵联通道一延时长",4980]
[87,"Arm81","通道一告警",4981]
[87,"Arm82","纵联通道二接收中断",4982]
[87,"Arm83","纵联通道二装置混联",4983]
[87,"Arm84","纵联通道二混联",4984]
[87,"Arm85","通道二自环与整定异常",4985]
[87,"Arm86","纵联通道二误码高告警",4986]
[87,"Arm87","纵联通道二延时长",4987]
[87,"Arm88","通道二告警",4988]
[87,"Arm89","通道故障",4989]
[87,"Arm90","其它保护开入异常",4990]
[87,"Arm91","通道二长期有差流",4991]
[87,"Arm92","通道一对侧通道异常",4992]
[87,"Arm93","通道二对侧通道异常",4993]
[87,"Arm94","远传1开入异常",4994]
[87,"Arm95","其它保护收信异常",4995]
[87,"Arm96","远传1收信异常",4996]
[87,"Arm97","对侧CT断线",4997]
[87,"Arm98","跳A相",4998]
[87,"Arm99","跳B相",4999]
[87,"Arm100","跳C相",5000]
[87,"Arm101","低气压闭锁重合闸",5001]
[87,"Arm102","重合闸充电完成",5002]
[87,"Arm103","远传1开出",5003]
[87,"Arm104","远传2开出",5004]
[87,"Arm105","闭锁重合闸",5005]
[87,"Arm106","远传1",5006]
[87,"Arm107","远传2",5007]
[87,"Arm108","其它保护动作",5008]
[87,"Arm109","分相跳闸位置TWJa",5009]
[87,"Arm110","分相跳闸位置TWJb",5010]
[87,"Arm111","分相跳闸位置TWJc",5011]
[87,"Arm112","纵联通道一自环",5012]
[87,"Arm113","纵联通道二自环",5013]
[87,"Arm114","保护启动",5014]
[87,"Arm115","保护动作",5015]
[87,"Arm116","沟通三跳",5016]
[87,"Arm117","跳闸失败",5017]
[87,"Arm118","永跳动作",5018]
[87,"Arm119","距离加速动作",5019]
[87,"Arm120","零序加速动作",5020]
[87,"Arm121","零序过流Ⅱ段动作",5021]
[87,"Arm122","零序过流Ⅲ段动作",5022]
[87,"Arm123","零序反时限动作",5023]
[87,"Arm124","远方其它保护动作",5024]
[87,"Arm125","快速距离保护动作",5025]
[87,"Arm126","分相差动动作",5026]
[87,"Arm127","接地距离Ⅰ段动作",5027]
[87,"Arm128","接地距离Ⅱ段动作",5028]
[87,"Arm129","接地距离Ⅲ段动作",5029]
[87,"Arm130","相间距离Ⅰ段动作",5030]
[87,"Arm131","相间距离Ⅱ段动作",5031]
[87,"Arm132","相间距离Ⅲ段动作",5032]
[87,"Arm133","零序差动动作",5033]
[87,"Arm134","重合闸动作",5034]
[87,"Arm135","网络状态1",5035]
[87,"Arm136","网络状态2",5036]
[87,"Arm137","装置通讯状态",5037]
[87,"Arm138","检修状态",5038]
[87,"Arm139","参数变化",5039]
[87,"Arm140","就地状态虚遥信",5040]
[87,"Arm141","遥控解除闭锁",5041]
[87,"Arm142","A网中断",5042]
[87,"Arm143","B网中断",5043]
[87,"Arm144","网络中断",5044]
[88,"Arm1","启动打印",5045]
[88,"Arm2","保护检修状态硬压板",5046]
[88,"Arm3","信号复归",5047]
[88,"Arm4","远方操作硬压板",5048]
[88,"Arm5","不停电传动使能",5049]
[88,"Arm6","A相不停电传动",5050]
[88,"Arm7","B相不停电传动",5051]
[88,"Arm8","C相不停电传动",5052]
[88,"Arm9","三相不停电传动",5053]
[88,"Arm10","开出传动使能",5054]
[88,"Arm11","A相跳闸出口",5055]
[88,"Arm12","B相跳闸出口",5056]
[88,"Arm13","C相跳闸出口",5057]
[88,"Arm14","重合闸出口",5058]
[88,"Arm15","保护跳闸出口",5059]
[88,"Arm16","保护三跳出口",5060]
[88,"Arm17","闭锁重合闸出口",5061]
[88,"Arm18","手动触发录波",5062]
[88,"Arm19","装置闭锁",5063]
[88,"Arm20","CID文件错误",5064]
[88,"Arm21","定值超范围",5065]
[88,"Arm22","板卡配置错误",5066]
[88,"Arm23","定值项变化告警",5067]
[88,"Arm24","插件8异常",5068]
[88,"Arm25","插件9异常",5069]
[88,"Arm26","插件11异常",5070]
[88,"Arm27","装置报警",5071]
[88,"Arm28","通信传动报警",5072]
[88,"Arm29","对时信号状态",5073]
[88,"Arm30","对时服务状态",5074]
[88,"Arm31","时间跳变侦测状态",5075]
[88,"Arm32","对时异常",5076]
[88,"Arm33","版本错误报警",5077]
[88,"Arm34","定值校验出错",5078]
[88,"Arm35","定值区不一致",5079]
[88,"Arm36","定值修改",5080]
[88,"Arm37","定值区切换",5081]
[88,"Arm38","内存不足",5082]
[88,"Arm39","IEC103配置文件无效",5083]
[88,"Arm40","插件8光耦电源异常",5084]
[88,"Arm41","插件9光耦电源异常",5085]
[88,"Arm42","电源异常",5086]
[88,"Arm43","装置高温告警",5087]
[88,"Arm44","装置低温告警",5088]
[88,"Arm45","装置电源监视告警",5089]
[88,"Arm46","纵联通道一接收光强越限告警",5090]
[88,"Arm47","纵联通道二接收光强越限告警",5091]
[88,"Arm48","运行",5092]
[88,"Arm49","异常",5093]
[88,"Arm50","检修",5094]
[88,"Arm51","纵联保护闭锁",5095]
[88,"Arm52","充电完成",5096]
[88,"Arm53","保护跳闸",5097]
[88,"Arm54","重合闸",5098]
[88,"Arm55","零序过流保护投入",5099]
[88,"Arm56","距离保护投入",5100]
[88,"Arm57","光纤通道一投入",5101]
[88,"Arm58","光纤通道二投入",5102]
[88,"Arm59","差动A相有效",5103]
[88,"Arm60","差动B相有效",5104]
[88,"Arm61","差动C相有效",5105]
[88,"Arm62","零序差动有效",5106]
[88,"Arm63","远方其它保护有效",5107]
[88,"Arm64","距离保护Ⅰ段有效",5108]
[88,"Arm65","距离保护Ⅱ段有效",5109]
[88,"Arm66","距离保护Ⅲ段有效",5110]
[88,"Arm67","零序过流Ⅱ段有效",5111]
[88,"Arm68","零序过流Ⅲ段有效",5112]
[88,"Arm69","零序反时限有效",5113]
[88,"Arm70","重合闸有效",5114]
[88,"Arm71","工频变化量距离有效",5115]
[88,"Arm72","闭锁主保护",5116]
[88,"Arm73","闭锁后备保护",5117]
[88,"Arm74","闭锁重合闸_(重复1)",5118]
[88,"Arm75","闭锁远方其它保护",5119]
[88,"Arm76","录波完成",5120]
[88,"Arm77","光纤通道一硬压板",5121]
[88,"Arm78","光纤通道二硬压板",5122]
[88,"Arm79","距离保护硬压板",5123]
[88,"Arm80","零序过流保护硬压板",5124]
[88,"Arm81","停用重合闸硬压板",5125]
[88,"Arm82","闭锁重合闸",5126]
[88,"Arm83","低气压闭锁重合闸",5127]
[88,"Arm84","分相跳闸位置TWJa",5128]
[88,"Arm85","分相跳闸位置TWJb",5129]
[88,"Arm86","分相跳闸位置TWJc",5130]
[88,"Arm87","其它保护动作",5131]
[88,"Arm88","远传1",5132]
[88,"Arm89","远传2",5133]
[88,"Arm90","闭锁重合闸_OPT",5134]
[88,"Arm91","低气压闭锁重合闸_OPT",5135]
[88,"Arm92","分相跳闸位置TWJa_OPT",5136]
[88,"Arm93","分相跳闸位置TWJb_OPT",5137]
[88,"Arm94","分相跳闸位置TWJc_OPT",5138]
[88,"Arm95","其它保护动作_OPT",5139]
[88,"Arm96","远传1_OPT",5140]
[88,"Arm97","远传2_OPT",5141]
[88,"Arm98","通道一收其它保护动作",5142]
[88,"Arm99","通道一收远传1",5143]
[88,"Arm100","通道一收远传2",5144]
[88,"Arm101","通道一对侧差动压板",5145]
[88,"Arm102","通道二收其它保护动作",5146]
[88,"Arm103","通道二收远传1",5147]
[88,"Arm104","通道二收远传2",5148]
[88,"Arm105","通道二对侧差动压板",5149]
[88,"Arm106","收其它保护动作",5150]
[88,"Arm107","收远传1",5151]
[88,"Arm108","收远传2",5152]
[88,"Arm109","重合闸充电完成",5153]
[88,"Arm110","远传1出口",5154]
[88,"Arm111","远传2出口",5155]
[88,"Arm112","通道告警出口",5156]
[88,"Arm113","A相跳闸出口_(重复1)",5157]
[88,"Arm114","B相跳闸出口_(重复1)",5158]
[88,"Arm115","C相跳闸出口_(重复1)",5159]
[88,"Arm116","重合闸出口_(重复1)",5160]
[88,"Arm117","保护跳闸出口_(重复1)",5161]
[88,"Arm118","保护三跳出口_(重复1)",5162]
[88,"Arm119","闭锁重合闸出口_(重复1)",5163]
[88,"Arm120","装置异常启动录波",5164]
[88,"Arm121","保护启动",5165]
[88,"Arm122","A相跳闸动作",5166]
[88,"Arm123","B相跳闸动作",5167]
[88,"Arm124","C相跳闸动作",5168]
[88,"Arm125","保护动作",5169]
[88,"Arm126","重合闸动作",5170]
[88,"Arm127","纵联差动保护动作",5171]
[88,"Arm128","工频变化量阻抗动作",5172]
[88,"Arm129","接地距离Ⅰ段动作",5173]
[88,"Arm130","相间距离Ⅰ段动作",5174]
[88,"Arm131","接地距离Ⅱ段动作",5175]
[88,"Arm132","相间距离Ⅱ段动作",5176]
[88,"Arm133","接地距离Ⅲ段动作",5177]
[88,"Arm134","相间距离Ⅲ段动作",5178]
[88,"Arm135","距离加速动作",5179]
[88,"Arm136","零序加速动作",5180]
[88,"Arm137","零序过流Ⅱ段动作",5181]
[88,"Arm138","零序过流Ⅲ段动作",5182]
[88,"Arm139","零序反时限动作",5183]
[88,"Arm140","选相无效三跳",5184]
[88,"Arm141","远方其它保护动作",5185]
[88,"Arm142","加速联跳动作",5186]
[88,"Arm143","单跳失败三跳",5187]
[88,"Arm144","单相运行三跳",5188]
[88,"Arm145","不停电传动跳闸",5189]
[88,"Arm146","保护CPU插件异常",5190]
[88,"Arm147","开出异常",5191]
[88,"Arm148","模拟量采集错",5192]
[88,"Arm149","启动DSP定值出错",5193]
[88,"Arm150","启动DSP内存出错",5194]
[88,"Arm151","启动DSP采样出错",5195]
[88,"Arm152","启动DSP校验出错",5196]
[88,"Arm153","启动DSP装置类型配置错",5197]
[88,"Arm154","跳合出口回路异常",5198]
[88,"Arm155","保护DSP装置类型配置错",5199]
[88,"Arm156","保护DSP校验出错",5200]
[88,"Arm157","保护DSP定值出错",5201]
[88,"Arm158","保护DSP内存出错",5202]
[88,"Arm159","保护DSP采样出错",5203]
[88,"Arm160","开入异常",5204]
[88,"Arm161","其它保护开入异常",5205]
[88,"Arm162","保护同期电压采样出错",5206]
[88,"Arm163","跳闸位置开入异常",5207]
[88,"Arm164","通道一无有效帧",5208]
[88,"Arm165","通道一识别码错",5209]
[88,"Arm166","通道一严重误码",5210]
[88,"Arm167","通道一连接错误",5211]
[88,"Arm168","通道二无有效帧",5212]
[88,"Arm169","通道二识别码错",5213]
[88,"Arm170","通道二严重误码",5214]
[88,"Arm171","通道二连接错误",5215]
[88,"Arm172","通道一通道异常",5216]
[88,"Arm173","通道一差动退出",5217]
[88,"Arm174","通道一差动自环异常",5218]
[88,"Arm175","通道一两侧差动投退不一致",5219]
[88,"Arm176","通道一同步异常",5220]
[88,"Arm177","通道一对侧异常闭锁差动",5221]
[88,"Arm178","通道一对侧CT断线",5222]
[88,"Arm179","通道二通道异常",5223]
[88,"Arm180","通道二差动退出",5224]
[88,"Arm181","通道二差动自环异常",5225]
[88,"Arm182","通道二两侧差动投退不一致",5226]
[88,"Arm183","通道二同步异常",5227]
[88,"Arm184","通道二对侧异常闭锁差动",5228]
[88,"Arm185","通道二对侧CT断线",5229]
[88,"Arm186","通道故障",5230]
[88,"Arm187","对侧CT断线",5231]
[88,"Arm188","其它保护收信异常",5232]
[88,"Arm189","长期启动报警",5233]
[88,"Arm190","零序长期启动",5234]
[88,"Arm191","CT断线",5235]
[88,"Arm192","PT断线",5236]
[88,"Arm193","同期电压异常",5237]
[88,"Arm194","保护PT中性线断线",5238]
[88,"Arm195","零序反时限告警",5239]
[88,"Arm196","通道一长期有差流",5240]
[88,"Arm197","通道一补偿参数错",5241]
[88,"Arm198","通道一CT变比失配",5242]
[88,"Arm199","通道二长期有差流",5243]
[88,"Arm200","通道二补偿参数错",5244]
[88,"Arm201","通道二CT变比失配",5245]
[88,"Arm202","重合方式整定出错",5246]
[88,"Arm203","光纤通道一软压板",5247]
[88,"Arm204","光纤通道二软压板",5248]
[88,"Arm205","距离保护软压板",5249]
[88,"Arm206","零序过流保护软压板",5250]
[88,"Arm207","停用重合闸软压板",5251]
[88,"Arm208","远方投退压板软压板",5252]
[88,"Arm209","远方切换定值区软压板",5253]
[88,"Arm210","远方修改定值软压板",5254]
[88,"Arm211","网络状态1",5255]
[88,"Arm212","网络状态2",5256]
[88,"Arm213","装置通讯状态",5257]
[88,"Arm214","检修状态",5258]
[88,"Arm215","参数变化",5259]
[88,"Arm216","就地状态虚遥信",5260]
[88,"Arm217","遥控解除闭锁",5261]
[88,"Arm218","A网中断",5262]
[88,"Arm219","B网中断",5263]
[88,"Arm220","网络中断",5264]
[89,"Arm1","I类告警总",5265]
[89,"Arm2","模拟量采集错",5266]
[89,"Arm3","设备参数错",5267]
[89,"Arm4","ROM和校验错",5268]
[89,"Arm5","定值错",5269]
[89,"Arm6","定值区指针错",5270]
[89,"Arm7","软压板错",5271]
[89,"Arm8","系统配置错",5272]
[89,"Arm9","开出异常",5273]
[89,"Arm10","开出配置错",5274]
[89,"Arm11","保护CPU插件异常",5275]
[89,"Arm12","开出EEPROM出错",5276]
[89,"Arm13","CPU通讯中断",5277]
[89,"Arm14","设备参数不一致",5278]
[89,"Arm15","定值区号不一致",5279]
[89,"Arm16","定值不一致",5280]
[89,"Arm17","压板不一致",5281]
[89,"Arm18","召唤配置无应答",5282]
[89,"Arm19","对时异常",5283]
[89,"Arm20","通道一光收越上限",5284]
[89,"Arm21","通道一光收越下限",5285]
[89,"Arm22","通道一光发越上限",5286]
[89,"Arm23","通道一光发越下限",5287]
[89,"Arm24","通道二光收越上限",5288]
[89,"Arm25","通道二光收越下限",5289]
[89,"Arm26","通道二光发越上限",5290]
[89,"Arm27","通道二光发越下限",5291]
[89,"Arm28","对时信号状态",5292]
[89,"Arm29","对时服务状态",5293]
[89,"Arm30","时间跳变侦测状态",5294]
[89,"Arm31","光纤通道一硬压板",5295]
[89,"Arm32","光纤通道二硬压板",5296]
[89,"Arm33","距离保护硬压板",5297]
[89,"Arm34","零序过流保护硬压板",5298]
[89,"Arm35","停用重合闸硬压板",5299]
[89,"Arm36","远方操作硬压板",5300]
[89,"Arm37","保护检修状态硬压板",5301]
[89,"Arm38","光纤通道一总压板",5302]
[89,"Arm39","光纤通道二总压板",5303]
[89,"Arm40","距离保护总压板",5304]
[89,"Arm41","零序过流保护总压板",5305]
[89,"Arm42","停用重合闸总压板",5306]
[89,"Arm43","运行",5307]
[89,"Arm44","异常",5308]
[89,"Arm45","检修",5309]
[89,"Arm46","纵联保护闭锁",5310]
[89,"Arm47","充电完成",5311]
[89,"Arm48","保护跳闸",5312]
[89,"Arm49","重合闸",5313]
[89,"Arm50","差动A相有效",5314]
[89,"Arm51","差动B相有效",5315]
[89,"Arm52","差动C相有效",5316]
[89,"Arm53","零序差动有效",5317]
[89,"Arm54","远方其它保护有效",5318]
[89,"Arm55","距离保护Ⅰ段有效",5319]
[89,"Arm56","距离保护Ⅱ段有效",5320]
[89,"Arm57","距离保护Ⅲ段有效",5321]
[89,"Arm58","零序过流Ⅱ段有效",5322]
[89,"Arm59","零序过流Ⅲ段有效",5323]
[89,"Arm60","零序反时限有效",5324]
[89,"Arm61","重合闸有效",5325]
[89,"Arm62","闭锁主保护",5326]
[89,"Arm63","闭锁后备保护",5327]
[89,"Arm64","闭锁重合闸_(重复2)",5328]
[89,"Arm65","闭锁远方其它保护",5329]
[89,"Arm66","光纤通道一投入",5330]
[89,"Arm67","光纤通道二投入",5331]
[89,"Arm68","距离保护投入",5332]
[89,"Arm69","零序过流保护投入",5333]
[89,"Arm70","录波完成",5334]
[89,"Arm71","录波启动",5335]
[89,"Arm72","光纤通道一软压板",5336]
[89,"Arm73","光纤通道二软压板",5337]
[89,"Arm74","距离保护软压板",5338]
[89,"Arm75","零序过流保护软压板",5339]
[89,"Arm76","停用重合闸软压板",5340]
[89,"Arm77","远方投退压板软压板",5341]
[89,"Arm78","远方切换定值区软压板",5342]
[89,"Arm79","远方修改定值软压板",5343]
[89,"Arm80","信号复归",5344]
[89,"Arm81","分相跳闸位置TWJa",5345]
[89,"Arm82","分相跳闸位置TWJb",5346]
[89,"Arm83","分相跳闸位置TWJc",5347]
[89,"Arm84","闭锁重合闸",5348]
[89,"Arm85","远传1",5349]
[89,"Arm86","远传2",5350]
[89,"Arm87","其它保护动作",5351]
[89,"Arm88","低气压闭锁重合闸",5352]
[89,"Arm89","重合闸充电完成",5353]
[89,"Arm90","保护动作",5354]
[89,"Arm91","零序辅助启动",5355]
[89,"Arm92","故障测距",5356]
[89,"Arm93","测距阻抗",5357]
[89,"Arm94","单跳启动重合",5358]
[89,"Arm95","三跳启动重合",5359]
[89,"Arm96","单相不对应启重合",5360]
[89,"Arm97","三相不对应启重合",5361]
[89,"Arm98","三跳闭锁重合闸",5362]
[89,"Arm99","同期相别改变",5363]
[89,"Arm100","单跳闭锁重合闸",5364]
[89,"Arm101","采样失步",5365]
[89,"Arm102","采样已同步",5366]
[89,"Arm103","闭锁重合闸_(重复1)",5367]
[89,"Arm104","数据来源通道一",5368]
[89,"Arm105","数据来源通道二",5369]
[89,"Arm106","其它保护动作开入",5370]
[89,"Arm107","远传命令1开入",5371]
[89,"Arm108","远传命令2开入",5372]
[89,"Arm109","对侧差动动作",5373]
[89,"Arm110","低气压闭锁重合闸_(重复1)",5374]
[89,"Arm111","闭锁重合闸开入",5375]
[89,"Arm112","保护启动",5376]
[89,"Arm113","三跳失败",5377]
[89,"Arm114","单跳失败三跳",5378]
[89,"Arm115","三相差动电流",5379]
[89,"Arm116","三相制动电流",5380]
[89,"Arm117","联跳三跳",5381]
[89,"Arm118","故障相电压",5382]
[89,"Arm119","阻抗元件启动",5383]
[89,"Arm120","静稳失稳启动",5384]
[89,"Arm121","距离Ⅱ段加速动作",5385]
[89,"Arm122","距离Ⅲ段加速动作",5386]
[89,"Arm123","距离相近加速动作",5387]
[89,"Arm124","距离Ⅰ段发展动作",5388]
[89,"Arm125","距离Ⅱ段发展动作",5389]
[89,"Arm126","距离加速动作",5390]
[89,"Arm127","零序过流Ⅱ段动作",5391]
[89,"Arm128","零序过流Ⅲ段动作",5392]
[89,"Arm129","零序手合加速动作",5393]
[89,"Arm130","重合闸动作",5394]
[89,"Arm131","分相差动动作",5395]
[89,"Arm132","零序差动动作",5396]
[89,"Arm133","差动发展动作",5397]
[89,"Arm134","差动手合动作",5398]
[89,"Arm135","差动弱馈启动",5399]
[89,"Arm136","差动远方召唤启动",5400]
[89,"Arm137","纵联差动保护动作",5401]
[89,"Arm138","远方其它保护动作",5402]
[89,"Arm139","远传命令1返回",5403]
[89,"Arm140","远传命令2返回",5404]
[89,"Arm141","远传命令1开出",5405]
[89,"Arm142","远传命令2开出",5406]
[89,"Arm143","CT变比差异大",5407]
[89,"Arm144","零序加速动作",5408]
[89,"Arm145","接地距离Ⅰ段动作",5409]
[89,"Arm146","接地距离Ⅱ段动作",5410]
[89,"Arm147","接地距离Ⅲ段动作",5411]
[89,"Arm148","相间距离Ⅰ段动作",5412]
[89,"Arm149","相间距离Ⅱ段动作",5413]
[89,"Arm150","相间距离Ⅲ段动作",5414]
[89,"Arm151","故障相电流",5415]
[89,"Arm152","II类告警总",5416]
[89,"Arm153","CT变比差异大",5417]
[89,"Arm154","SRAM自检异常",5418]
[89,"Arm155","FLASH自检异常",5419]
[89,"Arm156","低气压开入告警",5420]
[89,"Arm157","通道检修差动退出",5421]
[89,"Arm158","电流不平衡告警",5422]
[89,"Arm159","开入配置错",5423]
[89,"Arm160","开入异常",5424]
[89,"Arm161","开出通讯中断",5425]
[89,"Arm162","传动状态未复归",5426]
[89,"Arm163","开入击穿",5427]
[89,"Arm164","开入输入不正常",5428]
[89,"Arm165","双位置输入不一致",5429]
[89,"Arm166","开入自检回路出错",5430]
[89,"Arm167","开入EEPROM出错",5431]
[89,"Arm168","PT断线",5432]
[89,"Arm169","静稳越限告警",5433]
[89,"Arm170","CT断线",5434]
[89,"Arm171","跳位A开入异常",5435]
[89,"Arm172","跳位B开入异常",5436]
[89,"Arm173","跳位C开入异常",5437]
[89,"Arm174","同期电压异常",5438]
[89,"Arm175","本侧CT断线",5439]
[89,"Arm176","对侧CT断线",5440]
[89,"Arm177","长期有差流",5441]
[89,"Arm178","同步方式设置出错",5442]
[89,"Arm179","通道一环回错",5443]
[89,"Arm180","通道二环回错",5444]
[89,"Arm181","光纤通道一故障",5445]
[89,"Arm182","光纤通道二故障",5446]
[89,"Arm183","通道一无采样报文",5447]
[89,"Arm184","通道二无采样报文",5448]
[89,"Arm185","三相相序不对应",5449]
[89,"Arm186","模拟通道异常",5450]
[89,"Arm187","其它保护开入异常",5451]
[89,"Arm188","外接3I0接反",5452]
[89,"Arm189","保护永跳失败",5453]
[89,"Arm190","3次谐波过量告警",5454]
[89,"Arm191","通道环回长期投入",5455]
[89,"Arm192","重合方式整定出错",5456]
[89,"Arm193","两侧差动投退不一致",5457]
[89,"Arm194","纵联保护地址错一",5458]
[89,"Arm195","纵联保护地址错二",5459]
[89,"Arm196","通道一二交叉接错",5460]
[89,"Arm197","对侧通信异常",5461]
[89,"Arm198","工作于调试定值区",5462]
[89,"Arm199","反时限长期启动",5463]
[89,"Arm200","远传1开入异常",5464]
[89,"Arm201","其它保护收信异常",5465]
[89,"Arm202","对侧保护退出",5466]
[89,"Arm203","通道故障",5467]
[89,"Arm204","网络状态1",5468]
[89,"Arm205","网络状态2",5469]
[89,"Arm206","装置通讯状态",5470]
[89,"Arm207","检修状态",5471]
[89,"Arm208","参数变化",5472]
[89,"Arm209","就地状态虚遥信",5473]
[89,"Arm210","遥控解除闭锁",5474]
[89,"Arm211","A网中断",5475]
[89,"Arm212","B网中断",5476]
[89,"Arm213","网络中断",5477]
[90,"Arm1","启动打印",5478]
[90,"Arm2","保护检修状态硬压板",5479]
[90,"Arm3","信号复归",5480]
[90,"Arm4","远方操作硬压板",5481]
[90,"Arm5","不停电传动使能",5482]
[90,"Arm6","A相不停电传动",5483]
[90,"Arm7","B相不停电传动",5484]
[90,"Arm8","C相不停电传动",5485]
[90,"Arm9","三相不停电传动",5486]
[90,"Arm10","开出传动使能",5487]
[90,"Arm11","A相跳闸出口",5488]
[90,"Arm12","B相跳闸出口",5489]
[90,"Arm13","C相跳闸出口",5490]
[90,"Arm14","重合闸出口",5491]
[90,"Arm15","保护跳闸出口",5492]
[90,"Arm16","保护三跳出口",5493]
[90,"Arm17","闭锁重合闸出口",5494]
[90,"Arm18","手动触发录波",5495]
[90,"Arm19","装置闭锁",5496]
[90,"Arm20","CID文件错误",5497]
[90,"Arm21","定值超范围",5498]
[90,"Arm22","板卡配置错误",5499]
[90,"Arm23","定值项变化告警",5500]
[90,"Arm24","插件8异常",5501]
[90,"Arm25","插件9异常",5502]
[90,"Arm26","插件11异常",5503]
[90,"Arm27","装置报警",5504]
[90,"Arm28","通信传动报警",5505]
[90,"Arm29","对时信号状态",5506]
[90,"Arm30","对时服务状态",5507]
[90,"Arm31","时间跳变侦测状态",5508]
[90,"Arm32","对时异常",5509]
[90,"Arm33","版本错误报警",5510]
[90,"Arm34","定值校验出错",5511]
[90,"Arm35","定值区不一致",5512]
[90,"Arm36","定值修改",5513]
[90,"Arm37","定值区切换",5514]
[90,"Arm38","内存不足",5515]
[90,"Arm39","IEC103配置文件无效",5516]
[90,"Arm40","插件8光耦电源异常",5517]
[90,"Arm41","插件9光耦电源异常",5518]
[90,"Arm42","电源异常",5519]
[90,"Arm43","装置高温告警",5520]
[90,"Arm44","装置低温告警",5521]
[90,"Arm45","装置电源监视告警",5522]
[90,"Arm46","纵联通道一接收光强越限告警",5523]
[90,"Arm47","纵联通道二接收光强越限告警",5524]
[90,"Arm48","运行",5525]
[90,"Arm49","异常",5526]
[90,"Arm50","检修",5527]
[90,"Arm51","纵联保护闭锁",5528]
[90,"Arm52","充电完成",5529]
[90,"Arm53","保护跳闸",5530]
[90,"Arm54","重合闸",5531]
[90,"Arm55","零序过流保护投入",5532]
[90,"Arm56","距离保护投入",5533]
[90,"Arm57","光纤通道一投入",5534]
[90,"Arm58","光纤通道二投入",5535]
[90,"Arm59","差动A相有效",5536]
[90,"Arm60","差动B相有效",5537]
[90,"Arm61","差动C相有效",5538]
[90,"Arm62","零序差动有效",5539]
[90,"Arm63","远方其它保护有效",5540]
[90,"Arm64","距离保护Ⅰ段有效",5541]
[90,"Arm65","距离保护Ⅱ段有效",5542]
[90,"Arm66","距离保护Ⅲ段有效",5543]
[90,"Arm67","零序过流Ⅱ段有效",5544]
[90,"Arm68","零序过流Ⅲ段有效",5545]
[90,"Arm69","零序反时限有效",5546]
[90,"Arm70","重合闸有效",5547]
[90,"Arm71","工频变化量距离有效",5548]
[90,"Arm72","闭锁主保护",5549]
[90,"Arm73","闭锁后备保护",5550]
[90,"Arm74","闭锁重合闸_(重复1)",5551]
[90,"Arm75","闭锁远方其它保护",5552]
[90,"Arm76","录波完成",5553]
[90,"Arm77","光纤通道一硬压板",5554]
[90,"Arm78","光纤通道二硬压板",5555]
[90,"Arm79","距离保护硬压板",5556]
[90,"Arm80","零序过流保护硬压板",5557]
[90,"Arm81","停用重合闸硬压板",5558]
[90,"Arm82","闭锁重合闸",5559]
[90,"Arm83","低气压闭锁重合闸",5560]
[90,"Arm84","分相跳闸位置TWJa",5561]
[90,"Arm85","分相跳闸位置TWJb",5562]
[90,"Arm86","分相跳闸位置TWJc",5563]
[90,"Arm87","其它保护动作",5564]
[90,"Arm88","远传1",5565]
[90,"Arm89","远传2",5566]
[90,"Arm90","闭锁重合闸_OPT",5567]
[90,"Arm91","低气压闭锁重合闸_OPT",5568]
[90,"Arm92","分相跳闸位置TWJa_OPT",5569]
[90,"Arm93","分相跳闸位置TWJb_OPT",5570]
[90,"Arm94","分相跳闸位置TWJc_OPT",5571]
[90,"Arm95","其它保护动作_OPT",5572]
[90,"Arm96","远传1_OPT",5573]
[90,"Arm97","远传2_OPT",5574]
[90,"Arm98","通道一收其它保护动作",5575]
[90,"Arm99","通道一收远传1",5576]
[90,"Arm100","通道一收远传2",5577]
[90,"Arm101","通道一对侧差动压板",5578]
[90,"Arm102","通道二收其它保护动作",5579]
[90,"Arm103","通道二收远传1",5580]
[90,"Arm104","通道二收远传2",5581]
[90,"Arm105","通道二对侧差动压板",5582]
[90,"Arm106","收其它保护动作",5583]
[90,"Arm107","收远传1",5584]
[90,"Arm108","收远传2",5585]
[90,"Arm109","重合闸充电完成",5586]
[90,"Arm110","远传1出口",5587]
[90,"Arm111","远传2出口",5588]
[90,"Arm112","通道告警出口",5589]
[90,"Arm113","A相跳闸出口_(重复1)",5590]
[90,"Arm114","B相跳闸出口_(重复1)",5591]
[90,"Arm115","C相跳闸出口_(重复1)",5592]
[90,"Arm116","重合闸出口_(重复1)",5593]
[90,"Arm117","保护跳闸出口_(重复1)",5594]
[90,"Arm118","保护三跳出口_(重复1)",5595]
[90,"Arm119","闭锁重合闸出口_(重复1)",5596]
[90,"Arm120","装置异常启动录波",5597]
[90,"Arm121","保护启动",5598]
[90,"Arm122","A相跳闸动作",5599]
[90,"Arm123","B相跳闸动作",5600]
[90,"Arm124","C相跳闸动作",5601]
[90,"Arm125","保护动作",5602]
[90,"Arm126","重合闸动作",5603]
[90,"Arm127","纵联差动保护动作",5604]
[90,"Arm128","工频变化量阻抗动作",5605]
[90,"Arm129","接地距离Ⅰ段动作",5606]
[90,"Arm130","相间距离Ⅰ段动作",5607]
[90,"Arm131","接地距离Ⅱ段动作",5608]
[90,"Arm132","相间距离Ⅱ段动作",5609]
[90,"Arm133","接地距离Ⅲ段动作",5610]
[90,"Arm134","相间距离Ⅲ段动作",5611]
[90,"Arm135","距离加速动作",5612]
[90,"Arm136","零序加速动作",5613]
[90,"Arm137","零序过流Ⅱ段动作",5614]
[90,"Arm138","零序过流Ⅲ段动作",5615]
[90,"Arm139","零序反时限动作",5616]
[90,"Arm140","选相无效三跳",5617]
[90,"Arm141","远方其它保护动作",5618]
[90,"Arm142","加速联跳动作",5619]
[90,"Arm143","单跳失败三跳",5620]
[90,"Arm144","单相运行三跳",5621]
[90,"Arm145","不停电传动跳闸",5622]
[90,"Arm146","保护CPU插件异常",5623]
[90,"Arm147","开出异常",5624]
[90,"Arm148","模拟量采集错",5625]
[90,"Arm149","启动DSP定值出错",5626]
[90,"Arm150","启动DSP内存出错",5627]
[90,"Arm151","启动DSP采样出错",5628]
[90,"Arm152","启动DSP校验出错",5629]
[90,"Arm153","启动DSP装置类型配置错",5630]
[90,"Arm154","跳合出口回路异常",5631]
[90,"Arm155","保护DSP装置类型配置错",5632]
[90,"Arm156","保护DSP校验出错",5633]
[90,"Arm157","保护DSP定值出错",5634]
[90,"Arm158","保护DSP内存出错",5635]
[90,"Arm159","保护DSP采样出错",5636]
[90,"Arm160","开入异常",5637]
[90,"Arm161","其它保护开入异常",5638]
[90,"Arm162","保护同期电压采样出错",5639]
[90,"Arm163","跳闸位置开入异常",5640]
[90,"Arm164","通道一无有效帧",5641]
[90,"Arm165","通道一识别码错",5642]
[90,"Arm166","通道一严重误码",5643]
[90,"Arm167","通道一连接错误",5644]
[90,"Arm168","通道二无有效帧",5645]
[90,"Arm169","通道二识别码错",5646]
[90,"Arm170","通道二严重误码",5647]
[90,"Arm171","通道二连接错误",5648]
[90,"Arm172","通道一通道异常",5649]
[90,"Arm173","通道一差动退出",5650]
[90,"Arm174","通道一差动自环异常",5651]
[90,"Arm175","通道一两侧差动投退不一致",5652]
[90,"Arm176","通道一同步异常",5653]
[90,"Arm177","通道一对侧异常闭锁差动",5654]
[90,"Arm178","通道一对侧CT断线",5655]
[90,"Arm179","通道二通道异常",5656]
[90,"Arm180","通道二差动退出",5657]
[90,"Arm181","通道二差动自环异常",5658]
[90,"Arm182","通道二两侧差动投退不一致",5659]
[90,"Arm183","通道二同步异常",5660]
[90,"Arm184","通道二对侧异常闭锁差动",5661]
[90,"Arm185","通道二对侧CT断线",5662]
[90,"Arm186","通道故障",5663]
[90,"Arm187","对侧CT断线",5664]
[90,"Arm188","其它保护收信异常",5665]
[90,"Arm189","长期启动报警",5666]
[90,"Arm190","零序长期启动",5667]
[90,"Arm191","CT断线",5668]
[90,"Arm192","PT断线",5669]
[90,"Arm193","同期电压异常",5670]
[90,"Arm194","保护PT中性线断线",5671]
[90,"Arm195","零序反时限告警",5672]
[90,"Arm196","通道一长期有差流",5673]
[90,"Arm197","通道一补偿参数错",5674]
[90,"Arm198","通道一CT变比失配",5675]
[90,"Arm199","通道二长期有差流",5676]
[90,"Arm200","通道二补偿参数错",5677]
[90,"Arm201","通道二CT变比失配",5678]
[90,"Arm202","重合方式整定出错",5679]
[90,"Arm203","光纤通道一软压板",5680]
[90,"Arm204","光纤通道二软压板",5681]
[90,"Arm205","距离保护软压板",5682]
[90,"Arm206","零序过流保护软压板",5683]
[90,"Arm207","停用重合闸软压板",5684]
[90,"Arm208","远方投退压板软压板",5685]
[90,"Arm209","远方切换定值区软压板",5686]
[90,"Arm210","远方修改定值软压板",5687]
[90,"Arm211","网络状态1",5688]
[90,"Arm212","网络状态2",5689]
[90,"Arm213","装置通讯状态",5690]
[90,"Arm214","检修状态",5691]
[90,"Arm215","参数变化",5692]
[90,"Arm216","就地状态虚遥信",5693]
[90,"Arm217","遥控解除闭锁",5694]
[90,"Arm218","A网中断",5695]
[90,"Arm219","B网中断",5696]
[90,"Arm220","网络中断",5697]
[5,"PosOff","存308断路器分位",5698]
[5,"RkdOut","存308手车试验位置",5699]
[8,"PosOff","存408断路器分位",5700]
[8,"RkdOut","存408手车试验位置",5701]
[11,"PosOff","存508断路器分位",5702]
[11,"RkdOut","存508手车试验位置",5703]
[14,"PosOff","存608断路器分位",5704]
[14,"RkdOut","存608手车试验位置",5705]
[55,"PosOff","存309断路器分位",5706]
[55,"RkdOut","存309手车试验位置",5707]
[55,"ESPosOff","存3099地刀分位",5708]
[58,"PosOff","存419断路器分位",5709]
[58,"RkdOut","存419手车试验位置",5710]
[58,"ESPosOff","存4199地刀分位",5711]
[60,"PosOff","存509断路器分位",5712]
[60,"RkdOut","存509手车试验位置",5713]
[60,"ESPosOff","存509地刀分位",5714]
[62,"PosOff","存609断路器分位",5715]
[62,"RkdOut","存609手车试验位置",5716]
[62,"ESPosOff","存609地刀分位",5717]
[56,"PosOff","存310断路器分位",5718]
[56,"RkdOut","存310手车试验位置",5719]
[56,"ESPosOff","存3109地刀分位",5720]
[59,"PosOff","存410断路器分位",5721]
[59,"RkdOut","存410手车试验位置",5722]
[59,"ESPosOff","存4109地刀分位",5723]
[61,"PosOff","存510断路器分位",5724]
[61,"RkdOut","存510手车试验位置",5725]
[61,"ESPosOff","存5109地刀分位",5726]
[63,"PosOff","存610断路器分位",5727]
[63,"RkdOut","存610手车试验位置",5728]
[63,"ESPosOff","存6109地刀分位",5729]
[57,"PosOff","存311断路器分位",5730]
[57,"RkdOut","存311手车试验位置",5731]
[57,"ESPosOff","存3119地刀分位",5732]
[64,"PosOff","存611断路器分位",5733]
[64,"RkdOut","存611手车试验位置",5734]
[64,"ESPosOff","存6119地刀分位",5735]
[92,"PosOff","存902断路器分位",5736]
[92,"RkdOut","存902手车试验位置",5737]
[92,"ESPosOff","存9029地刀分位",5738]
[91,"RkdOut","存901站用进线手车试验位置",5739]
[91,"ESPosOff","存901站用进线地刀分位",5740]
[65,"PosOff","存314断路器分位",5741]
[65,"RkdOut","存314手车试验位置",5742]
[66,"PosOff","存415断路器分位",5743]
[66,"RkdOut","存415手车试验位置",5744]
[67,"PosOff","存516断路器分位",5745]
[67,"RkdOut","存516手车试验位置",5746]
[68,"PosOff","存613断路器分位",5747]
[68,"RkdOut","存613手车试验位置",5748]
[19,"RkdOut","互03b手车试验位置",5749]
[19,"sRkdOut","存3141隔离手车试验位置",5750]
[20,"RkdOut","互04b手车试验位置",5751]
[20,"sRkdOut","存4151隔离手车试验位置",5752]
[21,"RkdOut","互05b手车试验位置",5753]
[21,"sRkdOut","存5161隔离手车试验位置",5754]
[22,"RkdOut","互06b手车试验位置",5755]
[22,"sRkdOut","存6131隔离手车试验位置",5756]
[23,"PosOff","存301断路器分位",5757]
[23,"RkdOut","存301手车试验位置",5758]
[23,"ESPosOff","存3019地刀分位",5759]
[24,"PosOff","存302断路器分位",5760]
[24,"RkdOut","存302手车试验位置",5761]
[24,"ESPosOff","存3029地刀分位",5762]
[25,"PosOff","存303断路器分位",5763]
[25,"RkdOut","存303手车试验位置",5764]
[25,"ESPosOff","存3039地刀分位",5765]
[26,"PosOff","存304断路器分位",5766]
[26,"RkdOut","存304手车试验位置",5767]
[26,"ESPosOff","存3049地刀分位",5768]
[27,"PosOff","存305断路器分位",5769]
[27,"RkdOut","存305手车试验位置",5770]
[27,"ESPosOff","存3059地刀分位",5771]
[28,"PosOff","存306断路器分位",5772]
[28,"RkdOut","存306手车试验位置",5773]
[28,"ESPosOff","存3069地刀分位",5774]
[29,"PosOff","存307断路器分位",5775]
[29,"RkdOut","存307手车试验位置",5776]
[29,"ESPosOff","存3079地刀分位",5777]
[31,"PosOff","存401断路器分位",5778]
[31,"RkdOut","存401手车试验位置",5779]
[31,"ESPosOff","存4019地刀分位",5780]
[32,"PosOff","存402断路器分位",5781]
[32,"RkdOut","存402手车试验位置",5782]
[32,"ESPosOff","存4029地刀分位",5783]
[33,"PosOff","存403断路器分位",5784]
[33,"RkdOut","存403手车试验位置",5785]
[33,"ESPosOff","存4039地刀分位",5786]
[34,"PosOff","存404断路器分位",5787]
[34,"RkdOut","存404手车试验位置",5788]
[34,"ESPosOff","存4049地刀分位",5789]
[35,"PosOff","存405断路器分位",5790]
[35,"RkdOut","存405手车试验位置",5791]
[35,"ESPosOff","存4059地刀分位",5792]
[36,"PosOff","存406断路器分位",5793]
[36,"RkdOut","存406手车试验位置",5794]
[36,"ESPosOff","存4069地刀分位",5795]
[37,"PosOff","存407断路器分位",5796]
[37,"RkdOut","存407手车试验位置",5797]
[37,"ESPosOff","存4079地刀分位",5798]
[39,"PosOff","存501断路器分位",5799]
[39,"RkdOut","存501手车试验位置",5800]
[39,"ESPosOff","存5019地刀分位",5801]
[40,"PosOff","存502断路器分位",5802]
[40,"RkdOut","存502手车试验位置",5803]
[40,"ESPosOff","存5029地刀分位",5804]
[41,"PosOff","存503断路器分位",5805]
[41,"RkdOut","存503手车试验位置",5806]
[41,"ESPosOff","存5039地刀分位",5807]
[42,"PosOff","存504断路器分位",5808]
[42,"RkdOut","存504手车试验位置",5809]
[42,"ESPosOff","存504地刀分位",5810]
[43,"PosOff","存505断路器分位",5811]
[43,"RkdOut","存505手车试验位置",5812]
[43,"ESPosOff","存505地刀分位",5813]
[44,"PosOff","存506断路器分位",5814]
[44,"RkdOut","存506手车试验位置",5815]
[44,"ESPosOff","存506地刀分位",5816]
[45,"PosOff","存507断路器分位",5817]
[45,"RkdOut","存507手车试验位置",5818]
[45,"ESPosOff","存507地刀分位",5819]
[47,"PosOff","存601断路器分位",5820]
[47,"RkdOut","存601手车试验位置",5821]
[47,"ESPosOff","存601地刀分位",5822]
[48,"PosOff","存602断路器分位",5823]
[48,"RkdOut","存602手车试验位置",5824]
[48,"ESPosOff","存602地刀分位",5825]
[49,"PosOff","存603断路器分位",5826]
[49,"RkdOut","存603手车试验位置",5827]
[49,"ESPosOff","存603地刀分位",5828]
[50,"PosOff","存604断路器分位",5829]
[50,"RkdOut","存604手车试验位置",5830]
[50,"ESPosOff","存604地刀分位",5831]
[51,"PosOff","存605断路器分位",5832]
[51,"RkdOut","存605手车试验位置",5833]
[51,"ESPosOff","存605地刀分位",5834]
[52,"PosOff","存606断路器分位",5835]
[52,"RkdOut","存606手车试验位置",5836]
[52,"ESPosOff","存606地刀分位",5837]
[53,"PosOff","存607断路器分位",5838]
[53,"RkdOut","存607手车试验位置",5839]
[53,"ESPosOff","存607地刀分位",5840]

{"sheet":"数字量控制","index":4,"n_rows":2,"n_cols":4,"rows_kept":2}
["DEV_ID","TAG_NAME","DESCRIPTION","REMOTE_NO"]
["设备ID","标签名","点描述","远动号"]

{"sheet":"保护定值","index":5,"n_rows":2,"n_cols":8,"rows_kept":2}
["DEV_ID","GROUP_NO","SEQ_NO","DZ_SEQ","DESCRIPTION","RATIO","REVISE","VALUE_TEXT"]
["设备ID"," 定值组号","定值代号"," 定值序号","点描述","装置系数","修正值","数值描述文件"]